(footprint "XKB_X05C2040TZ_40S_P0.5_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.15 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp fdea8de6-5e6a-4aff-ae00-44d3e5f7cba1)
  )
  (fp_text value "XKB_X05C2040TZ_40S_P0.5_Vertical" (at 0 1.8 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp a914dff8-3af7-472d-aed9-9bcbf87be065)
  )
  (fp_text user "${REFERENCE}" (at 9.375 0.025 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 8178711a-83ed-410c-8e4a-25efd16e1ac9)
  )
  (fp_arc (start -12.775 -1.35) (mid -12.753033 -1.403033) (end -12.7 -1.425)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp a06a2ee8-6574-433e-b5e0-88496655ccdb))
  (fp_arc (start -12.7 1.425) (mid -12.753033 1.403033) (end -12.775 1.35)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 77ae75b3-ccee-4ac9-8481-a113e1d4d5c8))
  (fp_arc (start 12.7 -1.425) (mid 12.753033 -1.403033) (end 12.775 -1.35)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 85439d7f-62d5-4115-9f3a-a0974b8cbc23))
  (fp_arc (start 12.775 1.35) (mid 12.753033 1.403033) (end 12.7 1.425)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 0e7391b0-8068-423a-93b5-0d0fd8aa56ff))
  (fp_poly
    (pts
      (xy -9.575 2)
      (xy -9.925 2)
      (xy -9.75 1.65)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2b35a38d-9181-44d0-8ff1-94454e3f60a9))
  (fp_poly
    (pts
      (xy -11.7 -1.35)
      (xy -12.7 -1.35)
      (xy -12.7 1.35)
      (xy -11.7 1.35)
      (xy -11.7 1.5)
      (xy -12.7 1.5)
      (xy -12.85 1.35)
      (xy -12.85 -1.35)
      (xy -12.7 -1.5)
      (xy -11.7 -1.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp acc1f89d-13f8-46d4-9a87-8fb7df8cc987))
  (fp_poly
    (pts
      (xy 11.7 1.35)
      (xy 12.7 1.35)
      (xy 12.7 -1.35)
      (xy 11.7 -1.35)
      (xy 11.7 -1.5)
      (xy 12.7 -1.5)
      (xy 12.85 -1.35)
      (xy 12.85 1.35)
      (xy 12.7 1.5)
      (xy 11.7 1.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9e2238f5-6ed0-43e0-9efd-8ff4a78d4247))
  (fp_line (start -13.15 1.1) (end -13.15 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 09667bd8-1efd-43a8-8684-806a4f7b8e26))
  (fp_line (start -12.45 -1.8) (end 12.45 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e51d02c4-a4e6-4442-bad1-20c869dec8cf))
  (fp_line (start 12.45 1.8) (end -12.45 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7312c5c2-6098-488d-8a16-97173a18cf1a))
  (fp_line (start 13.15 -1.1) (end 13.15 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 75d89da0-58dd-4d37-ade3-585490429268))
  (fp_arc (start -13.15 -1.1) (mid -12.944975 -1.594975) (end -12.45 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 777d8970-7838-4843-83c1-58c3005b3231))
  (fp_arc (start -12.45 1.8) (mid -12.944975 1.594975) (end -13.15 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3242b275-17f4-456d-aacf-5611c80cf328))
  (fp_arc (start 12.45 -1.8) (mid 12.944975 -1.594975) (end 13.15 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9321415c-e5dd-4496-b267-3821ba23791b))
  (fp_arc (start 13.15 1.1) (mid 12.944975 1.594975) (end 12.45 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 449b18a4-477c-4d8a-a410-ecbc033e123b))
  (fp_line (start -12.8 -1) (end -12 -1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2960ce21-84f5-4df1-82da-785de48ec0fb))
  (fp_line (start -12.8 1) (end -12.8 -1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e94b81b7-9e98-4a56-989b-6ecb37b7c6d7))
  (fp_line (start -12 1) (end -12.8 1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 4ca1f169-0c4f-43c0-a727-3d78ac6b0505))
  (fp_line (start 12 -1) (end 12.8 -1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2ade3bb3-f0d3-4e8f-abe1-65e46e2de153))
  (fp_line (start 12.8 -1) (end 12.8 1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 458fc4ca-2d2e-430f-8c63-089207d4b3a8))
  (fp_line (start 12.8 1) (end 12 1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 16130a96-2de2-4465-af0c-f445bba4d643))
  (fp_rect (start -11.75 -1) (end 11.75 1)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 19ef6e31-d98b-4f89-92ea-f64d1a27b66b))
  (pad "1" smd roundrect (at -9.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 528bc1dc-3783-472e-8551-f3ae144fa3df))
  (pad "2" smd roundrect (at -9.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 12a5d048-a826-4a6d-b7e4-716d73e116c5))
  (pad "3" smd roundrect (at -8.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 46910f7d-a141-45d9-8bf8-d58ee1862f0d))
  (pad "4" smd roundrect (at -8.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 80a0e5ad-6785-4dd2-98eb-0eecd5f38d4a))
  (pad "5" smd roundrect (at -7.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1f0edc3f-d288-450e-a6c9-b76c124a8820))
  (pad "6" smd roundrect (at -7.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 91c83b2a-abb4-49b7-a5c8-f3812d9d088f))
  (pad "7" smd roundrect (at -6.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 76e30d60-2fe2-4956-9304-339358eb8abd))
  (pad "8" smd roundrect (at -6.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a1f6995d-a2e0-4768-9aac-9707aeb5b8da))
  (pad "9" smd roundrect (at -5.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp fd4346c2-9fc6-4ece-af2f-ab4309bc818b))
  (pad "10" smd roundrect (at -5.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 61e0cd6a-6f03-42ab-bb74-97187818e56a))
  (pad "11" smd roundrect (at -4.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1c340d4c-1888-4fb3-9f98-ad89039d0850))
  (pad "12" smd roundrect (at -4.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 315a8158-3581-4bf2-a354-cd65c1251b1d))
  (pad "13" smd roundrect (at -3.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2bc4da90-351a-42e7-8c09-b552f19d98ee))
  (pad "14" smd roundrect (at -3.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 334d55c8-8065-494d-812d-688b37c2330e))
  (pad "15" smd roundrect (at -2.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f22750e4-4b07-4d8a-9f75-741fdecb85ea))
  (pad "16" smd roundrect (at -2.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp aae741bd-a0b0-4603-a8aa-f849705d6282))
  (pad "17" smd roundrect (at -1.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 66cbaba1-e965-405a-9cc5-10fab47003a4))
  (pad "18" smd roundrect (at -1.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 02013653-18cf-481b-904c-b9b03c73576d))
  (pad "19" smd roundrect (at -0.75 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2606ff1a-25ff-4103-aa9e-ad6be0b3a3d5))
  (pad "20" smd roundrect (at -0.25 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a0484981-2c3b-44fd-8532-19366e0456b5))
  (pad "21" smd roundrect (at 0.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp eba0e8ba-c974-42ef-b90a-d70b36facfc9))
  (pad "22" smd roundrect (at 0.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d80b3ba3-bfb0-4382-88a8-1bbc3e747728))
  (pad "23" smd roundrect (at 1.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 96e04a8e-66bd-4c38-9566-ca2d159f9bc4))
  (pad "24" smd roundrect (at 1.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp bfab89ad-e923-438d-ace5-d841e34f831d))
  (pad "25" smd roundrect (at 2.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a3d8dde7-7970-4392-bf8b-92fd953e546e))
  (pad "26" smd roundrect (at 2.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c3cf1146-c164-49ce-bc27-10f9761a89bf))
  (pad "27" smd roundrect (at 3.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp cd80e5ab-135c-4f8e-b3fd-a7e62ba9a321))
  (pad "28" smd roundrect (at 3.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5dfc95a1-5fc5-4ba3-8c84-18367e4350c6))
  (pad "29" smd roundrect (at 4.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 3dc51d9f-5fe8-432b-b0dc-39b9eb64d17e))
  (pad "30" smd roundrect (at 4.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7ee14538-319e-4e0f-80dd-8cb5d6271bd4))
  (pad "31" smd roundrect (at 5.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d16785c6-9302-40bc-861f-3fd8fd6b4668))
  (pad "32" smd roundrect (at 5.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp fd8dbf80-7404-4506-b769-3b9f3b1f63d0))
  (pad "33" smd roundrect (at 6.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 110ce6a8-4643-4b6d-b1c7-f4bfe31ea78f))
  (pad "34" smd roundrect (at 6.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 3de11a62-d069-4db9-8577-5c18f4a93589))
  (pad "35" smd roundrect (at 7.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 66a9fbc7-68e9-4a27-9f9f-fd3b6db14bb2))
  (pad "36" smd roundrect (at 7.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 84803591-ea3f-4f26-92bf-db7ae7200e52))
  (pad "37" smd roundrect (at 8.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 51503a23-d45d-4b82-8190-c14c948cdd90))
  (pad "38" smd roundrect (at 8.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1862649c-7e8a-4e3f-8f7c-69898dc0dd6d))
  (pad "39" smd roundrect (at 9.25 0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a7c47ede-a044-4d8e-a6a1-1ba146dd2b76))
  (pad "40" smd roundrect (at 9.75 -0.975) (size 0.4 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp be65d88d-2629-4e20-980d-5d34a37eaa8b))
  (pad "MP" smd roundrect (at -11.55 0) (size 2 2.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 5aeec327-8b6a-4a33-901e-3a87a55b1e40))
  (pad "MP" smd roundrect (at 11.55 0) (size 2 2.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 43e142f2-72e1-4622-95bc-c99dddd7fbad))
  (model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/X05C2040XZ.stp"
    (offset (xyz 0 0 4.4))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
