(footprint "FPC_Pads_22P_P0.5_Bottom" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "CameraCable.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "J1" (at -5.5 2.6 180 unlocked) (layer "B.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left mirror))
    (tstamp 54dd35b7-7f72-4910-830f-79c26d68bd11)
  )
  (fp_text value "Camera_FPC_Connector_(22-pin_RPi,_module_side)" (at 0 -0.25 unlocked) (layer "B.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp b7050a83-4a5e-440b-b3d3-d19517e4e6ea)
  )
  (fp_text user "STIFFENER BOARD" (at 0 2.75 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp 066780a9-f1a0-4898-9874-5bc8bdd271c2)
  )
  (fp_text user "${REF}" (at 0 -1.5 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2e674135-20cb-4458-b54b-c12e5addfac9)
  )
  (fp_poly
    (pts
      (xy 5.5 2.75)
      (xy 5 2.75)
      (xy 5.25 2.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "B.SilkS") (tstamp b3577a64-ec33-4c66-9589-6a28a028c012))
  (fp_rect (start -5.75 0) (end 5.75 3.25)
    (stroke (width 0.05) (type solid)) (fill none) (layer "Dwgs.User") (tstamp 652d9502-83ee-4995-8c24-1dc16d8ccdd8))
  (pad "1" connect roundrect (at 5.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp f951abb9-5b27-4645-9eb3-51ce7b3d8664))
  (pad "2" connect roundrect (at 4.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 6bb6cb3c-3b94-4f3e-a4c5-d392b3020ab7))
  (pad "3" connect roundrect (at 4.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 2939c4b5-6382-4ef3-b995-6ae5dad507ec))
  (pad "4" connect roundrect (at 3.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp ec2e182c-46ea-46b8-905d-9f2e4cfe7625))
  (pad "5" connect roundrect (at 3.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp ab22f7c0-7112-4da3-8c5c-3bf9e20936b2))
  (pad "6" connect roundrect (at 2.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 0309be5a-7394-4ce5-8ba6-a08d2dc618f3))
  (pad "7" connect roundrect (at 2.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 051325f8-4df9-4823-bca1-efc7664f30cb))
  (pad "8" connect roundrect (at 1.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 134b9005-dcf8-479a-89b3-5ffbac309807))
  (pad "9" connect roundrect (at 1.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp c5dc546b-2f7a-4e5c-9083-5cabbadfc461))
  (pad "10" connect roundrect (at 0.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 2a3295f4-6625-4141-b54d-6a52f476977b))
  (pad "11" connect roundrect (at 0.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 07150c8f-da62-4e24-ba86-6323f8886a9a))
  (pad "12" connect roundrect (at -0.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp a42a3011-1ea0-405f-8588-b7b825594526))
  (pad "13" connect roundrect (at -0.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 439759a0-a57f-4479-9cdf-2b6832afda19))
  (pad "14" connect roundrect (at -1.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 23e2f9ef-3dec-4dcb-9e21-a9c12bb20e2f))
  (pad "15" connect roundrect (at -1.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 78cf0905-913a-4f05-88c1-b892b072e584))
  (pad "16" connect roundrect (at -2.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp a1b99729-3564-4f37-a0fd-a7534416fd43))
  (pad "17" connect roundrect (at -2.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 73f1d339-657d-4749-ae58-793fd837efb5))
  (pad "18" connect roundrect (at -3.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 50c6e32e-93f0-4f69-9eaa-ce251d98c141))
  (pad "19" connect roundrect (at -3.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 446eb335-818e-487a-b760-78da3ee80e57))
  (pad "20" connect roundrect (at -4.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 5996cc78-63a3-48ae-95ef-f51271202fba))
  (pad "21" connect roundrect (at -4.75 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 7de99d87-6946-4f05-bd2e-0a8fc7ad3aa6))
  (pad "22" connect roundrect (at -5.25 1) (size 0.3 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 99fcf4e9-cc03-401a-97e6-67b62cdd15bb))
)
