(footprint "D_SMC_KA" (version 20220621) (generator pcbnew)
  (layer "F.Cu")
  (descr "Diode SMC (DO-214AB)")
  (tags "Diode SMC (DO-214AB)")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "C310158")
  (property "MFG" "Brightking")
  (property "MPN" "SMDJ78CA/TR7")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (attr smd)
  (fp_text reference "D10" (at 0 -4.1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ae4d6541-8968-422a-8e43-0ce614cd4af1)
  )
  (fp_text value "78V 23.8A" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3724d8f1-d9ae-41bc-9a03-7d26c7411dd3)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.9) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 818297bc-603d-4692-bb41-555e98bf9f30)
  )
  (fp_poly
    (pts
      (xy 3.55 -3.1)
      (xy -3.7 -3.1)
      (xy -3.7 -1.8)
      (xy -4.8 -1.8)
      (xy -4.8 1.8)
      (xy -3.7 1.8)
      (xy -3.7 3.1)
      (xy 3.55 3.1)
      (xy 3.55 3.25)
      (xy -3.85 3.25)
      (xy -3.85 1.95)
      (xy -4.95 1.95)
      (xy -4.95 -1.95)
      (xy -3.85 -1.95)
      (xy -3.85 -3.25)
      (xy 3.55 -3.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp cfe4da63-feed-4152-93a6-add95eb60bf2))
  (fp_line (start -4.8 1.4) (end -4.8 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ce103f29-2d82-49ad-9f77-8b4fdc57be4a))
  (fp_line (start -4.4 -1.8) (end -3.8 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5cca95e2-1c6a-4585-be63-a30113fcb9ce))
  (fp_line (start -3.8 -1.8) (end -3.8 -3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 922b3d65-98c9-45bc-8d51-ac676cdf98c1))
  (fp_line (start -3.8 1.8) (end -4.4 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d14c6120-4d21-42ac-9a2d-1ced2e0ad9fe))
  (fp_line (start -3.8 3.1) (end -3.8 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b08a851a-a59f-4583-98a9-3ff2b6b0d61b))
  (fp_line (start -3.55 -3.35) (end 3.55 -3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 42dc5291-6073-45c4-810f-a3e7c8c26b18))
  (fp_line (start 3.55 3.35) (end -3.55 3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7155e167-8141-41b3-8077-1c75b8d47dc7))
  (fp_line (start 3.8 -3.1) (end 3.8 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9260c389-bab5-40c9-9faf-c54c4caf18c3))
  (fp_line (start 3.8 -1.8) (end 4.4 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3aecb10d-a9c9-4d7c-92e0-0082e710f3ea))
  (fp_line (start 3.8 1.8) (end 3.8 3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0a3bde83-4d30-4b7d-bfb7-7495066f0e1d))
  (fp_line (start 4.4 1.8) (end 3.8 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7c9f691e-ef04-49da-bbb7-51ac8322752e))
  (fp_line (start 4.8 -1.4) (end 4.8 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5607adfd-300b-40c4-992b-7d7df0138b0a))
  (fp_arc (start -4.8 -1.4) (mid -4.682843 -1.682843) (end -4.4 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8da292c7-16ac-434a-8230-b3bb4854bca7))
  (fp_arc (start -4.4 1.8) (mid -4.682843 1.682843) (end -4.8 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 03f2060a-502f-45c7-984e-4929f168c97e))
  (fp_arc (start -3.8 -3.1) (mid -3.726777 -3.276777) (end -3.55 -3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fccde08c-2cb5-4fca-b8ff-90b12aa937d7))
  (fp_arc (start -3.55 3.35) (mid -3.726777 3.276777) (end -3.8 3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1bbd04f0-0d7d-42b2-93af-313689cea828))
  (fp_arc (start 3.55 -3.35) (mid 3.726777 -3.276777) (end 3.8 -3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb6b618f-ccfe-4a74-a996-dba8f57b6f64))
  (fp_arc (start 3.8 3.1) (mid 3.726777 3.276777) (end 3.55 3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b639310-7178-464d-968b-fa72638a4dd7))
  (fp_arc (start 4.4 -1.8) (mid 4.682843 -1.682843) (end 4.8 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7cfd3474-29b8-4d92-aef1-edf25d947c50))
  (fp_arc (start 4.8 1.4) (mid 4.682843 1.682843) (end 4.4 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e57ce6e0-2d33-419a-82e7-9b922447ac74))
  (fp_line (start -3.55 3.1) (end -3.55 -3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eccb5b3a-4ebe-4858-8d5d-84532a2d8725))
  (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 309a400c-8e41-4254-bc04-4ea409ca4262))
  (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7dc2e373-31a3-4f29-9be9-5cde26ae0c95))
  (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0846a9dc-26a1-46e0-9851-8361650065bd))
  (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 796d9be9-41cd-42b4-9f83-e8b59539796d))
  (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8dedf0eb-f307-49bc-89ed-a1f1e326448e))
  (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e7859afb-df3b-45b7-9c47-87e998cb2854))
  (fp_line (start 3.55 -3.1) (end -3.55 -3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b0890f9-044d-4b8a-ba9f-960ab096f4ec))
  (fp_line (start 3.55 -3.1) (end 3.55 3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c15f05db-f468-4eba-9b8a-2dc61297314e))
  (fp_line (start 3.55 3.1) (end -3.55 3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bebbbf91-d50c-45c8-9403-a81d8126d4bb))
  (pad "A" smd roundrect (at 3.4 0 90) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 2f805c42-3494-4af3-93c8-93df4dd6d0ea))
  (pad "K" smd roundrect (at -3.4 0 90) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 28a79c6c-281e-4457-ae6f-283fec45141f))
  (model "${KICAD7_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
