(module ST_powerSTEP01 (layer F.Cu) (tedit 5C46F9C1)
  (solder_mask_margin 0.002)
  (solder_paste_margin -0.025)
  (attr smd)
  (fp_text reference U1 (at -5.6 -8) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value ST_powerSTEP01 (at 0 1.25) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_circle (center -6.25 -7.4) (end -6.15 -7.4) (layer F.SilkS) (width 0.125))
  (fp_line (start -5.9 7.4) (end -5.9 7.4) (layer F.SilkS) (width 0.01))
  (fp_line (start -6 7.5) (end -6 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -6 7.5) (end -5 7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 7.5) (end 5 7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 7.5) (end 6 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 -7.5) (end 6 -6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 -7.5) (end 5 -7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -6 -7.5) (end -5 -7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -6 -7.5) (end -6 -6.5) (layer F.SilkS) (width 0.125))
  (fp_circle (center -4.5 -6) (end -5 -6) (layer F.Fab) (width 0.05))
  (fp_line (start -5.5 -7) (end -5.5 -7) (layer F.Fab) (width 0.05))
  (fp_line (start -5.5 7) (end -5.5 -7) (layer F.Fab) (width 0.05))
  (fp_line (start 5.5 7) (end -5.5 7) (layer F.Fab) (width 0.05))
  (fp_line (start 5.5 -7) (end 5.5 7) (layer F.Fab) (width 0.05))
  (fp_line (start -5.5 -7) (end 5.5 -7) (layer F.Fab) (width 0.05))
  (pad E3 thru_hole circle (at -1.4 3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -2.2 3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -1.4 3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -2.2 3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -1.4 4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -2.2 4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -1.4 5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E3 thru_hole circle (at -2.2 5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 1.4 3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 2.2 3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 1.4 3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 2.2 3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 1.4 4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 2.2 4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 1.4 5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E4 thru_hole circle (at 2.2 5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 1.4 -3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 2.2 -3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 1.4 -3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 2.2 -3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 1.4 -4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 2.2 -4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 1.4 -5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E7 thru_hole circle (at 2.2 -5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -1.4 -3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -2.2 -3.08) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -1.4 -3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -2.2 -3.87) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -1.4 -4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -2.2 -4.66) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -1.4 -5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E8 thru_hole circle (at -2.2 -5.45) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 -0.4) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 -1.2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 2.45 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 1.65 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.85 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at 0.05 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -0.75 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -1.55 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E9 thru_hole circle (at -2.35 -2) (size 0.6302 0.6302) (drill 0.3302) (layers *.Cu))
  (pad E1 smd roundrect (at -4.3 -5.615) (size 1.44 3.57) (layers F.Cu F.Mask) (roundrect_rratio 0.06900000000000001))
  (pad E6 smd roundrect (at 4.3 -5.615) (size 1.44 3.57) (layers F.Cu F.Mask) (roundrect_rratio 0.06900000000000001))
  (pad E5 smd roundrect (at 4.3 5.615) (size 1.44 3.57) (layers F.Cu F.Mask) (roundrect_rratio 0.06900000000000001))
  (pad E1 smd roundrect (at -4.455 -5.315) (size 2.89 2.17) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E6 smd roundrect (at 4.455 -5.315) (size 2.89 2.17) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E5 smd roundrect (at 4.455 5.315) (size 2.89 2.17) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E2 smd roundrect (at -4.3 5.615) (size 1.44 3.57) (layers F.Cu F.Mask) (roundrect_rratio 0.06900000000000001))
  (pad E2 smd roundrect (at -4.455 5.315) (size 2.89 2.17) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E1 smd roundrect (at -4.08 -5.255) (size 2.17 2.88) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E6 smd roundrect (at 4.08 -5.255) (size 2.17 2.88) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E5 smd roundrect (at 4.08 5.255) (size 2.17 2.88) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E2 smd roundrect (at -4.08 5.255) (size 2.14 2.85) (layers F.Cu F.Mask) (roundrect_rratio 0.046))
  (pad E11 smd roundrect (at 1.41 6.8) (size 1.16 0.8) (layers F.Paste) (roundrect_rratio 0.33)
    (solder_paste_margin -0.1))
  (pad E10 smd roundrect (at -1.41 6.8) (size 1.16 0.8) (layers F.Paste) (roundrect_rratio 0.33)
    (solder_paste_margin -0.1))
  (pad E12 smd roundrect (at 1.41 -6.8) (size 1.16 1.2) (layers F.Cu F.Mask) (roundrect_rratio 0.08599999999999999))
  (pad E13 smd roundrect (at -1.41 -6.8) (size 1.16 1.2) (layers F.Cu F.Mask) (roundrect_rratio 0.08599999999999999))
  (pad E4 smd roundrect (at 1.37 4.265) (size 2.3 3.01) (layers F.Cu F.Mask) (roundrect_rratio 0.043))
  (pad E3 smd roundrect (at -1.37 4.265) (size 2.3 3.01) (layers F.Cu F.Mask) (roundrect_rratio 0.043))
  (pad E9 smd roundrect (at 0.04 0) (size 5.5 4.68) (layers F.Cu F.Mask) (roundrect_rratio 0.021))
  (pad 7 smd roundrect (at -5.5 -3.27) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -5.5 -2.65) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -5.5 -2.21) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -5.5 -1.81) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -5.5 -1.41) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -5.5 -1.01) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -5.5 -0.61) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -5.5 -0.21) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at -5.5 1.41 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at -5.5 3.27 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at -5.5 2.65 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -5.5 0.61 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at -5.5 1.81 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at -5.5 2.21 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -5.5 0.21 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at -5.5 1.01 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 65 smd roundrect (at 5.5 -3.27 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 64 smd roundrect (at 5.5 -2.65 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 63 smd roundrect (at 5.5 -2.25 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 62 smd roundrect (at 5.5 -1.85 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 61 smd roundrect (at 5.5 -1.13 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 60 smd roundrect (at 5.5 -0.4 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 59 smd roundrect (at 5.5 0 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 5.5 0.4 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 57 smd roundrect (at 5.5 0.8 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 56 smd roundrect (at 5.5 1.53 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 55 smd roundrect (at 5.5 1.93 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 54 smd roundrect (at 5.5 2.65 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 53 smd roundrect (at 5.5 3.27 180) (size 0.8 0.2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 76 smd roundrect (at 2.51 -7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 80 smd roundrect (at 0.32 -7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 81 smd roundrect (at -0.32 -7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 85 smd roundrect (at -2.51 -7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at -2.51 7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 37 smd roundrect (at -0.31 7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 38 smd roundrect (at 0.32 7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 42 smd roundrect (at 2.51 7) (size 0.2 0.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -5.5 -3.27) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 8 smd roundrect (at -5.5 -2.65) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 9 smd roundrect (at -5.5 -2.21) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 10 smd roundrect (at -5.5 -1.81) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 11 smd roundrect (at -5.5 -1.41) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 12 smd roundrect (at -5.5 -1.01) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 13 smd roundrect (at -5.5 -0.61) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 14 smd roundrect (at -5.5 -0.21) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 18 smd roundrect (at -5.5 1.41 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 22 smd roundrect (at -5.5 3.27 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 21 smd roundrect (at -5.5 2.65 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 16 smd roundrect (at -5.5 0.61 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 19 smd roundrect (at -5.5 1.81 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 20 smd roundrect (at -5.5 2.21 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 15 smd roundrect (at -5.5 0.21 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 17 smd roundrect (at -5.5 1.01 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 65 smd roundrect (at 5.5 -3.27 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 64 smd roundrect (at 5.5 -2.65 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 63 smd roundrect (at 5.5 -2.25 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 62 smd roundrect (at 5.5 -1.85 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 61 smd roundrect (at 5.5 -1.13 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 60 smd roundrect (at 5.5 -0.4 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 59 smd roundrect (at 5.5 0 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 58 smd roundrect (at 5.5 0.4 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 57 smd roundrect (at 5.5 0.8 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 56 smd roundrect (at 5.5 1.53 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 55 smd roundrect (at 5.5 1.93 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 54 smd roundrect (at 5.5 2.65 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 53 smd roundrect (at 5.5 3.27 180) (size 0.6 0.2) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 76 smd roundrect (at 2.51 -7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 80 smd roundrect (at 0.32 -7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 81 smd roundrect (at -0.32 -7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 85 smd roundrect (at -2.51 -7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 33 smd roundrect (at -2.51 7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 37 smd roundrect (at -0.31 7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 38 smd roundrect (at 0.32 7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad 42 smd roundrect (at 2.51 7) (size 0.2 0.6) (layers F.Paste) (roundrect_rratio 0.33))
  (pad E7 smd roundrect (at 1.37 -4.265) (size 2.3 3.01) (layers F.Cu F.Mask) (roundrect_rratio 0.043))
  (pad E8 smd roundrect (at -1.37 -4.265) (size 2.3 3.01) (layers F.Cu F.Mask) (roundrect_rratio 0.043)
    (solder_paste_margin -0.2))
  (pad E13 smd roundrect (at -1.41 -6.8) (size 1.16 0.8) (layers F.Paste) (roundrect_rratio 0.33)
    (solder_paste_margin -0.1))
  (pad E12 smd roundrect (at 1.41 -6.8) (size 1.16 0.8) (layers F.Paste) (roundrect_rratio 0.33)
    (solder_paste_margin -0.1))
  (pad E10 smd roundrect (at -1.41 6.8) (size 1.16 1.2) (layers F.Cu F.Mask) (roundrect_rratio 0.08599999999999999))
  (pad E11 smd roundrect (at 1.41 6.8) (size 1.16 1.2) (layers F.Cu F.Mask) (roundrect_rratio 0.08599999999999999))
  (pad E1 smd roundrect (at -3.5 -4.45) (size 0.75 1) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E1 smd roundrect (at -3.5 -6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E1 smd roundrect (at -4.7 -4.45) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E1 smd roundrect (at -4.7 -6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E6 smd roundrect (at 3.5 -4.45) (size 0.75 1) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E6 smd roundrect (at 4.7 -4.45) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E6 smd roundrect (at 4.7 -6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E6 smd roundrect (at 3.5 -6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E2 smd roundrect (at -3.5 4.45) (size 0.75 1) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E2 smd roundrect (at -4.7 4.45) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E2 smd roundrect (at -4.7 6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E2 smd roundrect (at -3.5 6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E5 smd roundrect (at 3.5 4.45) (size 0.75 1) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E5 smd roundrect (at 4.7 4.45) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E5 smd roundrect (at 3.5 6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E5 smd roundrect (at 4.7 6.05) (size 1 1.3) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E8 smd roundrect (at -0.8 -5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E8 smd roundrect (at -0.8 -3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E8 smd roundrect (at -2 -3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E8 smd roundrect (at -2 -5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E7 smd roundrect (at 0.8 -5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E7 smd roundrect (at 0.8 -3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E7 smd roundrect (at 2 -3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E7 smd roundrect (at 2 -5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E4 smd roundrect (at 2 3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E4 smd roundrect (at 0.8 3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E4 smd roundrect (at 0.8 5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E4 smd roundrect (at 2 5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E3 smd roundrect (at -0.8 3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E3 smd roundrect (at -0.8 5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E3 smd roundrect (at -2 5.1) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E3 smd roundrect (at -2 3.45) (size 0.8 1.4) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -1.95 -1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -0.65 -1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 0.65 -1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 1.95 -1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -1.95 0) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -0.65 0) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 0.65 0) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 1.95 0) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -1.95 1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at -0.65 1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 0.65 1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (pad E9 smd roundrect (at 1.95 1.3) (size 1.15 1.15) (layers F.Paste) (roundrect_rratio 0.25))
  (model Package_DFN_QFN.3dshapes/ST_powerSTEP01.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
