(footprint "4P_2x1.5_P2.0" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "NightLight.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole exclude_from_pos_files exclude_from_bom)
  (fp_text reference "J1" (at 0 -4.525 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp da08b8ff-609e-4109-8374-0f1c1a348554)
  )
  (fp_text value "SWD" (at 2.375 0 90 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 03311fd0-96a0-4e58-971b-1d9d7c0c11dc)
  )
  (fp_text user "${REF}" (at -0.1 -7.175 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 48f859c2-cff2-4782-a4ac-e5a9c5416425)
  )
  (fp_poly
    (pts
      (xy -1.15 -3)
      (xy -1.4 -2.8)
      (xy -1.4 -3.2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3b956370-1e75-422e-b1ea-0b2a34dea317))
  (fp_line (start -1.15 -3.5) (end -1.15 3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b0f96014-ac09-40de-aab6-2c1fe3beeea5))
  (fp_line (start 0.75 -3.9) (end -0.75 -3.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 944a2351-9b31-4ceb-9f67-2b2e64b27f1d))
  (fp_line (start 0.75 3.9) (end -0.75 3.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2fdcc3b3-17f9-4da1-88a3-55155c278a5c))
  (fp_line (start 1.15 3.5) (end 1.15 -3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85a2a54f-7d74-42ee-8d4b-a52fed18accf))
  (fp_arc (start -1.15 -3.5) (mid -1.032843 -3.782843) (end -0.75 -3.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6a06eb6d-52ab-474e-8061-764b096f0035))
  (fp_arc (start -0.75 3.9) (mid -1.032843 3.782843) (end -1.15 3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 13b4aef3-306c-47dc-b963-8db9f0240589))
  (fp_arc (start 0.75 -3.9) (mid 1.032843 -3.782843) (end 1.15 -3.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e126c090-37d6-4834-ac95-538e2c0ceb76))
  (fp_arc (start 1.15 3.5) (mid 1.032843 3.782843) (end 0.75 3.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b46a7896-f565-4ffb-9c71-a0a420d59ba8))
  (pad "1" connect roundrect (at 0 -3) (size 2 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp ee230bf6-81f6-45bf-a580-e8309afedbd1))
  (pad "2" connect roundrect (at 0 -1) (size 2 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 080fbcbe-b5cd-4772-8a3f-83df00447e55))
  (pad "3" connect roundrect (at 0 1) (size 2 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp c2440b3a-ec3d-42df-94e6-c05063038cd0))
  (pad "4" connect roundrect (at 0 3) (size 2 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 588acc93-9c9b-42c4-a6d5-926a7482a3b3))
)
