(footprint "MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly" (version 20210722) (generator pcbnew) (layer "F.Cu")
  (tedit 610A8851)
  (descr "Mounting Hole 3.2mm, M3, ISO7380")
  (tags "mounting hole 3.2mm m3 iso7380")
  (property "Sheetfile" "StepperDriverModuleCarrier.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "H2" (at 0 -3.85) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c47a818e-2547-43b2-92fd-ec575d406037)
  )
  (fp_text value "MOUNT_HOLE" (at 0 3.85) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 543e66fd-979d-491b-bac1-b49ee784607d)
  )
  (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9edb8403-0770-426a-8178-189e341fd8b3)
  )
  (fp_circle (center 0 0) (end 2.85 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 9660d92b-1f7a-4b8b-8b37-40a203815bfa))
  (fp_circle (center 0 0) (end 3.1 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 5bb02b26-6a0b-4a20-bf46-32adf63dbb68))
  (pad "1" connect circle (at 0 0) (size 5.7 5.7) (layers "F.Cu" "F.Mask") (tstamp be34f541-6f00-4f1a-9654-4c27b53705c5))
  (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask) (tstamp c4d4f680-8c45-436f-9398-0af805037976))
)
