(footprint "JST_SH_SM11B-SRSS-TB_1x11-1MP_P1.00mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, SM11B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH top entry")
  (property "Sheetfile" "Servo_Controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J10" (at 0.05 -3.4) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 119038e5-5e16-43e1-8895-aa8ae8554cb6)
  )
  (fp_text value "GPIO" (at 0 2.3) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 95c3c6e2-b0b4-4c5b-9939-89718e004641)
  )
  (fp_text user "${REFERENCE}" (at 0 1.9) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp cf55bfa6-b139-41fa-ad47-cb459ac63f0a)
  )
  (fp_line (start -6.61 -1.785) (end -5.56 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4734217f-9ad8-4920-813c-cf43ae9c01ff))
  (fp_line (start -6.61 0.715) (end -6.61 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3fd07b6e-23d2-4c4d-8233-1829c534e11c))
  (fp_line (start -5.56 -1.785) (end -5.56 -2.775)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6cf2ffbd-f66d-4e65-a8bb-2cf9469ee041))
  (fp_line (start -5.44 2.685) (end 5.44 2.685)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 810a6f67-a413-47eb-8af3-7e26a76bfb46))
  (fp_line (start 6.61 -1.785) (end 5.56 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5aaa320-9b89-444f-a350-3ab988910cff))
  (fp_line (start 6.61 0.715) (end 6.61 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0e92285-2f60-4e52-9db9-4bfe16b23f07))
  (fp_line (start -7.05 2.55) (end -7.05 1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 02a75282-ab40-4da1-a71a-980292a313cd))
  (fp_line (start -6.75 -1.7) (end -6.747014 0.811943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b1fc1314-e89c-494f-bc03-69f7b47dd183))
  (fp_line (start -6.65 2.95) (end 6.65 2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 98fc90c6-8c60-430c-b85b-9f620cb0c309))
  (fp_line (start -6.5 -1.95) (end -5.45 -1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 390b88d7-cd86-4bcc-99fd-a542bb358c4a))
  (fp_line (start -5.45 -1.95) (end -5.45 -2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b876b0de-5662-43c0-a31d-f03761e39393))
  (fp_line (start -5.15 -2.95) (end 5.15 -2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d59d0da-f433-4ab6-88a7-ead88e633841))
  (fp_line (start 5.45 -1.95) (end 5.45 -2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3d561738-56d2-49b4-aec2-12bb7965f266))
  (fp_line (start 6.5 -1.95) (end 5.45 -1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d11418d-65ce-49bd-b797-7cd20b48d7ae))
  (fp_line (start 6.75 -1.7) (end 6.747014 0.811943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 264ca2b2-3489-4a8b-9d9f-88fba30227ef))
  (fp_line (start 7.05 2.55) (end 7.05 1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1ecb4821-32bb-4701-b221-8ea1c9143152))
  (fp_arc (start -7.05 1.2) (mid -6.965282 0.953835) (end -6.747014 0.811943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9787ed8f-56fb-4312-96cb-be2885459ef9))
  (fp_arc (start -6.75 -1.7) (mid -6.676777 -1.876777) (end -6.5 -1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 424a955f-87e7-4c98-9e3f-52ce50ba0a0a))
  (fp_arc (start -6.65 2.95) (mid -6.932843 2.832843) (end -7.05 2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 138cfd7a-3c5b-45ac-85be-8fc0ab9b85f8))
  (fp_arc (start -5.45 -2.65) (mid -5.362132 -2.862132) (end -5.15 -2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9fc01c1b-f3d4-4bbd-88c9-29fbcccaf05c))
  (fp_arc (start 5.15 -2.95) (mid 5.362132 -2.862132) (end 5.45 -2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 188d4fa5-002d-4145-9c91-9ce11d004330))
  (fp_arc (start 6.5 -1.95) (mid 6.676777 -1.876777) (end 6.75 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0a067fae-fd97-4732-85a6-1ac50ee9545a))
  (fp_arc (start 6.747014 0.811943) (mid 6.965282 0.953835) (end 7.05 1.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 67a113b7-a9c3-4796-be05-2f2ab8707782))
  (fp_arc (start 7.05 2.55) (mid 6.932843 2.832843) (end 6.65 2.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d194f161-09df-4d1a-89dc-f95fcbbdc3a4))
  (fp_line (start -6.5 -1.675) (end -6.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9b98da48-6339-414d-af93-1c8b2380754f))
  (fp_line (start -6.5 -1.675) (end 6.5 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a482dbe4-86eb-4fd9-afa9-152822f353ca))
  (fp_line (start -6.5 2.575) (end 6.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 107d516c-dbf3-40a9-8f0f-f7a85c013147))
  (fp_line (start -5.5 -1.675) (end -5 -0.967893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31fe584c-98f3-450a-a167-e6548bc461cf))
  (fp_line (start -5 -0.967893) (end -4.5 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 763d83c0-dc3b-4ea8-bc9f-7afcaa9720e9))
  (fp_line (start 6.5 -1.675) (end 6.5 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ad7dfcd-ecbe-440d-9f00-5de44a7af19e))
  (pad "1" smd roundrect (at -5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 246058e5-e77d-43c3-9a92-ad94ee3c7b3c))
  (pad "2" smd roundrect (at -4 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 666fb25f-8472-4021-ab1f-459667068dd5))
  (pad "3" smd roundrect (at -3 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d3f996fd-bb78-4f74-b02d-24e4ec8daf4c))
  (pad "4" smd roundrect (at -2 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 599e465c-8c2d-40a0-bea7-c4430c94cc56))
  (pad "5" smd roundrect (at -1 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6ae89342-73ec-4c7a-b369-d5ffa4736f6f))
  (pad "6" smd roundrect (at 0 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0be4ebaf-7607-4cd9-9b63-c4970f2efc55))
  (pad "7" smd roundrect (at 1 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 472e6c62-33da-489c-bde0-aa2e138e9d7c))
  (pad "8" smd roundrect (at 2 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7ce5aaf9-613e-413a-8a05-b74fc139b421))
  (pad "9" smd roundrect (at 3 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1032d08a-5b55-4522-810c-6c14c94cf6a6))
  (pad "10" smd roundrect (at 4 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d8b79017-4b92-4b4c-8e7e-bf0ecc2cbf5d))
  (pad "11" smd roundrect (at 5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 571a4f35-d9f5-45f3-90fa-ff2ecf752005))
  (pad "MP" smd roundrect (at -6.3 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 993bbb96-09a0-4d6a-bc35-2eec50fefd05))
  (pad "MP" smd roundrect (at 6.3 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 43a2174a-52f7-4425-986c-c5810fb179e6))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM11B-SRSS-TB_1x11-1MP_P1.00mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/JST_SH_SM11B-SRSS-TB.STEP"
    (offset (xyz 0 -0.45 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
