(footprint "JP-2_Open"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "JP1"
		(at 0 -1 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d710271b-88b5-4055-8b5c-968a0859b251")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "5V"
		(at 0 0.7 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d11e32de-7a1c-4539-9693-78358b3bcbc4")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "JP-2_Open"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "033dbde9-5784-4383-9313-a56f62f7bb1d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a385fa90-a617-4aff-ad0b-8186f5050fd5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, open"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bbb3a5ad-d445-4f94-beb5-ede27eaf09ba")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "81263274-a1ed-4d96-80cf-ad944d4227d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e08ca3d4-2a2c-4e94-bda3-0a9ef2a89a04")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.000001)
	(attr through_hole exclude_from_pos_files exclude_from_bom)
	(net_tie_pad_groups "1, 2, ")
	(fp_line
		(start -0.5 0.4)
		(end -0.5 -0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b8f59da6-9834-4395-b5ac-20434026461b")
	)
	(fp_line
		(start -0.25 -0.65)
		(end 0.25 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dd7a9674-2577-4907-a07f-3341c37f6660")
	)
	(fp_line
		(start 0.25 0.65)
		(end -0.25 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "13ad79b2-25c0-4051-8e55-b08edfe7df60")
	)
	(fp_line
		(start 0.5 -0.4)
		(end 0.5 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "61ef2790-80ea-4485-bbf1-df59f3846174")
	)
	(fp_arc
		(start -0.5 -0.4)
		(mid -0.426777 -0.576777)
		(end -0.25 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "820a8254-b0a0-417b-b8c5-6b959d6340e4")
	)
	(fp_arc
		(start -0.25 0.65)
		(mid -0.426777 0.576777)
		(end -0.5 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "55504579-b2fd-4575-96a1-757f80b58cd8")
	)
	(fp_arc
		(start 0.25 -0.65)
		(mid 0.426777 -0.576777)
		(end 0.5 -0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "97e5c383-1f39-445a-b526-6475c742406b")
	)
	(fp_arc
		(start 0.5 0.4)
		(mid 0.426777 0.576777)
		(end 0.25 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "33a3cce3-a8a1-4cb0-9d25-ae86731e1d18")
	)
	(pad "" smd rect
		(at 0 0)
		(size 0.2 1)
		(layers "F.Mask")
		(zone_connect 0)
		(uuid "1a39947f-56b7-4276-90df-0f4ec7c161a3")
	)
	(pad "1" connect roundrect
		(at -0.225 0)
		(size 0.25 1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_right bottom_right)
		(uuid "1e7aa77e-b7e9-4686-ac5a-060c263f0ab1")
	)
	(pad "2" connect roundrect
		(at 0.225 0)
		(size 0.25 1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(uuid "1a251849-83e1-4645-96c9-6456ff730676")
	)
)
