(module ScrobbyRobotics_old:TI_TPS61200 (layer F.Cu) (tedit 5368B67B)
  (tags Step-Up)
  (attr smd)
  (fp_text reference U1 (at 0 -2.5 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value TPS61200 (at 0 2.75) (layer F.SilkS) hide
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -2 2) (end -2 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 2) (end 2 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -2) (end 2 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 1) (end -3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 0.5) (end -3 0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 0) (end -3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -0.5) (end -3 -0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -1) (end -3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 1) (end 3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 0.5) (end 3 0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 0) (end 3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -0.5) (end 3 -0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -1) (end 3 -1) (layer F.SilkS) (width 0.15))
  (fp_text user 1 (at -2.5 -1.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -1.5 -2) (end 2 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -2) (end -2 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 2) (end -2 2) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.5 -1) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.5 -0.5) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.5 0) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.5 0.5) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.5 1) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.5 1) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.5 0.5) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.5 0) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.5 -0.5) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.5 -1) (size 1 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask))
)
