(module R_1225_3264Metric (layer F.Cu) (tedit 5C56DF2D)
  (descr "Resistor SMD 1225 (3264 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20035/dcrcwe3.pdf)")
  (tags resistor)
  (attr smd)
  (fp_text reference R6 (at -0.05 -4.22) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 2.4 (at 0 4.22) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.12)))
  )
  (fp_line (start 2.25 3.52) (end -2.25 3.52) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 -3.5) (end 2.25 3.52) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 -3.5) (end 2.25 -3.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 3.52) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.777064 3.31) (end 0.777064 3.31) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.777064 -3.31) (end 0.777064 -3.31) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.6 3.2) (end -1.6 3.2) (layer F.Fab) (width 0.1))
  (fp_line (start 1.6 -3.2) (end 1.6 3.2) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 -3.2) (end 1.6 -3.2) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 3.2) (end -1.6 -3.2) (layer F.Fab) (width 0.1))
  (pad 2 smd roundrect (at 1.475 0) (size 1.05 6.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238))
  (pad 1 smd roundrect (at -1.475 0) (size 1.05 6.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238))
  (model ${KICAD7_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1264_3264Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
