(footprint "JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH side entry")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J27" (at 0 -2.65) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 37a18d06-b35d-4b57-8d45-5c10cbea054d)
  )
  (fp_text value "DEBUG_USB" (at 0 2.4) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 3aee09fa-c26e-4b3c-967b-cf4efb0e7ecc)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.65) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 25d24102-68f1-4d46-85e8-ef12664a4dc0)
  )
  (fp_line (start -3.11 -0.04) (end -3.11 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a55d2c2c-a027-4a18-a8f5-71ca22848141))
  (fp_line (start -3.11 1.11) (end -2.06 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fb8c3c3b-3d14-4e7b-86bf-58693b9ad9d8))
  (fp_line (start -2.06 1.11) (end -2.06 2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b52f228-72e1-46c1-b036-cff4d890583d))
  (fp_line (start -1.94 -2.01) (end 1.94 -2.01)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 25ec7f81-ed0c-4402-9c58-6ea9101c7e2f))
  (fp_line (start 3.11 -0.04) (end 3.11 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d85c6a0e-405e-4803-b953-2073b93a1355))
  (fp_line (start 3.11 1.11) (end 2.06 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 44081775-bf82-49c8-b459-7fe4ff83f6f3))
  (fp_line (start -3.55 -1.85) (end -3.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 256371e2-4250-4dbb-95d2-c775b364e6d4))
  (fp_line (start -3.25 1) (end -3.247014 -0.161943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0b6d7f97-f7dd-4074-bfd6-f0167ca04692))
  (fp_line (start -3 1.25) (end -1.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a1677154-f27c-47d4-941a-5d555c5808c4))
  (fp_line (start -1.95 1.25) (end -1.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp acd06eb4-8419-43fb-9bb5-d11c732cf56c))
  (fp_line (start 1.65 2.25) (end -1.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a9d23066-9efd-495c-bcae-d26f41fcf6f6))
  (fp_line (start 1.95 1.25) (end 1.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a0883120-96d8-420f-ba75-73cd038a8193))
  (fp_line (start 3 1.25) (end 1.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e54c9241-32d2-4bac-a674-f9b633296ddb))
  (fp_line (start 3.15 -2.25) (end -3.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 64e9a9f4-6eb6-4e08-80b8-2cf9ec3589a7))
  (fp_line (start 3.25 1) (end 3.247014 -0.161943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0b9a6e41-acdb-4150-afcd-1df280dc81fb))
  (fp_line (start 3.55 -1.85) (end 3.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c91258e7-026a-4880-b26f-6a6eecde193b))
  (fp_arc (start -3.55 -1.85) (mid -3.432843 -2.132843) (end -3.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f215b206-60ae-487f-830b-162f3be42d28))
  (fp_arc (start -3.247014 -0.161943) (mid -3.465282 -0.303835) (end -3.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 78141a38-3f6e-4a39-b0db-ca6ff3c172e6))
  (fp_arc (start -3 1.25) (mid -3.176777 1.176777) (end -3.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 255c0d87-7e93-4523-bce4-56e07edca286))
  (fp_arc (start -1.65 2.25) (mid -1.862132 2.162132) (end -1.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c545209c-d01c-43dd-b26b-f244a6a8a29e))
  (fp_arc (start 1.95 1.95) (mid 1.862132 2.162132) (end 1.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d0b2dc0e-cc6e-4403-9e0e-76ddd123565b))
  (fp_arc (start 3.15 -2.25) (mid 3.432843 -2.132843) (end 3.55 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 04f6e694-cf4c-4108-8fd1-86816044b197))
  (fp_arc (start 3.25 1) (mid 3.176777 1.176777) (end 3 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fd272d53-c01a-4ea2-9e50-b355c31ecca9))
  (fp_arc (start 3.55 -0.55) (mid 3.465282 -0.303835) (end 3.247014 -0.161943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 95b309f7-f41a-48c7-9f1c-334d5eab427c))
  (fp_line (start -3 -1.9) (end 3 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 204fe597-9587-4e0e-8024-f6a838ad9936))
  (fp_line (start -3 1) (end -3 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a5298805-b346-401e-bcb5-4f006941ac7e))
  (fp_line (start -3 1) (end 3 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b08c0167-fe35-4ce3-a46a-6c9da6f9cd29))
  (fp_line (start -2 1) (end -1.5 0.292893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8332e446-5f27-41d7-9856-b7d5727d553b))
  (fp_line (start -1.65 -1.55) (end -1.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b1bbbf52-383f-4985-af0c-e6cf91904b6e))
  (fp_line (start -1.65 -0.95) (end -1.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c5d101f0-a6d2-4e73-827e-f7fce06ace9a))
  (fp_line (start -1.5 0.292893) (end -1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be664875-e71f-4685-9e41-568d11cad830))
  (fp_line (start -1.35 -1.55) (end -1.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77bc3df9-7771-41a7-a4b8-fe359a8d3409))
  (fp_line (start -1.35 -0.95) (end -1.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f23556ea-d35a-4999-b1d1-0a93a6e07a54))
  (fp_line (start -0.65 -1.55) (end -0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4a9aa2e2-9eab-4ea0-95c9-d0103f51e81c))
  (fp_line (start -0.65 -0.95) (end -0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b562cf71-6826-4cd3-a21a-14a4e8174e8e))
  (fp_line (start -0.35 -1.55) (end -0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 11866f9a-44b0-4cf5-af57-19cc7a0abdc9))
  (fp_line (start -0.35 -0.95) (end -0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1109e454-407e-4c0e-9b58-0c0ad745819d))
  (fp_line (start 0.35 -1.55) (end 0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b002b8b1-0c29-45f4-a044-dd0ead113e4c))
  (fp_line (start 0.35 -0.95) (end 0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d5d7787-a0b9-4a1b-90b3-b4b8ba3af9c3))
  (fp_line (start 0.65 -1.55) (end 0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b5e496f-1a9c-4902-906b-76d73093b211))
  (fp_line (start 0.65 -0.95) (end 0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 97a3cf12-8f18-49f0-a5a1-b87e781c1d88))
  (fp_line (start 1.35 -1.55) (end 1.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8db75006-7bcc-41bf-8d23-aa7c54bdba2d))
  (fp_line (start 1.35 -0.95) (end 1.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0569dccd-030e-449b-8b7c-0a855d047660))
  (fp_line (start 1.65 -1.55) (end 1.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81cb5445-18c0-4665-9c20-33e45cb6f0f3))
  (fp_line (start 1.65 -0.95) (end 1.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0ee00366-0992-4da7-adbe-ed4a3a620450))
  (fp_line (start 3 1) (end 3 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8556d7b8-dee0-431f-8161-4b428688bf13))
  (pad "1" smd roundrect (at -1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 59f28d58-e056-4a76-b6ad-b5bfd064b471))
  (pad "2" smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9f3aaaee-79e4-4bca-a0c2-7e8f76295f4c))
  (pad "3" smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 103e7987-39d9-40f6-be1b-ab02af02ddd2))
  (pad "4" smd roundrect (at 1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 26da1872-bac7-4586-8112-77b06b0c7cb1))
  (pad "MP" smd roundrect (at -2.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 0f88e8f2-601a-4d51-bf32-28d4f03cdc0f))
  (pad "MP" smd roundrect (at 2.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp dea08756-5acb-4d4d-91ba-1c906bf4142c))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB.STEP"
    (offset (xyz 0 0.45 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
