(footprint "2P_7.3x7.3_P8.55" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6006DEB5)
  (property "MPN" "NO PART")
  (property "Sheet file" "BrushedMotorController18V15A.kicad_sch")
  (property "Sheet name" "")
  (attr exclude_from_pos_files)
  (fp_text reference "M1" (at -8.6 0 90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 377ef299-c6b7-49d1-98cc-fc861f4c9be9)
  )
  (fp_text value "MOTOR" (at -6.5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 41dd27b7-bc6b-43a4-b623-5cee0f3b3a6c)
  )
  (fp_text user "${REF}" (at -5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d56cf250-205a-481e-b146-44497cd1c066)
  )
  (pad "1" connect rect (at -4.275 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp fba12576-bd4e-4da1-a994-adb289ab9120))
  (pad "2" connect rect (at 4.275 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 4ea44218-4ba1-4f20-a1f8-03c7e99e2075))
)
