(module "LGA-10_2x2mm_P0.5mm" (layer F.Cu) (tedit 5CECC1FD)
  (descr "LGA10")
  (tags "lga land grid array")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.85) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "LGA-10_2x2mm_P0.5mm" (at 0 1.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.1))
  (fp_line (start -1 1) (end -1 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1 -0.5) (end -0.5 -1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1) (end 1 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 -1.1) (end 1.1 -1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.1 -1.1) (end 1.1 -0.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.1 -0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.1 0.6) (end 1.1 1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.1 1.1) (end 0.6 1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.6 1.1) (end 0.6 1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.6 1.1) (end -1.1 1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.1 1.1) (end -1.1 0.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.1 0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.6 -1.1) (end -1.1 -1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.1 -1.1) (end -1.1 -1.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.25 -1.25) (end 1.25 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 1.25) (end -1.25 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 1.25) (end -1.25 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 -1.25) (end 1.25 -1.25) (layer F.CrtYd) (width 0.05))
  (pad "1" smd rect (at -0.7625 -0.25) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -0.7625 0.25) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 0.7625 -0.25) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 0.7625 0.25) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 0.5125 0.75) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 0.5125 -0.75) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -0.5 0.7625 90) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0 0.7625 90) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 0 -0.7625 90) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -0.5 -0.7625 90) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KICAD7_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
