(module 8-LFCSP_UD_2x2_0.5mm_TE_DFN (layer F.Cu) (tedit 585DB022)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.025)
  (attr smd)
  (fp_text reference REF** (at 0 -1.65) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value 8-LFCSP_UD_2x2_0.5mm_TE_DFN (at 1.5 0 90) (layer F.Fab)
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (fp_line (start -1 -1) (end 1 -1) (layer F.Fab) (width 0.05))
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.05))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.05))
  (fp_line (start -1 1) (end -1 -1) (layer F.Fab) (width 0.05))
  (fp_line (start -1.2 1.2) (end -1.2 0.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 1.2) (end -1 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 -1.2) (end -1 -1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 -1.2) (end -1.2 -0.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 -1.2) (end 1 -1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 -1.2) (end 1.2 -0.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 1.2) (end 1 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 1.2) (end 1.2 0.7) (layer F.SilkS) (width 0.125))
  (fp_circle (center -1.4 1.15) (end -1.4 1.2) (layer F.SilkS) (width 0.125))
  (pad 1 smd roundrect (at -0.75 0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 9 smd roundrect (at 0 0) (size 1.6 1) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.05)
    (solder_paste_margin_ratio -0.3))
  (pad 2 smd roundrect (at -0.25 0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 3 smd roundrect (at 0.25 0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 4 smd roundrect (at 0.75 0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 5 smd roundrect (at 0.75 -0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 6 smd roundrect (at 0.25 -0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 7 smd roundrect (at -0.25 -0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (pad 8 smd roundrect (at -0.75 -0.875) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.2))
  (model Package_DFN_QFN.3dshapes/8-LFCSP_UD_2x2_0.5_TE.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
