(footprint "6432_C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "MFG" "")
  (property "MPN" "")
  (property "Sheetfile" "G4ESC.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Shunt resistor, US symbol")
  (property "ki_keywords" "R res shunt resistor")
  (attr smd)
  (fp_text reference "R1" (at -2.7 -2.3) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 938b2c9e-ee05-40c0-a2f8-2a11d1b22a57)
  )
  (fp_text value "R_Shunt" (at 0 -1.1) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp cc3fd940-848e-412d-9c89-dc512119bd61)
  )
  (fp_line (start -1.8 -1.7) (end 1.8 -1.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 866b442a-18d8-4cfe-91f5-51baa2f75d68))
  (fp_line (start -1.8 1.7) (end 1.8 1.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f977dcf4-072a-4116-9439-381a7aaefdc2))
  (fp_line (start -3.45 -1.55) (end -3.45 1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 671324e5-a5ce-4b57-b3ec-e120ea391077))
  (fp_line (start -3.15 1.85) (end 3.15 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6222081-c5ab-48c8-9441-6fdeda184151))
  (fp_line (start 3.15 -1.85) (end -3.15 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d49672ce-fedf-41c9-92e3-1a4d204fd208))
  (fp_line (start 3.45 1.55) (end 3.45 -1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9ff31b93-69e2-4e81-bd86-1d7a45050645))
  (fp_arc (start -3.45 -1.55) (mid -3.362132 -1.762132) (end -3.15 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 784db787-3146-488a-896c-7ed3d1692834))
  (fp_arc (start -3.15 1.85) (mid -3.362132 1.762132) (end -3.45 1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7bcd7b10-982b-4c36-95f6-21f331fc490c))
  (fp_arc (start 3.15 -1.85) (mid 3.362132 -1.762132) (end 3.45 -1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 989da9a1-8256-423f-9517-e19a93c0a9a6))
  (fp_arc (start 3.45 1.55) (mid 3.362132 1.762132) (end 3.15 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 73834526-19f7-4cc3-8746-b4816b6d88d2))
  (fp_line (start -3.2 -1.6) (end 3.2 -1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp f23b4dc7-2ae0-4217-884e-c501e1fba4ef))
  (fp_line (start -3.2 1.6) (end -3.2 -1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 70882957-a268-454a-b5c9-ce7d9564ada1))
  (fp_line (start 3.2 -1.6) (end 3.2 1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 0b1cce8a-7e43-4975-b312-ef940b3d2586))
  (fp_line (start 3.2 1.6) (end -3.2 1.6)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 644587b6-846a-4a1c-8364-6fab922ab10f))
  (pad "1" smd roundrect (at -2.75 0) (size 1.1 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.119) (tstamp 5ad01fc4-67d2-4e3c-8a6d-efe4eb01cbf5))
  (pad "2" smd roundrect (at 2.75 0) (size 1.1 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.119) (tstamp 5bcb55e3-fbd4-48f9-8e6e-e4b74085ae6f))
  (model "Resistor_SMD.3dshapes/Resistor_SMD_6432.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
