(footprint "Battery_Connector_Contacts_[BC-35-3P]_mod" (version 20220211) (generator pcbnew)
  (layer "F.Cu")
  (tedit 620A795D)
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.9 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c58960d9-4cac-4036-ad2e-1aef26946dae)
  )
  (fp_text value "Battery_Connector_Contacts_[BC-35-3P]_mod" (at 0 0.95 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 5b96c1ad-46ba-4366-8241-fbc1cd0e9bbd)
  )
  (fp_text user "${REFERENCE}" (at 0 3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp fced3dbe-eec8-4979-aefd-686432f00d6c)
  )
  (fp_arc (start -3.975 -2.9) (mid -3.953033 -2.953033) (end -3.9 -2.975)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1732b93f-cd0e-4ca4-a905-bb406354ca33))
  (fp_arc (start -3.9 2.975) (mid -3.953033 2.953033) (end -3.975 2.9)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e0d7c1d9-102e-4758-a8b7-ff248f1ce315))
  (fp_arc (start 3.9 -2.975) (mid 3.953033 -2.953033) (end 3.975 -2.9)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 0c544a8c-9f45-4205-9bca-1d91c95d58ef))
  (fp_arc (start 3.975 2.9) (mid 3.953033 2.953033) (end 3.9 2.975)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp cd50b8dc-829d-4a1d-8f2a-6471f378ba87))
  (fp_poly
    (pts
      (xy -3.9 1.9)
      (xy -3.9 2.9)
      (xy -2.9 2.9)
      (xy -2.9 3.05)
      (xy -3.9 3.05)
      (xy -4.05 2.9)
      (xy -4.05 1.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2028d85e-9e27-4758-8c0b-559fad072813))
  (fp_poly
    (pts
      (xy -3.35 -2.9)
      (xy -3.9 -2.9)
      (xy -3.9 -1.9)
      (xy -4.05 -1.9)
      (xy -4.05 -2.9)
      (xy -3.9 -3.05)
      (xy -3.35 -3.05)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f6a3288e-9575-42bb-af05-a920d59aded8))
  (fp_poly
    (pts
      (xy 2.9 2.9)
      (xy 3.9 2.9)
      (xy 3.9 1.9)
      (xy 4.05 1.9)
      (xy 4.05 2.9)
      (xy 3.9 3.05)
      (xy 2.9 3.05)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp bb5d2eae-a96e-45dd-89aa-125fe22cc2fa))
  (fp_poly
    (pts
      (xy 3.9 -1.9)
      (xy 3.9 -2.9)
      (xy 3.35 -2.9)
      (xy 3.35 -3.05)
      (xy 3.9 -3.05)
      (xy 4.05 -2.9)
      (xy 4.05 -1.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp facb0614-068b-4c9c-a466-d374df96a94c))
  (fp_rect (start -3.75 -2.725) (end 3.75 2.725)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp dfcef016-1bf5-4158-8a79-72d38a522877))
  (pad "1" smd roundrect (at -2.5 -2.225) (size 1.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07142857143)
    (thermal_bridge_angle 45) (tstamp 42ecdba3-f348-4384-8d4b-cd21e56f3613))
  (pad "2" smd roundrect (at 0 -2.225) (size 1.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07142857143)
    (thermal_bridge_angle 45) (tstamp f08895dc-4dcb-4aef-a39b-5a08864cdaaf))
  (pad "3" smd roundrect (at 2.5 -2.225) (size 1.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07142857143)
    (thermal_bridge_angle 45) (tstamp 2ba25c40-ea42-478e-9150-1d94fa1c8ae9))
  (pad "MP" smd roundrect (at -1.25 2.225) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 96781640-c07e-4eea-a372-067ded96b703))
  (pad "MP" smd roundrect (at 1.25 2.225) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 3c3e06bd-c8bb-4ec8-84e0-f7f9437909b3))
  (model "${KICAD7_3DMODEL_DIR}/Connector.3dshapes/Battery_Connector_Contacts_[BC-35-3P]_mod.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
