(module Sharp_GP2S60 (layer F.Cu) (tedit 5BDDB89E)
  (solder_mask_margin 0.002)
  (solder_paste_margin -0.08)
  (attr smd)
  (fp_text reference U1 (at 0 -1.3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Sharp_GP2S60 (at 0 1) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user ZONE (at -0.5 0.7) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user COPPER (at -0.4 0.499999) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user NO (at -0.65 0.3) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_line (start 0.85 -0.85) (end 0.85 0.85) (layer F.Fab) (width 0.05))
  (fp_line (start -0.85 -0.85) (end -0.85 0.85) (layer F.Fab) (width 0.05))
  (fp_circle (center -1.5 -1.1) (end -1.6 -1.1) (layer F.SilkS) (width 0.125))
  (fp_circle (center 0 -0.5) (end 0 -0.3) (layer F.Fab) (width 0.05))
  (fp_text user Detector (at -0.499999 -0.35 90) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user Emitter (at 0.7 -0.25 90) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_line (start 0.625 0.22) (end 0.775 0.22) (layer F.Fab) (width 0.05))
  (fp_line (start 0.7 0.149999) (end 0.699999 0.3) (layer F.Fab) (width 0.05))
  (fp_line (start -0.624999 -0.3) (end -0.775 -0.299999) (layer F.Fab) (width 0.05))
  (fp_line (start -0.7 -0.375001) (end -0.699999 -0.225) (layer F.Fab) (width 0.05))
  (fp_line (start -1.35 -0.325) (end -1.35 -0.85) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 -0.325) (end -1.35 -0.325) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 0.325) (end -1.6 -0.325) (layer F.Fab) (width 0.05))
  (fp_line (start -1.35 0.325) (end -1.6 0.325) (layer F.Fab) (width 0.05))
  (fp_line (start -1.349999 0.85) (end -1.35 0.325) (layer F.Fab) (width 0.05))
  (fp_line (start 1.35 -0.325) (end 1.349999 -0.85) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 -0.325) (end 1.35 -0.325) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 0.325) (end 1.6 -0.325) (layer F.Fab) (width 0.05))
  (fp_line (start 1.35 0.325) (end 1.6 0.325) (layer F.Fab) (width 0.05))
  (fp_line (start 1.35 0.85) (end 1.35 0.325) (layer F.Fab) (width 0.05))
  (fp_line (start -1.349999 0.85) (end 1.35 0.85) (layer F.Fab) (width 0.05))
  (fp_line (start -1.35 -0.85) (end 1.349999 -0.85) (layer F.Fab) (width 0.05))
  (pad 4 smd roundrect (at 1.35 -0.55) (size 1 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 1.349999 0.55) (size 1 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1.35 0.55) (size 1 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -1.349999 -0.55) (size 1 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Sensor_Optical.3dshapes/Sharp_GP2S60.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
