(footprint "Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm_ThermalVias"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Texas SIL0008D MicroSiP, 8 Pin (http://www.ti.com/lit/ds/symlink/tps82130.pdf#page=19), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Texas MicroSiP NoLead")
	(property "Reference" "U9"
		(at 0 -2.450001 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d625e05f-d9c3-4fcd-910a-240553c30277")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TPS82130"
		(at 0 2.450001 0)
		(layer "F.Fab")
		(uuid "3aaaaa85-b5cc-41a4-9927-3f8d169371a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm_ThermalVias"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5576de9e-e429-4f76-9ea0-aeed57245786")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps82130.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "00060531-47ee-4af7-b443-d719495147df")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "17V Input 3A Step-Down Converter MicroSiP Module with Integrated Inductor, μSiL-8"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1ed5faf4-f93c-4729-b3ce-535507866863")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(zone_connect 2)
	(attr smd)
	(fp_line
		(start -1.4 1.609999)
		(end 1.4 1.609999)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "88e9ac8e-5dab-4180-b494-f79a1d9f280a")
	)
	(fp_line
		(start -1.29 -1.61)
		(end 1.4 -1.609999)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "011b4bd9-8ef9-4a51-9bab-ea1dbe29e66a")
	)
	(fp_poly
		(pts
			(xy -1.53 -1.38) (xy -1.81 -1.38) (xy -1.53 -1.66) (xy -1.53 -1.38)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "4b763b6a-d003-4949-8c69-b46aa803ecc5")
	)
	(fp_line
		(start -1.65 1.5)
		(end -1.65 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "13533c56-5643-4906-a863-7090c17cbba0")
	)
	(fp_line
		(start -1.4 -1.749999)
		(end 1.4 -1.749999)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "445d6b67-d4b1-4d1b-928f-b337ae77b702")
	)
	(fp_line
		(start 1.4 1.749999)
		(end -1.4 1.749999)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0a5ce8f2-c59b-4057-9554-02cc7f4b93bd")
	)
	(fp_line
		(start 1.65 -1.5)
		(end 1.65 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a67cd77f-070f-4357-aa53-871c6b93e7d3")
	)
	(fp_arc
		(start -1.65 -1.5)
		(mid -1.576777 -1.676777)
		(end -1.4 -1.749999)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b4e46e29-9cd3-4cda-bad2-ddc61ea9d10c")
	)
	(fp_arc
		(start -1.4 1.749999)
		(mid -1.576776 1.676776)
		(end -1.65 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ea542702-fb2a-4649-9c94-45b2ee3bad83")
	)
	(fp_arc
		(start 1.4 -1.749999)
		(mid 1.576776 -1.676776)
		(end 1.65 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2f5c58fa-b648-415a-9e18-920ccd4168ce")
	)
	(fp_arc
		(start 1.65 1.5)
		(mid 1.576777 1.676777)
		(end 1.4 1.749999)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8c1ba966-2b00-4852-9036-f119f9293e06")
	)
	(fp_line
		(start -1.4 -1.5)
		(end 1.4 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "17dcf04e-ed24-47bd-aaf6-a7bb2c5d7f14")
	)
	(fp_line
		(start -1.4 -0.8)
		(end -0.7 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4e1c8042-c153-461e-b2dd-1108827de87b")
	)
	(fp_line
		(start -1.4 1.5)
		(end -1.4 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "29f84443-749b-4277-80f0-dcbe0cdc45fe")
	)
	(fp_line
		(start 1.4 -1.5)
		(end 1.4 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7f27f7b0-2b64-4f29-bd76-7dea1f7888f5")
	)
	(fp_line
		(start 1.4 1.5)
		(end -1.4 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ffd0dbee-4f49-4679-99a9-1944ee7d6f0d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "ce614d33-edb6-4b65-a0f5-4643b54e1089")
		(effects
			(font
				(size 0.75 0.75)
				(thickness 0.11)
			)
		)
	)
	(pad "" smd roundrect
		(at 0 -0.63)
		(size 0.95 0.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "20bf9d9b-0a17-476f-b462-554eccab3462")
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 0.95 0.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f9170b1a-b9c9-491a-8eaa-a309d960ea0d")
	)
	(pad "" smd roundrect
		(at 0 0.63)
		(size 0.95 0.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "659ef01a-3f52-4195-b41e-0658eb052975")
	)
	(pad "1" smd roundrect
		(at -1.0625 -0.975)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "b283742a-9a1b-4314-82af-8b142b90b24c")
	)
	(pad "2" smd roundrect
		(at -1.0625 -0.325)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ceb7d8ce-85a5-498e-b385-33f5362175b5")
	)
	(pad "3" smd roundrect
		(at -1.0625 0.325)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "6704d804-86f8-4fb5-8936-9adeda4adcdc")
	)
	(pad "4" smd roundrect
		(at -1.0625 0.975)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "14f8e9eb-5d6c-4f79-b2c5-38fb54947ce1")
	)
	(pad "5" smd roundrect
		(at 1.0625 0.975)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "3d5e1d91-e4b8-4830-b1bf-4ceb45c5b688")
	)
	(pad "6" smd roundrect
		(at 1.0625 0.325)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "09579408-4aa3-4218-a4d2-f6ef9fd318c0")
	)
	(pad "7" smd roundrect
		(at 1.0625 -0.325)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "459de701-2d8d-4f85-8d1a-45fb0ca87267")
	)
	(pad "8" smd roundrect
		(at 1.0625 -0.975)
		(size 0.625 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "88198422-6228-4d84-b2ce-eeb79cdaacb1")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.1 1.9)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(uuid "4e810989-d75f-42c7-a327-b958d348dfa2")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_LGA.3dshapes/Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/SIL0008D.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
