(footprint "Wurth WE-STST 4532" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.35 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 05303614-d4ec-429a-85c5-651e27cfc106)
  )
  (fp_text value "Wurth WE-STST 4532" (at -0.55 -0.85 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 07057619-fa23-4187-af70-4fb979056633)
  )
  (fp_text user "${REFERENCE}" (at 0.85 0.8 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp f2e0150b-7d13-491e-b4d8-aa8344f27447)
  )
  (fp_rect (start -2.6 -0.95) (end -2.45 0.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 208e9bf1-93ac-44cc-864f-9cace74f5aaf))
  (fp_rect (start -1.25 -1.7) (end 1.25 -1.85)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2f305931-4165-4f8b-aa1e-20884e3d3e00))
  (fp_rect (start -1.25 1.85) (end 1.25 1.7)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a5af8ecb-0c46-43d8-af1b-30a4c62fd58c))
  (fp_rect (start 2.45 -0.3) (end 2.6 0.95)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8ffa265c-c4c3-4d1d-8837-9b44a71ebb5b))
  (fp_line (start -2.75 -1.5) (end -2.75 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c09ba683-ee09-471c-9d91-662a91c97c7c))
  (fp_line (start -2.4 -1.85) (end 2.4 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6885dc4-53fc-43aa-a300-aa5d7acc4ba6))
  (fp_line (start 2.4 1.85) (end -2.4 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85c23fad-d03e-4e91-a3ca-19b1adbc9751))
  (fp_line (start 2.75 1.5) (end 2.75 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0732a7d8-d7fb-4da3-bfcc-50c10a2fcb1c))
  (fp_arc (start -2.75 -1.5) (mid -2.647487 -1.747487) (end -2.4 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 427bc772-aa24-4fdb-97e9-6019b35f19aa))
  (fp_arc (start -2.4 1.85) (mid -2.647487 1.747487) (end -2.75 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 77f04694-6d30-4513-8b64-b7df80388ed8))
  (fp_arc (start 2.4 -1.85) (mid 2.647487 -1.747487) (end 2.75 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4d8612e9-f393-4677-a97f-926bb6eb816b))
  (fp_arc (start 2.75 1.5) (mid 2.647487 1.747487) (end 2.4 1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ba029bfa-a6a9-4f7e-8bb6-480942556e78))
  (fp_rect (start -2.35 -1.61) (end 2.35 1.61)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp c4d6b6d0-fec1-4be5-86e0-7492592637f8))
  (pad "1" smd custom (at -1.99 1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.6 -0.05)
          (xy -0.4 -0.25)
          (xy 0.6 -0.25)
          (xy 0.6 0.25)
          (xy -0.4 0.25)
          (xy -0.6 0.05)
        )
        (width 0) (fill yes))
      (gr_circle (center -0.4 -0.05) (end -0.2 -0.05) (width 0) (fill yes))
      (gr_circle (center -0.4 0.05) (end -0.2 0.05) (width 0) (fill yes))
    ) (tstamp 957a119b-bed6-4043-9175-a84a300d0b8e))
  (pad "2" smd custom (at -1.99 0.7) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.6 -0.05)
          (xy -0.4 -0.25)
          (xy 0.6 -0.25)
          (xy 0.6 0.25)
          (xy -0.4 0.25)
          (xy -0.6 0.05)
        )
        (width 0) (fill yes))
      (gr_circle (center -0.4 -0.05) (end -0.2 -0.05) (width 0) (fill yes))
      (gr_circle (center -0.4 0.05) (end -0.2 0.05) (width 0) (fill yes))
    ) (tstamp 64667e67-fa4f-43d0-848c-542047e14df4))
  (pad "3" smd custom (at -2.39 -1.35) (size 0.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.2 -0.25)
          (xy 0.23 0.25)
          (xy 0 0.25)
          (xy 0 -0.25)
        )
        (width 0) (fill yes))
      (gr_line (start -0.1 -0.15) (end -0.1 0.15) (width 0.2))
    ) (tstamp 034ea452-0d10-4511-a260-4fb71fd4ce9c))
  (pad "4" smd custom (at -1.55 -1.35) (size 0.1 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0 -0.25)
          (xy 0 0.25)
          (xy -0.15 0.25)
          (xy -0.28 -0.25)
        )
        (width 0) (fill yes))
      (gr_line (start 0.05 -0.15) (end 0.05 0.15) (width 0.2))
    ) (tstamp ff10c8ee-816a-4896-a975-8422d1b9a36d))
  (pad "5" smd custom (at 1.99 1.35 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.6 -0.05)
          (xy -0.4 -0.25)
          (xy 0.6 -0.25)
          (xy 0.6 0.25)
          (xy -0.4 0.25)
          (xy -0.6 0.05)
        )
        (width 0) (fill yes))
      (gr_circle (center -0.4 -0.05) (end -0.2 -0.05) (width 0) (fill yes))
      (gr_circle (center -0.4 0.05) (end -0.2 0.05) (width 0) (fill yes))
    ) (tstamp 6ff61c19-d0df-4f8d-ab83-e8988079f4fd))
  (pad "6" smd custom (at 1.99 -0.7 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.6 -0.05)
          (xy -0.4 -0.25)
          (xy 0.6 -0.25)
          (xy 0.6 0.25)
          (xy -0.4 0.25)
          (xy -0.6 0.05)
        )
        (width 0) (fill yes))
      (gr_circle (center -0.4 -0.05) (end -0.2 -0.05) (width 0) (fill yes))
      (gr_circle (center -0.4 0.05) (end -0.2 0.05) (width 0) (fill yes))
    ) (tstamp cef509b4-3125-4199-b28c-403d689e7e09))
  (pad "7" smd custom (at 1.99 -1.35 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.6 -0.05)
          (xy -0.4 -0.25)
          (xy 0.6 -0.25)
          (xy 0.6 0.25)
          (xy -0.4 0.25)
          (xy -0.6 0.05)
        )
        (width 0) (fill yes))
      (gr_circle (center -0.4 -0.05) (end -0.2 -0.05) (width 0) (fill yes))
      (gr_circle (center -0.4 0.05) (end -0.2 0.05) (width 0) (fill yes))
    ) (tstamp 0aa368db-8153-4c25-a58f-e0232a4831e9))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 444e422f-500c-47f5-a4ea-af41e34c8d5f) (name "No traces underneath") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -2.35 -1.1)
        (xy -1.4 -1.1)
        (xy -1.4 -1.6)
        (xy 1.39 -1.6)
        (xy 1.39 -0.45)
        (xy 2.35 -0.45)
        (xy 2.35 1.1)
        (xy 1.39 1.1)
        (xy 1.39 1.6)
        (xy -1.39 1.6)
        (xy -1.39 0.45)
        (xy -2.35 0.45)
      )
    )
  )
  (model "${KICAD7_3DMODEL_DIR}/Transformer_SMD.3dshapes/Wurth WE-STST 4532.stp"
    (offset (xyz 0 0 0.97))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
