(footprint "microSD_XKB_XKTF-015-x" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "DisplayModule.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Micro SD Card Socket with one card detection pin")
  (property "ki_keywords" "connector SD microsd")
  (attr smd)
  (fp_text reference "J4" (at 0 -16.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 262b8526-03eb-41e5-af1d-e63cd45bfb0b)
  )
  (fp_text value "Micro_SD_Card_Det1" (at 0 4.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 28f28603-1db1-4228-826e-ce5d16b7ff79)
  )
  (fp_text user "${REFERENCE}" (at 0 6.2 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 60ebf673-f2c8-442a-83d0-10f418a9d339)
  )
  (fp_line (start -7.65 0) (end 6.25 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 03d20190-5174-4304-a2ff-2d61cd843635))
  (fp_line (start -7.3 2.5) (end 5.35 2.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7fcfaeba-6348-42f2-99af-3c889f8a19a4))
  (pad "" np_thru_hole circle (at -4.95 -4) (size 1.2 1.2) (drill 1) (layers "F&B.Cu" "*.Mask") (tstamp 80408b86-27b6-4612-8533-c4269aa27d43))
  (pad "" np_thru_hole circle (at 3.05 -4) (size 1.2 1.2) (drill 1) (layers "F&B.Cu" "*.Mask") (tstamp 9a50d42d-cbeb-4382-be88-8c1fc641d804))
  (pad "1" smd roundrect (at 2.25 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp c1c91706-5467-4abe-960e-2f78ea9bd018))
  (pad "2" smd roundrect (at 1.15 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 673ede09-7bba-4821-a88d-82c7921f115b))
  (pad "3" smd roundrect (at 0.05 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 8cc97dab-c99e-4281-985c-31dd419ae9c9))
  (pad "4" smd roundrect (at -1.05 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 1f0e6190-bf31-40d7-9db8-52f1429b18bb))
  (pad "5" smd roundrect (at -2.15 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 75bf974f-a434-4aab-8e1e-80a74372aaad))
  (pad "6" smd roundrect (at -3.25 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 0f370e5d-a5c8-4479-9722-a6c9d0169edc))
  (pad "7" smd roundrect (at -4.35 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 5e04ae24-38af-4f82-ae7d-3c142d3f0eff))
  (pad "8" smd roundrect (at -5.45 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp 940ee49e-7b9c-4248-88b0-f1199c4d5d56))
  (pad "9" smd roundrect (at -6.55 -15) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1428571429) (tstamp aa217da0-b10f-478f-873e-750aefb81453))
  (pad "10" smd roundrect (at -7.75 -14) (size 1.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06666666667) (tstamp 3dff3efd-2d17-46b0-b984-8624fc12043b))
  (pad "10" smd roundrect (at -7.75 -4.4) (size 1.2 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06666666667) (tstamp acd0af30-6b2e-44b3-854c-1aae77a87b8d))
  (pad "10" smd roundrect (at 6.85 -14) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06666666667) (tstamp 3a86bc95-cf23-423b-b65a-a6f3882da01e))
  (pad "10" smd roundrect (at 7.75 -4.4) (size 1.2 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06666666667) (tstamp 9fdf7629-fd4d-4670-b1a3-be75259a97f7))
  (model ":KICAD7_3DMODEL_DIR:Connector_Card.3dshapes/xktf-015-x.stp"
    (offset (xyz 0 7.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
