(module "USB_A_PCB_traces_small" (layer "F.Cu") (tedit 5FB8AC27)
  (property "Description" "Not Populated")
  (property "Sheet file" "/home/stefan/Projects/Current/USBtoCANFD/USBtoCANFD.kicad_sch")
  (property "Sheet name" "")
  (attr exclude_from_pos_files)
  (fp_text reference "J1" (at 4.9 -5.2 180) (layer "F.SilkS") hide
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp 5976f3b6-7569-4545-a81e-d71365e7a234)
  )
  (fp_text value "HOST" (at 7.8 -5.2 180) (layer "F.SilkS") hide
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp 045829e5-b113-4bb7-a4f5-f64587bb385e)
  )
  (fp_text user "DN" (at 1.9 2.4) (layer "Cmts.User")
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp 3a36ea47-c222-4572-8fd4-6557b05a6e52)
  )
  (fp_text user "Front clearance" (at 0.4 0 90) (layer "Cmts.User")
    (effects (font (size 0.3 0.3) (thickness 0.05)))
    (tstamp 66f4f9b5-6579-48b9-bcb9-3b9123d9b384)
  )
  (fp_text user "+" (at 0.9 5.1) (layer "Cmts.User")
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp 66f9c200-e9e8-44aa-ad0e-fc9ed632ac8c)
  )
  (fp_text user "Insertion depth" (at 8.7 0 90) (layer "Cmts.User")
    (effects (font (size 0.3 0.3) (thickness 0.05)))
    (tstamp 7d8a85f9-f210-4fda-8e38-73ed2823ade8)
  )
  (fp_text user "-" (at 0.9 -5.2) (layer "Cmts.User")
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp a8dfe134-1773-4ce7-856b-0630fd059472)
  )
  (fp_text user "DP" (at 1.9 -2.4) (layer "Cmts.User")
    (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp d8456ee3-f14f-497d-b8d1-6081592a9a79)
  )
  (fp_line (start 0.6 -6.1) (end 0.6 6.1) (layer "Dwgs.User") (width 0.01) (tstamp bee7cf4e-cc50-40de-9841-08ea77448ac2))
  (fp_line (start 9 -6.1) (end 9 6.1) (layer "Dwgs.User") (width 0.01) (tstamp dcd90c58-36f3-4789-bf25-a73b06171dcd))
  (fp_line (start 11.5 8.5) (end 11.5 -8.5) (layer "Cmts.User") (width 0.1) (tstamp 924dded0-ffc3-4e5d-a1c0-a576fa3f925d))
  (fp_line (start 11.5 8.5) (end 12 8.5) (layer "Cmts.User") (width 0.1) (tstamp 9ee68bf4-afd8-4f45-9baa-57c9448be0ad))
  (fp_line (start 11.5 -8.5) (end 12 -8.5) (layer "Cmts.User") (width 0.1) (tstamp d1395f86-c2bc-49e1-8caa-425be42bd3c6))
  (fp_line (start 0 -6.1) (end 11.5 -6.1) (layer "F.CrtYd") (width 0.05) (tstamp 1426a354-3773-4df9-ae53-94722f9575e5))
  (fp_line (start 11.5 -6.1) (end 11.5 6.1) (layer "F.CrtYd") (width 0.05) (tstamp 8561acce-1ec4-4a93-8380-1e7a9c55739e))
  (fp_line (start 11.5 6.1) (end 0 6.1) (layer "F.CrtYd") (width 0.05) (tstamp 963ace61-5792-412b-90b4-1b5490b3559c))
  (fp_line (start 0 -6.1) (end 0 6.1) (layer "F.CrtYd") (width 0.05) (tstamp e7f64604-e8fc-44db-9f76-77604f31954c))
  (pad "1" connect roundrect (at 4.85 3.81) (size 8.5 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.067) (tstamp d8ea13f9-e436-4db9-93be-e65d174e1ad3))
  (pad "2" connect roundrect (at 5.225 1.27) (size 7.75 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.091) (tstamp b7ce7f92-8189-423c-96c7-fee7134078da))
  (pad "3" connect roundrect (at 5.225 -1.27) (size 7.75 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.091) (tstamp 0434fcc7-d30f-48a9-9965-645eaa378fd2))
  (pad "4" connect roundrect (at 4.85 -3.81) (size 8.5 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.067) (tstamp 20bb466b-d6ad-4a65-bc3d-99b919f1074f))
)
