(module JST_ZPD-32V-S (layer F.Cu) (tedit 539F4129)
  (attr smd)
  (fp_text reference P3 (at 0 1.25) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SCROBBY_HARNESS (at 0 -1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 1 (at -12.25 -4.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start 11.7 -3.9) (end 11.7 -2.65) (layer F.SilkS) (width 0.127))
  (fp_line (start -11.7 -3.9) (end -11.7 -2.65) (layer F.SilkS) (width 0.127))
  (fp_line (start -11.7 -2.65) (end 11.7 -2.65) (layer F.SilkS) (width 0.127))
  (fp_line (start -13.85 3.5) (end 13.85 3.5) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.85 -3.9) (end 13.85 3.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -13.85 -3.9) (end -13.85 3.5) (layer F.SilkS) (width 0.127))
  (fp_line (start -13.85 -3.9) (end 13.85 -3.9) (layer F.SilkS) (width 0.127))
  (pad 1 smd oval (at -11.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -11.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -9.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -9.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -8.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -8.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -6.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at -6.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at -5.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at -5.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at -3.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at -3.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at -2.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at -2.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at -0.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at -0.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 0.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 0.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 2.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at 2.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at 3.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at 3.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at 5.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at 5.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd oval (at 6.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd oval (at 6.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd oval (at 8.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd oval (at 8.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd oval (at -13.35 -2) (size 0.7 3.2) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd oval (at 13.35 -2) (size 0.7 3.2) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd oval (at 9.75 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd oval (at 9.75 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd oval (at 11.25 -3.25) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd oval (at 11.25 4) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask))
  (model "3D/SH/jst zpd bm32b-zpdss-tf.wrl"
    (at (xyz -0.4865 0.105 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 270 0 180))
  )
)
