(module HopeRF_RFM98W_Castellated (layer F.Cu) (tedit 56EB39F8)
  (fp_text reference A2 (at -2.5 -7.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value HopeRF_RFM98W (at -4.25 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8 8) (end -8 -8) (layer F.Fab) (width 0.05))
  (fp_line (start 8 8) (end -8 8) (layer F.Fab) (width 0.05))
  (fp_line (start 8 -8) (end 8 8) (layer F.Fab) (width 0.05))
  (fp_line (start -8 -8) (end 8 -8) (layer F.Fab) (width 0.05))
  (fp_text user 1 (at -5.25 -7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user ANT (at 4.5 7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -7.75 8) (end -6.5 8) (layer F.SilkS) (width 0.125))
  (fp_line (start 6.5 -8) (end 7.75 -8) (layer F.SilkS) (width 0.125))
  (fp_line (start -7.75 -8) (end -6.5 -8) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.75 -8.5) (end 8.75 8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.75 8.5) (end -8.75 8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.75 8.5) (end -8.75 -8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.75 -8.5) (end 8.75 -8.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.5 8) (end 7.75 8) (layer F.SilkS) (width 0.125))
  (pad 1 thru_hole circle (at -8 -7) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 smd oval (at -7.375 -5) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 3 smd oval (at -7.375 -3) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 4 smd oval (at -7.375 -1) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 5 smd oval (at -7.375 1) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 6 smd oval (at -7.375 3) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 7 smd oval (at -7.375 5) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 8 smd oval (at -7.375 7) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 9 smd oval (at 7.375 7) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 10 smd oval (at 7.375 5) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 11 smd oval (at 7.375 3) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 12 smd oval (at 7.375 1) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 13 smd oval (at 7.375 -1) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 14 smd oval (at 7.375 -3) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 15 smd oval (at 7.375 -5) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 16 smd oval (at 7.375 -7) (size 2.75 1.5) (layers F.Cu F.Mask))
  (pad 2 thru_hole circle (at -8 -5) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -8 -3) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -8 -1) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -8 1) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -8 3) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -8 5) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -8 7) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 8 7) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 8 5) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 8 3) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 8 1) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 8 -1) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 8 -3) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 8 -5) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 8 -7) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 smd oval (at -7.375 -7) (size 2.75 1.5) (layers F.Cu F.Mask))
  (model 3D/walter/rf_modules/RFM9X_W.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
