(footprint "JST_GH_SM10B-GHS-TB_1x10-1MP_P1.25mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST GH series connector, SM10B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST GH top entry")
  (property "Sheetfile" "G4ESC.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J9" (at 0 -3.9 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 18e6afb9-686b-48c1-9a72-8399811983f4)
  )
  (fp_text value "CAN & PWM" (at 0 3.9 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6ee20737-750a-45db-8abc-39c9d24a9a8a)
  )
  (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e82b5390-1914-4b68-baa6-d3841a3037bb)
  )
  (fp_line (start -7.985 -1.71) (end -6.185 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee88a0ae-5532-4778-8db8-a7f1f91f0cfa))
  (fp_line (start -7.985 -0.26) (end -7.985 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 221b0554-d396-4bdf-801e-ac96af26d03d))
  (fp_line (start -6.715 2.56) (end 6.715 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e457242-e2fd-4f19-aa3d-6686d02a1090))
  (fp_line (start -6.185 -1.71) (end -6.185 -2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6055fa35-67e8-4e85-9032-e9ba62db90bd))
  (fp_line (start 7.985 -1.71) (end 6.185 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be4edb59-b553-4101-997d-5081cc81ec51))
  (fp_line (start 7.985 -0.26) (end 7.985 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f8f8a9d-62e2-4aab-81a9-70aacdf92f53))
  (fp_line (start -8.15 -1.6) (end -8.15 2.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8bd78dc3-32cd-42da-8057-3d702ec0440c))
  (fp_line (start -7.9 -1.85) (end -6.1 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ccedcd63-18d5-4055-be9f-6be0ec14144f))
  (fp_line (start -6.1 -1.85) (end -6.1 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1cb318da-d5f7-4b11-a550-3a5b19177565))
  (fp_line (start -5.8 -2.85) (end 5.8 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dd914e9a-4097-4aad-a5b2-d924a132c53f))
  (fp_line (start 6.1 -1.85) (end 6.1 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2f56f0eb-5c55-4555-918c-b3bee505667b))
  (fp_line (start 7.8 2.85) (end -7.8 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0e55e4a6-4627-4fe5-a0b7-704b5ea50124))
  (fp_line (start 7.9 -1.85) (end 6.1 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp aabb3d51-7292-4012-9b8b-ebe7eb3487d4))
  (fp_line (start 8.15 -1.6) (end 8.15 2.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 79560427-e729-4b7f-a065-c459b61876c9))
  (fp_arc (start -8.15 -1.6) (mid -8.076777 -1.776777) (end -7.9 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c16227cd-52d8-42b0-aae6-c8790a42809b))
  (fp_arc (start -7.8 2.85) (mid -8.047487 2.747487) (end -8.15 2.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2acefc70-1303-4e56-ad8e-11a18cc6740c))
  (fp_arc (start -6.1 -2.55) (mid -6.012132 -2.762132) (end -5.8 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 968239f2-914c-40fc-9551-ad6cffc8a1d6))
  (fp_arc (start 5.8 -2.85) (mid 6.012132 -2.762132) (end 6.1 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 043321bf-bc34-4103-8f99-6321e4379f72))
  (fp_arc (start 7.9 -1.85) (mid 8.076777 -1.776777) (end 8.15 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1bc77214-8370-425c-a1db-334f7bb8e4cc))
  (fp_arc (start 8.15 2.5) (mid 8.047487 2.747487) (end 7.8 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d419a9e0-20ed-415e-8407-d47502867294))
  (fp_line (start -7.875 -1.6) (end -7.875 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d63d735-d900-4fdd-b620-b423b696c86a))
  (fp_line (start -7.875 -1.6) (end 7.875 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d4ad1be6-7e9e-4fd8-9af0-11546a9992bc))
  (fp_line (start -7.875 2.45) (end 7.875 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fcb1465c-ef48-4f07-8ffd-32e6a99ca0ed))
  (fp_line (start -6.125 -1.6) (end -5.625 -0.892893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 23af9973-5022-4daf-bb7b-d96c8e613176))
  (fp_line (start -5.625 -0.892893) (end -5.125 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f79d40b3-3812-4650-916e-08a8a6ba8d53))
  (fp_line (start 7.875 -1.6) (end 7.875 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b280f1b-fce6-4726-af5f-21711bbd1f04))
  (pad "1" smd roundrect (at -5.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6e53750a-1ba1-4a1a-bb1d-64b2213a4c7f))
  (pad "2" smd roundrect (at -4.375 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 527006ff-0e39-4a34-9409-ceeaa99baa59))
  (pad "3" smd roundrect (at -3.125 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 73c1489a-90ab-46a1-82ed-c0dee8435a3f))
  (pad "4" smd roundrect (at -1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 35dd122b-0a51-4e92-9739-e7a85bcb000d))
  (pad "5" smd roundrect (at -0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 24303e26-d4b1-4df3-8537-4978dd858f7a))
  (pad "6" smd roundrect (at 0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d117c099-797d-4e8f-86c2-cd296dc36c2a))
  (pad "7" smd roundrect (at 1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp beca2e31-1056-4e91-95f4-8f9755238373))
  (pad "8" smd roundrect (at 3.125 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 41885cff-3008-4460-8971-2ecaa39139a6))
  (pad "9" smd roundrect (at 4.375 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp be2e6b7a-aeab-4379-9f91-09e32046da42))
  (pad "10" smd roundrect (at 5.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b647de36-a5da-4d88-9cc9-9ee80a6cf847))
  (pad "MP" smd roundrect (at -7.475 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15) (tstamp 6237fa78-6d2d-4e70-9bd4-5f529d6380eb))
  (pad "MP" smd roundrect (at 7.475 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15) (tstamp da581595-bc3f-460e-815c-be586674548d))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_SM10B-GHS-TB_1x10-1MP_P1.25mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
