(footprint "FPC_Pads_15P_P1.0" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "CameraCable.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x15, script generated")
  (property "ki_keywords" "connector")
  (attr exclude_from_pos_files)
  (fp_text reference "J2" (at -7.4 4.15 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp 2de8f433-2c2a-4f0d-a398-9c9ff5c4beb2)
  )
  (fp_text value "RPI" (at 0 -0.9 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2002dfaa-b0f8-43cc-b9e7-dddee7eead5d)
  )
  (fp_text user "STIFFENER BOARD" (at 3.8 4.4 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp 04f4a426-e50c-4cf9-8eb8-b979017abc25)
  )
  (fp_text user "${REF}" (at 0 -2.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fd61e61b-e54a-4e16-96dd-6df785c49948)
  )
  (fp_poly
    (pts
      (xy 7.2 3.65)
      (xy 6.8 3.65)
      (xy 7 3.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a43d1212-f48a-46a8-a6be-ce8842b53fa3))
  (fp_rect (start -8 0) (end 8 5)
    (stroke (width 0.05) (type solid)) (fill none) (layer "Dwgs.User") (tstamp 7b8613f6-2ef1-408f-9dc5-41b4314bbb1e))
  (pad "1" connect roundrect (at 7 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 100e24a4-2d28-4040-8c1a-4ba64507391e))
  (pad "2" connect roundrect (at 6 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp eb6cd7e9-6a9c-446b-a164-33799d6e1bdf))
  (pad "3" connect roundrect (at 5 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp ad2278e0-7ce7-42dc-952e-d7c6ed4088d7))
  (pad "4" connect roundrect (at 4 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 4e9ee56e-e4d1-4a70-8ca6-5f6b65542452))
  (pad "5" connect roundrect (at 3 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 3057af66-1b6e-47e8-9f29-67dc883e6b3d))
  (pad "6" connect roundrect (at 2 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp e03f04ba-048a-473a-af3a-be8441b7a190))
  (pad "7" connect roundrect (at 1 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 8f0eb4ff-6891-4ded-a116-fe27b79ae429))
  (pad "8" connect roundrect (at 0 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 4c259ff5-c84c-4644-b090-1cd25aad6d2e))
  (pad "9" connect roundrect (at -1 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp f13d1f3a-e8ab-4ee5-8db6-cb276a9c670d))
  (pad "10" connect roundrect (at -2 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp b907e177-6046-4441-8b43-3ee45ce5bbcb))
  (pad "11" connect roundrect (at -3 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp dd3c227f-1657-4436-98ce-2580b7174ecf))
  (pad "12" connect roundrect (at -4 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 941a4496-81f5-46a4-86a4-579c9e5d51e4))
  (pad "13" connect roundrect (at -5 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 5b9ab8fd-21da-41f3-9e0b-9a3fc7e02e37))
  (pad "14" connect roundrect (at -6 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 7fb44bec-89ec-4aad-8498-8034188424c6))
  (pad "15" connect roundrect (at -7 1.6) (size 0.7 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.01) (chamfer top_left top_right) (tstamp 63ffeba6-8540-4086-b271-59aa84184278))
)
