(footprint "Plain_Hole_3.4mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (solder_mask_margin 0.075)
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -0.5) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp eec1c2bf-0540-454f-8403-e43b39fe92d5)
  )
  (fp_text value "Plain_Hole_4mm" (at 0 0.5) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp e9786748-1827-418e-912d-0c6d6c8b19ae)
  )
  (pad "" np_thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3.4) (layers "F&B.Cu" "*.Mask") (tstamp 63716510-52d7-4414-925f-894505377204))
)
