(module Pulse_PA4344.XXXNLT (layer F.Cu) (tedit 5BDDB42A)
  (solder_mask_margin -0.001)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference L1 (at -9.5 -9) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value PA4344.333NLT (at 0 -5.5) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_line (start -8.6 -8.6) (end -8.6 8.6) (layer F.Fab) (width 0.05))
  (fp_line (start -8.6 8.6) (end 8.6 8.6) (layer F.Fab) (width 0.05))
  (fp_line (start 8.6 8.6) (end 8.6 -8.6) (layer F.Fab) (width 0.05))
  (fp_line (start 8.6 -8.6) (end -8.6 -8.6) (layer F.Fab) (width 0.05))
  (fp_line (start -8.6 -8.6) (end -8.6 -8.6) (layer F.Fab) (width 0.05))
  (fp_line (start -5.95 -8.6) (end -5.95 -8.85) (layer F.Fab) (width 0.05))
  (fp_line (start -5.95 -8.85) (end 5.95 -8.85) (layer F.Fab) (width 0.05))
  (fp_line (start 5.95 -8.85) (end 5.95 -8.6) (layer F.Fab) (width 0.05))
  (fp_line (start 5.95 -8.6) (end 5.95 -8.6) (layer F.Fab) (width 0.05))
  (fp_line (start -5.95 8.6) (end -5.95 8.85) (layer F.Fab) (width 0.05))
  (fp_line (start -5.95 8.85) (end 5.95 8.85) (layer F.Fab) (width 0.05))
  (fp_line (start 5.95 8.85) (end 5.95 8.6) (layer F.Fab) (width 0.05))
  (fp_line (start 5.95 8.6) (end 5.95 8.6) (layer F.Fab) (width 0.05))
  (fp_line (start -8.85 -8.85) (end -8.85 -7.85) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.85 -8.85) (end -7.85 -8.85) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.85 8.85) (end -8.85 7.85) (layer F.SilkS) (width 0.125))
  (fp_line (start -8.85 8.85) (end -7.85 8.85) (layer F.SilkS) (width 0.125))
  (fp_line (start 7.85 8.85) (end 8.85 8.85) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.85 8.85) (end 8.85 7.85) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.85 -8.85) (end 8.85 -7.85) (layer F.SilkS) (width 0.125))
  (fp_line (start 8.85 -8.85) (end 7.85 -8.85) (layer F.SilkS) (width 0.125))
  (pad 1 smd roundrect (at 0 -7.675) (size 12.5 3.15) (layers F.Cu F.Mask) (roundrect_rratio 0.079))
  (pad 2 smd roundrect (at 0 7.675) (size 12.5 3.15) (layers F.Cu F.Mask) (roundrect_rratio 0.079))
  (pad 1 smd roundrect (at -5.25 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -5.25 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at -3.15 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at -1.05 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 1.05 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 3.15 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 5.25 -8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at -5.25 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at -3.15 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at -1.05 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 1.05 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 3.15 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 1 smd roundrect (at 5.25 -6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -3.15 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -1.05 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 1.05 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 3.15 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 5.25 8.5) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -5.25 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -3.15 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at -1.05 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 1.05 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 3.15 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (pad 2 smd roundrect (at 5.25 6.8) (size 1.8 1.4) (layers F.Paste) (roundrect_rratio 0.107))
  (model ${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/Pulse_PA4344NLT.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
