(footprint "UCBGA-36_2.5x2.5mm_Layout6x6_P0.4mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "UCBGA-36, 6x6 raster, 2.5x2.5mm package, pitch 0.4mm; https://www.latticesemi.com/view_document?document_id=213")
  (tags "BGA 36 0.4")
  (property "LCSC" "C3656650")
  (property "MFG" "TI")
  (property "MPN" "TMUX646ZECR")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.035)
  (solder_paste_margin 0.000001)
  (attr smd)
  (fp_text reference "U1" (at 0 -2.25 180) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 21181613-2e08-43b9-b372-b4e36fd69ebb)
  )
  (fp_text value "TI_TMUX646_C-PHY" (at 0.1 2.45 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eb26396c-5a1e-4ca7-a95d-ce19928653e5)
  )
  (fp_text user "INPUT" (at 1 0.2 90 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold) (justify bottom))
    (tstamp 74eca50d-c1f6-4682-a9ff-bd95171154c9)
  )
  (fp_text user "OUTPUT A" (at 0.2 0 90 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold) (justify bottom))
    (tstamp 7e238fe9-0c82-4f60-8046-e2dd5feed235)
  )
  (fp_text user "OUTPUT B" (at -0.6 0.2 90 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold) (justify bottom))
    (tstamp 91876352-d2a8-46cb-aae6-7b189aeb09cb)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.8 180) (layer "F.Fab")
      (effects (font (size 0.58 0.58) (thickness 0.087)))
    (tstamp 9ca09727-8c3a-4f19-9d22-2c759f156bd3)
  )
  (fp_line (start -1.36 1.36) (end -1.36 -0.735)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2103998d-52fc-4b46-95e3-ae35b79dd131))
  (fp_line (start -0.735 -1.36) (end 1.36 -1.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ced39f20-fef0-44f5-8e3f-f8c5f5e54fa8))
  (fp_line (start 1.36 -1.36) (end 1.36 1.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a13200ef-f7b1-4adc-8bac-81b30c0fb71c))
  (fp_line (start 1.36 1.36) (end -1.36 1.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 79fa8ae7-4b6e-441f-bc41-2ef2a240bfea))
  (fp_line (start -0.4 -0.8) (end -1.2 -0.8)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 5bf1eb08-b5b0-4f19-a9ce-be49d57b9a2d))
  (fp_line (start -0.4 -0.8) (end -0.4 -1.2)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp c6f16076-ad29-4fdd-95ad-54118fb7b1a8))
  (fp_line (start -0.4 -0.4) (end 0.4 0)
    (stroke (width 0.05) (type dash)) (layer "Dwgs.User") (tstamp 0503bb56-b7ea-4ae4-ae2f-3aac4769632e))
  (fp_line (start -0.4 0) (end 0.4 -0.4)
    (stroke (width 0.05) (type dash)) (layer "Dwgs.User") (tstamp daa5e57c-ab2f-4272-a08d-c0a76059b7de))
  (fp_line (start -0.4 1.2) (end -0.4 -0.8)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 38703c3d-76f2-4b8c-9d5f-7645170d0817))
  (fp_line (start 0.4 -0.8) (end 0.4 -1.2)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 6239bbb0-214c-4d33-9239-d263976ca434))
  (fp_line (start 0.4 -0.8) (end 0.4 1.2)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp f51227cf-cfcd-444f-8204-3c1ed5fb3ea6))
  (fp_line (start 1.2 -0.8) (end 0.4 -0.8)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 5ddc78dd-e19c-47a1-b848-cf42f2069e9e))
  (fp_line (start -2.25 -1.25) (end -2.25 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f495c1b9-1bad-43ad-a34c-396033e1be77))
  (fp_line (start -1.25 2.25) (end 1.25 2.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62c5753a-df58-4749-8d56-a35192871302))
  (fp_line (start 1.25 -2.25) (end -1.25 -2.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d6b75027-2e67-4fcf-9e6b-07f22d129129))
  (fp_line (start 2.25 1.25) (end 2.25 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25436f18-f8c3-4a5d-bbbe-6e9eb8b59740))
  (fp_arc (start -2.25 -1.25) (mid -1.957107 -1.957107) (end -1.25 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 72a5a970-31a0-48e8-ab40-ac0166ac70ea))
  (fp_arc (start -1.25 2.25) (mid -1.957107 1.957107) (end -2.25 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4ca8c587-e616-4141-96c8-29886f734299))
  (fp_arc (start 1.25 -2.25) (mid 1.957107 -1.957107) (end 2.25 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4e9b1538-0f6f-4003-84aa-5cbfbd282852))
  (fp_arc (start 2.25 1.25) (mid 1.957107 1.957107) (end 1.25 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 388b13b0-1fdf-4b8a-9abd-7886e94bab32))
  (fp_line (start -1.25 -1.25) (end 1.25 -1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 30e560aa-4396-4ecc-83e0-36b0cdc9f9ef))
  (fp_line (start -1.25 -0.625) (end -0.625 -1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5123af53-eefa-4bf5-92ec-d013aa8c1e5e))
  (fp_line (start -1.25 1.25) (end -1.25 -1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa118c07-1edb-4b61-a2e8-5f9566f928c5))
  (fp_line (start 1.25 -1.25) (end 1.25 1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp acbbb8f9-e59d-4cb7-92bf-cc1a859c101e))
  (fp_line (start 1.25 1.25) (end -1.25 1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1ae0f15-a40f-424f-8f5c-5677f7ebac1c))
  (pad "A1" smd circle (at -1 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 34f052e4-f87c-4d47-82c0-4b7d741bd199))
  (pad "A2" smd circle (at -0.6 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6aa96bc9-0f5b-4578-ba5d-1c3ebf475d4f))
  (pad "A3" smd circle (at -0.2 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 221484c1-331c-4675-8d42-3ad9802b08f8))
  (pad "A4" smd circle (at 0.2 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8c825a53-256d-483d-94d0-4171acd95e30))
  (pad "A5" smd circle (at 0.6 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 583cec77-9397-4ee3-b5cc-d702d2ddba03))
  (pad "A6" smd circle (at 1 -1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 61714cff-5cc6-434c-84ef-2387c1bb8dbc))
  (pad "B1" smd circle (at -1 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3803a4db-e860-40a8-948d-bb55bd354d89))
  (pad "B2" smd circle (at -0.6 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4c16d1ab-5c26-4f80-88c8-237bbb233757))
  (pad "B3" smd circle (at -0.2 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f440bac6-5392-4a03-b991-f85840b0cb25))
  (pad "B4" smd circle (at 0.2 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 43604da5-ce96-4b8c-bb24-bde7bdc3a08f))
  (pad "B5" smd circle (at 0.6 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e9598824-9cec-4b63-882b-0184eface2ac))
  (pad "B6" smd circle (at 1 -0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp da9dcad6-0ad6-4499-bd67-293dcc36771a))
  (pad "C1" smd circle (at -1 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 940ce755-2d29-4a29-89aa-e1d032e20bb5))
  (pad "C2" smd circle (at -0.6 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 254cf3bc-17e2-48f7-9c8e-93f3864a9e5f))
  (pad "C3" smd circle (at -0.2 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fd19a204-63a3-419d-8d16-fb36bb641554))
  (pad "C4" smd circle (at 0.2 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0d9c495b-e27b-4ee2-9b7b-32f85e558a89))
  (pad "C5" smd circle (at 0.6 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 09d8a382-efb0-4115-bb8e-c27c7fd7b2d3))
  (pad "C6" smd circle (at 1 -0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a123a620-cd95-449b-bf41-daec27e58e70))
  (pad "D1" smd circle (at -1 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e8bd28c0-86e0-4d34-a8af-7770078dc240))
  (pad "D2" smd circle (at -0.6 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp dcb2ef8f-fd13-4d53-bcfa-4d7caaefeaea))
  (pad "D3" smd circle (at -0.2 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 38158259-1389-468f-aa82-e37f399f35a2))
  (pad "D4" smd circle (at 0.2 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 33ab86e2-541e-4367-8e5e-9473e4d68149))
  (pad "D5" smd circle (at 0.6 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3fa80e6d-c825-49a4-8b32-6c1b165c0d4c))
  (pad "D6" smd circle (at 1 0.2) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 23c88b97-64a7-41f8-a456-ad75953eb64d))
  (pad "E1" smd circle (at -1 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0bfa7c4a-ef22-4eb6-925c-6fcabac8a666))
  (pad "E2" smd circle (at -0.6 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp acb3541b-4957-4a1a-ace3-fca0bc66fd5a))
  (pad "E3" smd circle (at -0.2 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a6dfe602-770e-47e6-87a0-5e800f4e5326))
  (pad "E4" smd circle (at 0.2 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 50158daa-d6bb-4414-ad47-70713ab2b6b3))
  (pad "E5" smd circle (at 0.6 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bcaf6655-52a9-4a6a-a233-85e8bb34f9fa))
  (pad "E6" smd circle (at 1 0.6) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2f027494-f48c-4db1-b231-d95250e5a62f))
  (pad "F1" smd circle (at -1 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d8069c6c-c080-48a1-8194-bff68b06f9af))
  (pad "F2" smd circle (at -0.6 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ec82de98-8972-4ff5-a07b-57e840e858c2))
  (pad "F3" smd circle (at -0.2 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9585da7a-4e9f-4729-926e-c684e18edea1))
  (pad "F4" smd circle (at 0.2 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d021cbd2-4551-49cb-a1df-8e3920586863))
  (pad "F5" smd circle (at 0.6 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bd58a7dd-82ec-4dd8-ac51-8c8bc7dfcabf))
  (pad "F6" smd circle (at 1 1) (size 0.27 0.27) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ea276c5c-7c12-425c-8d4a-698c811c48ef))
  (model ":KICAD7_3DMODEL_DIR:Package_BGA.3dshapes/ucBGA-36_2.5x2.5mm_Layout6x6_P0.4mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
