(footprint "VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.35 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 3aac7023-b850-4ae0-a159-1c723504f4d0)
  )
  (fp_text value "VSON-8-1EP_3x3mm_P0.65mm_EP1.65x2.4mm" (at 0 1.95 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp f7baf291-904f-4a6f-94b6-5104accd0fb2)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.95 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 8af2afb3-3d7c-45c1-ae80-3eb01654ce7d)
  )
  (fp_arc (start -1.675 -1.6) (mid -1.653033 -1.653033) (end -1.6 -1.675)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp ce1dbedf-831c-4982-b18a-73ef32f7a93b))
  (fp_arc (start -1.6 1.675) (mid -1.653033 1.653033) (end -1.675 1.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 37bc842c-79ea-4aab-b3e3-50bcbe51b45e))
  (fp_arc (start 1.6 -1.675) (mid 1.653033 -1.653033) (end 1.675 -1.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 9fc0473e-de23-428f-9761-d817ace637b4))
  (fp_arc (start 1.675 1.6) (mid 1.653033 1.653033) (end 1.6 1.675)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 11b2977e-8228-4f3d-8dd2-f80b7dfa4681))
  (fp_poly
    (pts
      (xy -1.8 -1)
      (xy -2 -1.15)
      (xy -2 -0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp bd882ac0-9cdc-4b6b-9e31-97f4cf8e2e6b))
  (fp_poly
    (pts
      (xy -1.6 -1.25)
      (xy -1.6 -1.6)
      (xy -0.8 -1.6)
      (xy -0.8 -1.75)
      (xy -1.6 -1.75)
      (xy -1.75 -1.6)
      (xy -1.75 -1.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7591f8fe-6be4-49df-ab87-b7425606e7c0))
  (fp_poly
    (pts
      (xy -1.6 1.25)
      (xy -1.6 1.6)
      (xy -0.8 1.6)
      (xy -0.8 1.75)
      (xy -1.6 1.75)
      (xy -1.75 1.6)
      (xy -1.75 1.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 00c9b8b4-3731-4be1-a2fc-5614d87ca11f))
  (fp_poly
    (pts
      (xy 1.6 -1.25)
      (xy 1.6 -1.6)
      (xy 0.8 -1.6)
      (xy 0.8 -1.75)
      (xy 1.6 -1.75)
      (xy 1.75 -1.6)
      (xy 1.75 -1.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp c2f86ef7-f2d3-445c-92dd-4c53915aa7f0))
  (fp_poly
    (pts
      (xy 1.6 1.25)
      (xy 1.6 1.6)
      (xy 0.8 1.6)
      (xy 0.8 1.75)
      (xy 1.6 1.75)
      (xy 1.75 1.6)
      (xy 1.75 1.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6cdfb0f4-5666-44dd-b0eb-80fce70deea5))
  (fp_line (start -1.85 -1.05) (end -1.85 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 579f3e5c-5a6c-4b43-ab51-a22ae0efd0ed))
  (fp_line (start -1.75 -1.5) (end -1.75 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc659f04-39fc-4911-83bc-80ff17130a47))
  (fp_line (start -1.75 1.25) (end -1.75 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 18b61e46-554e-495e-a3d2-06b145f0aeab))
  (fp_line (start -1.5 1.75) (end 1.5 1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 79c48bff-1ab4-4b69-a73c-209f26b227ae))
  (fp_line (start 1.5 -1.75) (end -1.5 -1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7bf57170-d1fa-432b-9c13-3bd447d9c181))
  (fp_line (start 1.75 -1.5) (end 1.75 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc3a899a-6868-448a-8968-9eb1400cb390))
  (fp_line (start 1.75 1.25) (end 1.75 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 468c19d3-e0ff-459f-ac80-d30f3d986d89))
  (fp_line (start 1.85 1.05) (end 1.85 -1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 01fcb5f0-aa30-4c4f-8c6a-b4816f56e5b2))
  (fp_arc (start -1.85 -1.05) (mid -1.823607 -1.161803) (end -1.75 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3060f254-c421-498f-a925-434500f04eec))
  (fp_arc (start -1.75 -1.5) (mid -1.676777 -1.676777) (end -1.5 -1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6dce3de9-fca8-4c6c-956a-979fa8ba5644))
  (fp_arc (start -1.75 1.25) (mid -1.823607 1.161803) (end -1.85 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 05e52278-8430-408f-9869-67cda3f58278))
  (fp_arc (start -1.5 1.75) (mid -1.676777 1.676777) (end -1.75 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 10e592ee-35a5-4925-b463-ba2b3fd33e06))
  (fp_arc (start 1.5 -1.75) (mid 1.676777 -1.676777) (end 1.75 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d8eeb14f-1e5c-4129-b56f-0c3cc8a26818))
  (fp_arc (start 1.75 -1.25) (mid 1.823607 -1.161803) (end 1.85 -1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ae12b830-6421-4367-8fae-64727a5a0b3a))
  (fp_arc (start 1.75 1.5) (mid 1.676777 1.676777) (end 1.5 1.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 25381cc3-9ca2-4591-93b1-64facbce82ac))
  (fp_arc (start 1.85 1.05) (mid 1.823607 1.161803) (end 1.75 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 52477403-e099-4adf-bcc2-6e66533c95c4))
  (fp_rect (start -1.5 -1.5) (end 1.5 1.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 1a9dd4ed-1d77-4ca5-9444-617cd4b52b12))
  (pad "" smd oval (at -1.4 -0.975) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f1c8dbe2-2546-41c7-a08d-3883ecc27368))
  (pad "" smd oval (at -1.4 -0.325) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b57c40da-39a5-45cd-9eb4-611c583b902e))
  (pad "" smd oval (at -1.4 0.325) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9e0418a8-075f-4a85-bf49-e191fc345b67))
  (pad "" smd oval (at -1.4 0.975) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp bdee8b9b-6f81-4377-a276-b7e6006d83b1))
  (pad "" smd roundrect (at -0.475 -0.875) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp 1ebfb1b3-ce97-45d1-949c-a5864243b9d1))
  (pad "" smd roundrect (at -0.475 0) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp 15b94b70-e20c-4c7f-994a-3fd355f935d8))
  (pad "" smd roundrect (at -0.475 0.875) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp 08182c72-0607-43f7-afc7-92f492b85209))
  (pad "" smd roundrect (at 0.475 -0.875) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp 6ba9e647-a20f-4ce9-b6ef-03777eaa4011))
  (pad "" smd roundrect (at 0.475 0) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp f4ccecfc-631a-499d-a80b-07e7ff97ee7b))
  (pad "" smd roundrect (at 0.475 0.875) (size 0.7 0.65) (layers "F.Paste") (roundrect_rratio 0.2307692308)
    (thermal_bridge_angle 45) (tstamp 0c2472ab-9f92-4378-9ead-3665b77963ef))
  (pad "" smd oval (at 1.4 -0.975) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ededbf2b-f8ec-4478-a472-61ba39529a6c))
  (pad "" smd oval (at 1.4 -0.325) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 386ad528-39e8-42bc-a09d-d62a76bb84f7))
  (pad "" smd oval (at 1.4 0.325) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4375dc69-68fd-4f40-b599-d46201544902))
  (pad "" smd oval (at 1.4 0.975) (size 0.5 0.25) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2372b828-34b1-40fe-b3a3-e149d17763a7))
  (pad "1" smd roundrect (at -1.4 -0.975) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp 39159fff-2bc8-436c-b39b-f1a221cbe4c8))
  (pad "2" smd roundrect (at -1.4 -0.325) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp 91a237de-ac71-46a4-b87c-0ee9081531e2))
  (pad "3" smd roundrect (at -1.4 0.325) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp 93f864dd-4513-4cd1-8624-d4a626c2276c))
  (pad "4" smd roundrect (at -1.4 0.975) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp 57fb8033-3bc2-45c5-b2dc-d8a605164d1d))
  (pad "5" smd roundrect (at 1.4 0.975 180) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp 29463405-254c-414f-a998-e881e1f75e59))
  (pad "6" smd roundrect (at 1.4 0.325 180) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp c46d2601-3c2f-40f4-8e5c-8d435198906e))
  (pad "7" smd roundrect (at 1.4 -0.325 180) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp dbd85900-c744-422c-9950-26d323d99da5))
  (pad "8" smd roundrect (at 1.4 -0.975 180) (size 0.6 0.31) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right)
    (thermal_bridge_angle 45) (tstamp e25ba3ff-6db9-46f6-867b-6642c9fd5b11))
  (pad "9" smd roundrect (at 0 0) (size 1.65 2.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.06060606061)
    (thermal_bridge_angle 45) (tstamp db38520e-dc51-4c4c-bedb-9da321c5982f))
)
