(footprint "SolderJumper-2_1.2x1.2mm_Open_Rounded"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
	(tags "net tie solder jumper bridged")
	(property "Reference" "JP24"
		(at 0 -1.8 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "0a5dfecd-8259-4c42-b412-515d8b9824f1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "IMU-OIS_SDA"
		(at 0 1.9 180)
		(layer "F.Fab")
		(uuid "e445a6bf-6892-4064-851c-60d3840aa1ae")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Jumper:SolderJumper-2_1.2x1.2mm_Open_Rounded"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c3e7c30a-9969-4107-9274-5aee8d0cf9f1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4d4cd858-38a2-4255-b426-1082b5e3ca1a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, open"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e532b229-7a8c-421d-b63a-9040a134495e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4c75dfa0-3699-42c5-86f4-8f3cb4b5715c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(net_tie_pad_groups "1, 2")
	(fp_line
		(start -0.9 0.3)
		(end -0.9 -0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5801d0c5-e8b0-47bf-8dd0-c1e604d0f438")
	)
	(fp_line
		(start 0.9 -0.3)
		(end 0.9 0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d7d3a377-5360-4487-94ba-441ec25c675d")
	)
	(fp_rect
		(start -0.4 -0.875)
		(end -0.125 -0.725)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "6011076d-c6fe-4c60-9af9-e4d1f10f560e")
	)
	(fp_rect
		(start -0.4 0.725)
		(end -0.125 0.875)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "1a77a9a0-5108-4ac4-a77d-e2a665f9e394")
	)
	(fp_rect
		(start 0.125 -0.875)
		(end 0.4 -0.725)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "a75ffb66-ee26-4dac-8f06-3e21a2d00d29")
	)
	(fp_rect
		(start 0.125 0.725)
		(end 0.4 0.875)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bb31a1fa-a26d-496a-be4e-c04a4c99bf0d")
	)
	(fp_arc
		(start -0.9 -0.3)
		(mid -0.753553 -0.653553)
		(end -0.4 -0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bb44eec0-fc86-43fc-85e1-2b61fda5639a")
	)
	(fp_arc
		(start -0.4 0.8)
		(mid -0.753553 0.653553)
		(end -0.9 0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ec72c05e-c13e-4eac-a62f-44e071fa35a8")
	)
	(fp_arc
		(start 0.4 -0.8)
		(mid 0.753553 -0.653553)
		(end 0.9 -0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "096271f2-de40-4f45-8956-d49559312c87")
	)
	(fp_arc
		(start 0.9 0.3)
		(mid 0.753553 0.653553)
		(end 0.4 0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bd08fe5d-018e-46bc-8b27-59c872fae9a7")
	)
	(fp_rect
		(start -0.1 -0.6)
		(end 0.1 0.6)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Mask")
		(uuid "250eeb08-ba5e-4aef-b046-f0d6dc9e7f45")
	)
	(fp_line
		(start -0.949999 -0.3)
		(end -0.949999 0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "55c52a83-a674-4552-a5aa-453b1d170933")
	)
	(fp_line
		(start -0.4 0.85)
		(end 0.4 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cc80260e-06ef-439b-9c34-df197987bed1")
	)
	(fp_line
		(start 0.4 -0.85)
		(end -0.4 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "014e0cdc-a42a-48b4-aa02-7dc1267aa12b")
	)
	(fp_line
		(start 0.949999 0.3)
		(end 0.949999 -0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c2811365-9f23-4e58-b31a-a51a3d17c22e")
	)
	(fp_arc
		(start -0.949999 -0.3)
		(mid -0.788908 -0.688908)
		(end -0.4 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0742cdfc-0e41-44b9-9202-089646184d99")
	)
	(fp_arc
		(start -0.4 0.85)
		(mid -0.788909 0.688909)
		(end -0.949999 0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ca42eb2d-bb11-4cbf-ba10-d4f5cf7d6c9d")
	)
	(fp_arc
		(start 0.4 -0.85)
		(mid 0.788909 -0.688909)
		(end 0.949999 -0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "63f4af3b-c8bb-40ea-b7ac-2efeff8a2cc8")
	)
	(fp_arc
		(start 0.949999 0.3)
		(mid 0.788908 0.688908)
		(end 0.4 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c053fd0c-d60a-4ad7-89c6-d759ed00fd39")
	)
	(pad "1" smd roundrect
		(at -0.5 0 180)
		(size 0.6 1.2)
		(drill
			(offset -0.1 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.2)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "91cfca9b-1b2a-41ea-bb5b-e98988b9254b")
	)
	(pad "2" smd roundrect
		(at 0.5 0)
		(size 0.6 1.2)
		(drill
			(offset -0.1 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.2)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c41c8d82-3af9-4a47-a0e3-154cd90f915a")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "fadb7a6a-c304-459a-9163-1b58593de69d")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.075 -0.6) (xy -0.075 0.6) (xy 0.075 0.6) (xy 0.075 -0.6)
			)
		)
	)
)
