(footprint "DRQFN-116-1EP_9x9mm_P0.5_EP4x5" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -5.25 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 99a71cf3-bd38-4b1b-9dc4-db9ca18c5be1)
  )
  (fp_text value "DRQFN-116-1EP_9x9mm_P0.5_EP4x5" (at 0 3.1 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp a6c28cc1-47b2-4fec-bb57-559402e5e8a6)
  )
  (fp_text user "${REFERENCE}" (at 0 2.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 95b75c81-8da2-4e13-a11b-e1dd075d3ab0)
  )
  (fp_arc (start -4.725 -4.65) (mid -4.703033 -4.703033) (end -4.65 -4.725)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7eb6f6a9-6cfd-4034-aefc-8c65fb43ff6a))
  (fp_arc (start -4.65 4.725) (mid -4.703033 4.703033) (end -4.725 4.65)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 6e0be36e-6f59-4bc5-a2fd-defa9b76710c))
  (fp_arc (start 4.65 -4.725) (mid 4.703033 -4.703033) (end 4.725 -4.65)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 28751ac4-4095-4953-8e94-03a637f5a30a))
  (fp_arc (start 4.725 4.65) (mid 4.703033 4.703033) (end 4.65 4.725)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp d66776f7-c0fe-4d8f-b8b5-9616151d23a2))
  (fp_poly
    (pts
      (xy -4.8 -3.75)
      (xy -5 -3.6)
      (xy -5 -3.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5ab789a0-e104-453f-b18d-b5cda526ddaa))
  (fp_poly
    (pts
      (xy -4.65 4)
      (xy -4.65 4.65)
      (xy -4 4.65)
      (xy -4 4.8)
      (xy -4.65 4.8)
      (xy -4.8 4.65)
      (xy -4.8 4)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp de7ec430-6e23-4cbc-b6c4-4370a85fa5ac))
  (fp_poly
    (pts
      (xy -4 -4.65)
      (xy -4.65 -4.65)
      (xy -4.65 -4)
      (xy -4.8 -4)
      (xy -4.8 -4.65)
      (xy -4.65 -4.8)
      (xy -4 -4.8)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8cc01b4e-b845-4b37-b755-6382f9bb4506))
  (fp_poly
    (pts
      (xy 4 4.65)
      (xy 4.65 4.65)
      (xy 4.65 4)
      (xy 4.8 4)
      (xy 4.8 4.65)
      (xy 4.65 4.8)
      (xy 4 4.8)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d2df01c6-58a2-4d76-ae10-462c6aeb04cf))
  (fp_poly
    (pts
      (xy 4.65 -4)
      (xy 4.65 -4.65)
      (xy 4 -4.65)
      (xy 4 -4.8)
      (xy 4.65 -4.8)
      (xy 4.8 -4.65)
      (xy 4.8 -4)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 35825198-a912-40de-9098-d728be791385))
  (fp_line (start -4.85 4.1) (end -4.85 -4.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 912a4d93-16be-4faa-8e65-8d982beb96ca))
  (fp_line (start -4.1 -4.85) (end 4.1 -4.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e8f9a15d-40a0-47ad-b0ab-914ce53e46ab))
  (fp_line (start 4.1 4.85) (end -4.1 4.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f430b041-9c7f-4038-97bf-a8911fef9906))
  (fp_line (start 4.85 -4.1) (end 4.85 4.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2baea17e-1f9c-45ec-8d02-cb9567c4e8d5))
  (fp_arc (start -4.85 -4.1) (mid -4.63033 -4.63033) (end -4.1 -4.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 07344f4e-43c2-4358-90cf-eb9b796c6eda))
  (fp_arc (start -4.1 4.85) (mid -4.63033 4.63033) (end -4.85 4.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc163acd-cc18-4755-b81c-a72156d3d010))
  (fp_arc (start 4.1 -4.85) (mid 4.63033 -4.63033) (end 4.85 -4.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3a056b4c-f77e-4c28-bb00-eeade7933a71))
  (fp_arc (start 4.85 4.1) (mid 4.63033 4.63033) (end 4.1 4.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb301ca4-4895-4131-b3f0-f7af644b8232))
  (fp_rect (start -4.5 -4.5) (end 4.5 4.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 621ad640-9d52-47c5-ba29-32db19e0502b))
  (fp_circle (center -3.75 -3.75) (end -3.5 -3.75)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Fab") (tstamp f24efbd5-86cd-4cc1-ac90-3f1bd799d3a1))
  (pad "" smd roundrect (at -4.35 -3.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 242194a2-1bfa-4ed2-9da2-103d10b51bb0))
  (pad "" smd roundrect (at -4.35 -3.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ed9ffdf0-f3b2-4ad0-b661-a17d18f437e9))
  (pad "" smd roundrect (at -4.35 -2.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 737aeccf-5253-4b0b-a2da-9712cfe5afea))
  (pad "" smd roundrect (at -4.35 -2.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 43b62de5-357b-455d-a68e-ccf5c1104cec))
  (pad "" smd roundrect (at -4.35 -1.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 556b383f-f797-4dfa-ad97-0854f869ff8b))
  (pad "" smd roundrect (at -4.35 -1.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a25e4277-c0cc-4047-a6b9-ba9a7e97b4ca))
  (pad "" smd roundrect (at -4.35 -0.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7b3f80cf-a561-4c0e-89c6-114b0235ea0a))
  (pad "" smd roundrect (at -4.35 -0.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 02e43723-544f-4d02-a1bf-7a9c5478bf7d))
  (pad "" smd roundrect (at -4.35 0.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 75a40068-349c-4e0a-bac6-d3ca8a914cd9))
  (pad "" smd roundrect (at -4.35 0.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 4817acb1-abe3-4e95-bbf4-b9726346db4a))
  (pad "" smd roundrect (at -4.35 1.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a23b1b20-6a3b-4f51-96c1-6949284779ad))
  (pad "" smd roundrect (at -4.35 1.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp feba5efd-4353-4f6b-ac4b-50a1b4e8d094))
  (pad "" smd roundrect (at -4.35 2.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b16eb16a-dde9-4775-b1e2-e7ee0a6ceb26))
  (pad "" smd roundrect (at -4.35 2.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 77978893-9ba2-4aa6-b277-1244a08532bf))
  (pad "" smd roundrect (at -4.35 3.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 58865650-c959-4ecf-a6f5-dc3a170432f2))
  (pad "" smd roundrect (at -4.35 3.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e6ca1126-9630-4e37-9d96-7cb11ef9c84e))
  (pad "" smd roundrect (at -3.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp dbf22ce1-b123-4085-ac91-5af64ba320da))
  (pad "" smd roundrect (at -3.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 3b276f4d-f1ee-4946-b7d9-ff1ec6c53805))
  (pad "" smd roundrect (at -3.65 -3) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 88222675-71fd-4044-b40b-9aefd4e97c3c))
  (pad "" smd roundrect (at -3.65 -2.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ea53c555-0e4d-43bc-b7ae-16c0ee61b4a5))
  (pad "" smd roundrect (at -3.65 -2) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 21cd3c69-0429-40fa-97ed-6d5cd2fcce60))
  (pad "" smd roundrect (at -3.65 -1.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ea1ad475-336f-4da4-916a-6cbe91e5a87a))
  (pad "" smd roundrect (at -3.65 -1) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e4b9a9e6-e1e8-48e8-aadc-4826af1b71ac))
  (pad "" smd roundrect (at -3.65 -0.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 71a6eca2-affc-4681-88b3-584cb667866f))
  (pad "" smd roundrect (at -3.65 0) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp af1cd15e-4a3b-460c-8e6f-5a21e3e1637a))
  (pad "" smd roundrect (at -3.65 0.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp fb763aad-7985-461f-9f27-cea8d5de3f9f))
  (pad "" smd roundrect (at -3.65 1) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 99160d49-9ad2-4063-a51e-2f681dd4837c))
  (pad "" smd roundrect (at -3.65 1.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c78761af-133c-435b-9a8b-8e3cadb10639))
  (pad "" smd roundrect (at -3.65 2) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5ffa83ee-f80c-4264-90ff-3ca767d9ab8b))
  (pad "" smd roundrect (at -3.65 2.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 437a2cc9-6707-4531-843a-c006643bcbcb))
  (pad "" smd roundrect (at -3.65 3) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 94e8c367-2d68-4b4a-bb27-4f5f2b272c6a))
  (pad "" smd roundrect (at -3.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 674cae51-c290-49f3-aba9-cd6395d558b4))
  (pad "" smd roundrect (at -3.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d7401553-0036-4a7c-8759-e6e0dac1fabc))
  (pad "" smd roundrect (at -3 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 32c19a73-22c9-4f25-9552-c527c376f52b))
  (pad "" smd roundrect (at -3 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 112541b9-c146-40ba-92a9-1169822ea84b))
  (pad "" smd roundrect (at -2.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d20e5979-f74b-44e7-afda-abbbd012298f))
  (pad "" smd roundrect (at -2.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f3d7f4fd-2b2b-4ee5-bfa8-899c65dc1ffb))
  (pad "" smd roundrect (at -2.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2c10e36a-f2db-4248-a332-07552fd058b4))
  (pad "" smd roundrect (at -2.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 8d3c8e3f-2d33-4b24-8b6e-078b75a64cfa))
  (pad "" smd roundrect (at -2.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0b807717-fb59-47ec-bba5-ca6db8f3dfee))
  (pad "" smd roundrect (at -2.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e06f429f-ab20-4398-9480-c66fe7b05375))
  (pad "" smd roundrect (at -2 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e892f32d-47fb-4c8d-9d51-c0b9ec7217fb))
  (pad "" smd roundrect (at -2 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 26fb6b16-30d5-41b7-a797-1abde443b472))
  (pad "" smd roundrect (at -1.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp bb23c2a2-6098-40f1-ae77-f93d13d10de5))
  (pad "" smd roundrect (at -1.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0f60152f-ce19-4d56-868f-c9bef065bd02))
  (pad "" smd roundrect (at -1.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a2486e28-4a72-4e76-b58e-27d6b518a9d4))
  (pad "" smd roundrect (at -1.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f037d5c9-72a0-4f8b-9404-3b3b1f9984f9))
  (pad "" smd roundrect (at -1.45 -1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 5fece4dc-1721-46ee-910a-a9d1a9337687))
  (pad "" smd roundrect (at -1.45 0) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp d523f442-bd04-4532-88da-57bb22d4dbef))
  (pad "" smd roundrect (at -1.45 1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 859d2e6e-8951-4e7f-8e55-47c3c54f1b9e))
  (pad "" smd roundrect (at -1.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 36899775-4885-4108-abe5-5aa0a89aede1))
  (pad "" smd roundrect (at -1.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 79a7e178-addb-4455-bb01-9ab0e190d7fc))
  (pad "" smd roundrect (at -1 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 8b881c3f-ae2b-422f-a5ee-95ce60d6952a))
  (pad "" smd roundrect (at -1 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 6af17b37-6555-4b28-8ab0-7f1cae51bf4e))
  (pad "" smd roundrect (at -0.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0c796914-8236-4aa5-a8e5-a65f09f9b644))
  (pad "" smd roundrect (at -0.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b2a086d8-5dfe-4923-9046-a84e10961d7d))
  (pad "" smd roundrect (at -0.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 88d48b67-02cf-4dd8-b8d4-c5386638c040))
  (pad "" smd roundrect (at -0.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 871f5109-6201-4464-927f-d0061ca0e6fe))
  (pad "" smd roundrect (at -0.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 66f50dca-7daf-4523-81d9-9dac046f2427))
  (pad "" smd roundrect (at -0.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 70131c1e-e8fd-415b-9379-db67357193ef))
  (pad "" smd roundrect (at 0 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b247a1a2-45a2-410c-9c41-17f5c2ef6e49))
  (pad "" smd roundrect (at 0 -1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp ebad939b-5818-4378-82e1-78f00fa36f46))
  (pad "" smd roundrect (at 0 0) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 61e9dd15-0ad7-47aa-8d5d-b3cae1e2287a))
  (pad "" smd roundrect (at 0 1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 2ae7d660-cce9-4305-bccb-0490af85e1a0))
  (pad "" smd roundrect (at 0 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0d9e8189-1183-4118-af28-57b28b7e101f))
  (pad "" smd roundrect (at 0.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a0937034-8df1-4efe-b54f-96e1b6095a27))
  (pad "" smd roundrect (at 0.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5ee37446-4f98-493e-a68f-7467c84cc40a))
  (pad "" smd roundrect (at 0.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 34e8a005-c7f0-4787-b0ae-ef36b75367be))
  (pad "" smd roundrect (at 0.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7487e9b4-b070-4efe-bf2a-35009796d5b3))
  (pad "" smd roundrect (at 0.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 14bbabb9-54b8-4c5e-b3a5-5700c581aed7))
  (pad "" smd roundrect (at 0.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c4652e3e-a0dc-4c10-9255-1a55fcd87cff))
  (pad "" smd roundrect (at 1 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 80c5c755-d579-4eaf-a395-27c5f98df016))
  (pad "" smd roundrect (at 1 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2e587204-2f26-49e0-8de9-c00baebe247a))
  (pad "" smd roundrect (at 1.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 9bfa73f7-6839-4365-9357-5aec9d987c7c))
  (pad "" smd roundrect (at 1.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp dbb3564b-3ced-4fee-9cde-ac6566bfb828))
  (pad "" smd roundrect (at 1.45 -1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp b726bed9-8c3a-416a-aeec-af7c4546492a))
  (pad "" smd roundrect (at 1.45 0) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 0fedf77c-29f9-4d83-819e-7ee75d9527ec))
  (pad "" smd roundrect (at 1.45 1.6) (size 1.1 1.3) (layers "F.Paste") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp aa37895d-ad9f-487b-afe9-b18dc7e494ca))
  (pad "" smd roundrect (at 1.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d402e0f2-013e-4e17-93a8-e980b72e81ae))
  (pad "" smd roundrect (at 1.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 4e440ef1-f018-42cc-ae84-91e464ebc954))
  (pad "" smd roundrect (at 1.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1f77e2d6-c699-4814-8567-f31f32c2e5fe))
  (pad "" smd roundrect (at 1.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 92a0ef03-4a80-435f-bb89-d0b7b2de7342))
  (pad "" smd roundrect (at 2 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 91320086-a370-45c3-9ce6-3b6dba050c8d))
  (pad "" smd roundrect (at 2 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 8c63f6d5-54e1-4412-b12c-17534ae8feb5))
  (pad "" smd roundrect (at 2.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e381f75f-e88b-4bd8-8c76-f24eae7f216e))
  (pad "" smd roundrect (at 2.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 3863189f-3d35-4993-bc1e-4e7d236d39bc))
  (pad "" smd roundrect (at 2.5 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0adb2714-493b-43b4-be31-07d53cfad0e9))
  (pad "" smd roundrect (at 2.5 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 11adbff2-637f-4232-a2a8-d3957d865a74))
  (pad "" smd roundrect (at 2.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 1241cda8-9e88-426b-b195-96d64b5c274d))
  (pad "" smd roundrect (at 2.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 69430cc5-ee39-4735-8771-d0641a6e9a33))
  (pad "" smd roundrect (at 3 -3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b655c51b-3733-4700-ba45-0fe1f362118b))
  (pad "" smd roundrect (at 3 3.65 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ca4d2b68-3e04-41f6-ab0b-786daadd065c))
  (pad "" smd roundrect (at 3.25 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 361e9288-2f3d-419d-993a-826f6f5ce427))
  (pad "" smd roundrect (at 3.25 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 250580d0-fdc2-4ade-9d95-37e1cbda47d6))
  (pad "" smd roundrect (at 3.65 -3) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 71cbf2c3-8704-4c01-9589-7c4a239a7980))
  (pad "" smd roundrect (at 3.65 -2.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ef488dc6-f752-4467-bf03-ba25614efd4d))
  (pad "" smd roundrect (at 3.65 -2) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d83b5987-dccd-4e4b-af48-ab80a9cfc3f0))
  (pad "" smd roundrect (at 3.65 -1.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f5d6df20-3c07-46cc-b3e6-c0d1e3e14eaf))
  (pad "" smd roundrect (at 3.65 -1) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp c94ed3e6-55fb-4e65-a421-ed9526280bb7))
  (pad "" smd roundrect (at 3.65 -0.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b4543408-cc53-46c5-a663-4a2b138d7129))
  (pad "" smd roundrect (at 3.65 0) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 0b01cdc5-dd77-49e7-984f-aac5425d9db5))
  (pad "" smd roundrect (at 3.65 0.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 59df6f21-9816-47ab-af8c-965fdfe634d7))
  (pad "" smd roundrect (at 3.65 1) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7c15b669-061d-4faa-b657-97cba1e333e2))
  (pad "" smd roundrect (at 3.65 1.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 33ffdf9c-1b7f-4c9a-977e-436c77d98ae8))
  (pad "" smd roundrect (at 3.65 2) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f39ac786-2dbc-4e04-a5f5-4fe3f42ffe83))
  (pad "" smd roundrect (at 3.65 2.5) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 8652be53-d9c6-4ef7-ae7a-046d8250fc95))
  (pad "" smd roundrect (at 3.65 3) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 25ee8133-f7f8-4ee7-9e0f-bc5ae13265d9))
  (pad "" smd roundrect (at 3.75 -4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 63a5723e-af72-4531-9b8e-38a0be686e08))
  (pad "" smd roundrect (at 3.75 4.35 90) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 31ec8593-9399-4430-a4b5-f2d8c10973ec))
  (pad "" smd roundrect (at 4.35 -3.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5ad35f98-6619-4f17-b96b-d285e8f1b1d2))
  (pad "" smd roundrect (at 4.35 -3.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 053675bc-8538-4582-96af-19fcf93a7d7b))
  (pad "" smd roundrect (at 4.35 -2.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b2568e6b-c10d-4106-aafa-4c3456e05b4a))
  (pad "" smd roundrect (at 4.35 -2.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7ed7ce31-4ecb-4a26-a5a7-1d67e8a6d472))
  (pad "" smd roundrect (at 4.35 -1.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp cf849ce5-d71c-4c49-9b06-1ddbb312ddc6))
  (pad "" smd roundrect (at 4.35 -1.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 6ad350b0-0d8f-4551-9676-b4f7e4765d57))
  (pad "" smd roundrect (at 4.35 -0.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp f3a3c2a6-b4ea-4e87-94f0-956f187d1086))
  (pad "" smd roundrect (at 4.35 -0.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e30b65f5-4a9e-4ca6-a3ff-00fd7b68232f))
  (pad "" smd roundrect (at 4.35 0.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2c47078a-c631-48ec-971e-b3e08f7fd243))
  (pad "" smd roundrect (at 4.35 0.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 18e57c42-56ef-4999-84ad-024a36820dd3))
  (pad "" smd roundrect (at 4.35 1.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 4e476cbc-97a5-473b-8c37-265200d8faa1))
  (pad "" smd roundrect (at 4.35 1.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5cf4a0cb-fae6-4dea-adc9-77a748fa916b))
  (pad "" smd roundrect (at 4.35 2.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 88f18853-b651-4783-b556-ce3266766503))
  (pad "" smd roundrect (at 4.35 2.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 306654ad-a0e2-4384-bfad-4b692bc2d7c1))
  (pad "" smd roundrect (at 4.35 3.25) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e6249b81-59b5-4112-bbdf-5c1a10343b87))
  (pad "" smd roundrect (at 4.35 3.75) (size 0.4 0.2) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp e08c5020-bc3b-4d35-b090-e9e24a329c6f))
  (pad "117" smd roundrect (at 0 0) (size 4 4.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.025)
    (thermal_bridge_angle 45) (tstamp 39754866-0ce4-4bb3-adde-3107f98ca3b5))
  (pad "A1" smd roundrect (at -4.4 -3.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4898e4c6-d213-4599-b327-27dd3632c4db))
  (pad "A2" smd roundrect (at -4.4 -3.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp fe5d4f68-587a-46de-b5cf-ed72d26f3421))
  (pad "A3" smd roundrect (at -4.4 -2.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 8068c6e6-d5b2-4efb-add7-9b000d35a07d))
  (pad "A4" smd roundrect (at -4.4 -2.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 054b7c30-41d8-47ad-bb78-ba916a8a2064))
  (pad "A5" smd roundrect (at -4.4 -1.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e72bd84a-323d-4f68-acc1-f817c611743b))
  (pad "A6" smd roundrect (at -4.4 -1.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d2b6254e-1698-4ac9-9d58-8f162fd344c8))
  (pad "A7" smd roundrect (at -4.4 -0.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 827f28fd-d61f-411b-a649-2bce4ebb33fd))
  (pad "A8" smd roundrect (at -4.4 -0.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 42b0e096-0ae6-49fb-a0fc-25354ae261eb))
  (pad "A9" smd roundrect (at -4.4 0.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e8519a1c-2ebb-437a-bca1-64ca1180cac3))
  (pad "A10" smd roundrect (at -4.4 0.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp cc273f65-19d6-4869-9f44-844e17596fbf))
  (pad "A11" smd roundrect (at -4.4 1.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 196c9464-c740-495a-aba2-fb32bf3c99a5))
  (pad "A12" smd roundrect (at -4.4 1.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e0b09841-c49a-4b95-9ca2-428639bdc9cc))
  (pad "A13" smd roundrect (at -4.4 2.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ab49713e-082e-46ec-a0ee-2e2ffd911ccc))
  (pad "A14" smd roundrect (at -4.4 2.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e4fb20f3-81d5-423d-8a24-fbc0c0e3910d))
  (pad "A15" smd roundrect (at -4.4 3.25) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 3687004a-efc0-45d5-b70c-71beafc9931d))
  (pad "A16" smd roundrect (at -4.4 3.75) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b9b3e93c-13f0-4d2c-a055-e46b12e03c03))
  (pad "A17" smd roundrect (at -3.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 6c2d3cd7-e0a5-45b6-b5c2-49861eeed81e))
  (pad "A18" smd roundrect (at -3.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 58d99d20-267f-42ee-8a5c-73f3de912079))
  (pad "A19" smd roundrect (at -2.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d435da48-d0c4-4c5b-a8d6-9799938841ff))
  (pad "A20" smd roundrect (at -2.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 677d537c-7c66-44de-9ef0-12a8ebf0f9b9))
  (pad "A21" smd roundrect (at -1.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5a6e71b4-a055-4d94-8d86-de5adbc3e9e5))
  (pad "A22" smd roundrect (at -1.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f6d29ac6-2205-4034-8961-bd50f8706ff6))
  (pad "A23" smd roundrect (at -0.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ae020df9-e215-40e7-a384-3e73cb32e59e))
  (pad "A24" smd roundrect (at -0.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7a20133c-e27e-4a56-a9ba-a31df2d66312))
  (pad "A25" smd roundrect (at 0.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 0961d949-7954-436f-a603-c1222f71d6c4))
  (pad "A26" smd roundrect (at 0.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 62919d24-291e-4aeb-9879-920beb3dbf4e))
  (pad "A27" smd roundrect (at 1.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 126d777a-a474-464b-acc3-39da1b4f7844))
  (pad "A28" smd roundrect (at 1.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9c11d824-4db9-48d0-82ed-d391653054fb))
  (pad "A29" smd roundrect (at 2.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 87326458-ff9f-4cd7-92b3-212f382751e2))
  (pad "A30" smd roundrect (at 2.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp cc47b24a-a444-4a35-b1ee-33a5285fda33))
  (pad "A31" smd roundrect (at 3.25 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 678b35b1-3796-44c9-9911-411fee976a79))
  (pad "A32" smd roundrect (at 3.75 4.4 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d8dc2cc1-688a-4bed-93be-b02523928dae))
  (pad "A33" smd roundrect (at 4.4 3.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 90163141-f84a-4d43-ac39-4575bfd864e8))
  (pad "A34" smd roundrect (at 4.4 3.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 23963ff5-a731-4c4b-b223-62d9cd0084e5))
  (pad "A35" smd roundrect (at 4.4 2.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 60b0d9be-caeb-47c6-a3af-386d0ae5a436))
  (pad "A36" smd roundrect (at 4.4 2.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp c8d2f074-204a-4320-949a-4953c023ab76))
  (pad "A37" smd roundrect (at 4.4 1.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ef6dc3f5-ebf3-4fc4-9eec-d969ac8081d4))
  (pad "A38" smd roundrect (at 4.4 1.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e6679f7d-93db-4dfa-b10c-398874d45d00))
  (pad "A39" smd roundrect (at 4.4 0.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 50d6ede3-396a-414c-9d0b-bc5c616fa3c8))
  (pad "A40" smd roundrect (at 4.4 0.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 81afe8f8-4019-44af-b2d2-148563785783))
  (pad "A41" smd roundrect (at 4.4 -0.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 041dec97-d82e-4de1-b623-084d1fd1875d))
  (pad "A42" smd roundrect (at 4.4 -0.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b1d6690b-04bc-4d0e-af3f-91a6f88a0add))
  (pad "A43" smd roundrect (at 4.4 -1.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 1ebdba8a-446f-437a-b339-3fd4cf5db14a))
  (pad "A44" smd roundrect (at 4.4 -1.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7bc26229-9ddb-4d89-982a-c1b5a5e170ef))
  (pad "A45" smd roundrect (at 4.4 -2.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 191cec4f-d23b-4746-9459-468f535e85d2))
  (pad "A46" smd roundrect (at 4.4 -2.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 3d6c9a66-51bb-430f-bfe3-a2617d572aa1))
  (pad "A47" smd roundrect (at 4.4 -3.25 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 32af7eac-6022-40b3-8fa4-da847865657d))
  (pad "A48" smd roundrect (at 4.4 -3.75 180) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 73cef0fc-a00b-43c3-9807-b076cd8b68f4))
  (pad "A49" smd roundrect (at 3.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 85103c33-c255-432c-a4ec-0d86c411d786))
  (pad "A50" smd roundrect (at 3.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 82ce6174-53f3-4d7d-bf1e-19916d7b6eab))
  (pad "A51" smd roundrect (at 2.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ceb4b930-42e2-4e5e-beb4-d38fe7d5c538))
  (pad "A52" smd roundrect (at 2.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp add17917-2b65-442c-a433-8bd046d2d80a))
  (pad "A53" smd roundrect (at 1.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp cce85c90-e140-44ae-8902-29b0582d2cc8))
  (pad "A54" smd roundrect (at 1.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d5aac1bf-90c3-4f44-b4c9-68b7a08e8164))
  (pad "A55" smd roundrect (at 0.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 06543a01-2f21-499b-b2bf-79ebde9619f6))
  (pad "A56" smd roundrect (at 0.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e333f3dc-654e-4a18-b90b-609aa1e4046d))
  (pad "A57" smd roundrect (at -0.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4ef72c61-f6b6-45e6-a79e-2e56a7c6f6a2))
  (pad "A58" smd roundrect (at -0.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 20d14572-b30f-4aa4-bf44-9b4db2a829b8))
  (pad "A59" smd roundrect (at -1.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 557f2068-b96d-44d3-82f0-ffd4c0fad9b5))
  (pad "A60" smd roundrect (at -1.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ede3598f-15ba-48e4-8a76-dea7e887b7c1))
  (pad "A61" smd roundrect (at -2.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ff4a3898-4c4f-49b8-b7e1-aaa9dbe3d21a))
  (pad "A62" smd roundrect (at -2.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7934b076-e57e-44ad-a3f0-4931354f7b7c))
  (pad "A63" smd roundrect (at -3.25 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f579ce5d-2e24-4059-a402-2ce23259f388))
  (pad "A64" smd roundrect (at -3.75 -4.4 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5e03b4ab-4593-41ef-b595-8669b0c9b888))
  (pad "B1" smd roundrect (at -3.6 -3) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 75c0dfd2-2086-4b3c-93af-12c67297648c))
  (pad "B2" smd roundrect (at -3.6 -2.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ed749cd0-96db-4f7c-a585-caa394180bf1))
  (pad "B3" smd roundrect (at -3.6 -2) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 1203c6af-1674-4fab-8b93-c4b1d101ce17))
  (pad "B4" smd roundrect (at -3.6 -1.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 6329fcb1-540d-47a4-8dd4-97d606ade390))
  (pad "B5" smd roundrect (at -3.6 -1) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9e4ba653-1875-4e5d-99ab-d57866460a4e))
  (pad "B6" smd roundrect (at -3.6 -0.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 2762b528-87f8-44b6-98da-a09be999a2a2))
  (pad "B7" smd roundrect (at -3.6 0) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5c5aa0e7-a59d-4c29-ab49-b319d3173f2e))
  (pad "B8" smd roundrect (at -3.6 0.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 29622e6f-64d0-4562-9b98-396b654b0b0a))
  (pad "B9" smd roundrect (at -3.6 1) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 04db0162-4540-42d6-a643-bbed4d2d8139))
  (pad "B10" smd roundrect (at -3.6 1.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 43717148-d204-4f3d-90c0-60bd42fd7902))
  (pad "B11" smd roundrect (at -3.6 2) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 8dfdf5c1-9f42-47e3-b938-c8b3f4267880))
  (pad "B12" smd roundrect (at -3.6 2.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5012b535-272d-4630-85f5-d73af3c535b1))
  (pad "B13" smd roundrect (at -3.6 3) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp a6f8b18d-a274-4a5e-afb8-5fe0e0c66858))
  (pad "B14" smd roundrect (at -3 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 943a2344-af82-40a3-adec-db524208f693))
  (pad "B15" smd roundrect (at -2.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 95e05a0a-72b8-4553-9fb3-288056472ad7))
  (pad "B16" smd roundrect (at -2 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e4a8f25d-666c-4433-a2b8-b76e340d717d))
  (pad "B17" smd roundrect (at -1.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 0bcf487b-ca0a-4f4a-a372-5e70a081ef3c))
  (pad "B18" smd roundrect (at -1 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e0f7c995-b25c-4af8-82b0-50f72b464042))
  (pad "B19" smd roundrect (at -0.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9c54dcad-12d9-4088-a74f-90174772714a))
  (pad "B20" smd roundrect (at 0 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f7537585-c129-4e99-8749-efb8603ee102))
  (pad "B21" smd roundrect (at 0.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b3ee90bb-4e84-4e69-8f82-e9a7d7f29e75))
  (pad "B22" smd roundrect (at 1 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp f2ef2cdb-858a-491f-bb8e-0e1ea8f5ab97))
  (pad "B23" smd roundrect (at 1.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp adab0142-d941-480d-93c9-9aa242854007))
  (pad "B24" smd roundrect (at 2 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 14238866-d501-4416-acb9-17065487415a))
  (pad "B25" smd roundrect (at 2.5 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 4ea0b36c-e12c-43cf-86be-b784bd299099))
  (pad "B26" smd roundrect (at 3 3.6 270) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 489e26b1-8f2f-4106-bb74-812ae403cbc0))
  (pad "B27" smd roundrect (at 3.6 3) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 88dac696-5a7e-49b0-b522-0c57a001430c))
  (pad "B28" smd roundrect (at 3.6 2.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e8ea4e0a-d96a-47d2-b654-32f56c760b2a))
  (pad "B29" smd roundrect (at 3.6 2) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 817f650a-d542-44c6-a6d8-6763dd9925a1))
  (pad "B30" smd roundrect (at 3.6 1.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e6eca711-d53f-45de-9398-8c6fbd8600e1))
  (pad "B31" smd roundrect (at 3.6 1) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp fe8d9dea-e88e-43f6-8395-5915471630f5))
  (pad "B32" smd roundrect (at 3.6 0.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 03ced447-b8f1-457c-a880-abf60b78c17a))
  (pad "B33" smd roundrect (at 3.6 0) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp a9d989c7-7016-4eb3-a049-ccb4e8b8c7fe))
  (pad "B34" smd roundrect (at 3.6 -0.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 18c68185-906e-4c59-aac4-a1f678dd2280))
  (pad "B35" smd roundrect (at 3.6 -1) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp d2449c9b-b7a7-47f1-b813-def4ceb6d494))
  (pad "B36" smd roundrect (at 3.6 -1.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 9c521534-a83a-49db-bb62-d574afd09097))
  (pad "B37" smd roundrect (at 3.6 -2) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 0140e350-ecd0-4687-a8ca-8857c9ad651d))
  (pad "B38" smd roundrect (at 3.6 -2.5) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 15caa6a8-4dd9-4bb2-bed8-8b2e87492523))
  (pad "B39" smd roundrect (at 3.6 -3) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 75f2a189-cae8-48ef-bd03-8f3b2f3696f9))
  (pad "B40" smd roundrect (at 3 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 19389cba-62c2-4219-9807-9b59ed7f3e22))
  (pad "B41" smd roundrect (at 2.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 363c3a93-440e-47e0-b926-ffb6e8824b94))
  (pad "B42" smd roundrect (at 2 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 7bbc685a-5c16-42a1-b086-cf168917a048))
  (pad "B43" smd roundrect (at 1.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp e8951d35-9da1-46a1-9184-09912c788c05))
  (pad "B44" smd roundrect (at 1 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 39658bb4-3600-4bc8-bfe1-12674184c0d2))
  (pad "B45" smd roundrect (at 0.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 033a3a43-185e-4e04-9cbe-873d5dbde311))
  (pad "B46" smd roundrect (at 0 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 77839874-0606-41bf-af33-f724c41e9674))
  (pad "B47" smd roundrect (at -0.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 24a56f91-2df5-4a78-9830-82826ddd6b8b))
  (pad "B48" smd roundrect (at -1 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 5d3f03b4-ce9a-40a4-a61d-f9e6962ff400))
  (pad "B49" smd roundrect (at -1.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp abbb24a9-1085-471f-8cb1-175af788da07))
  (pad "B50" smd roundrect (at -2 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp ec4fc39f-9073-4a40-a683-44227cc1e4c4))
  (pad "B51" smd roundrect (at -2.5 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp aa694b74-8f9f-4638-a60f-80ea7f975b1c))
  (pad "B52" smd roundrect (at -3 -3.6 90) (size 0.6 0.28) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 676870e6-183a-4668-aac5-aa7bbfd0352f))
)
