(module SO-8 (layer F.Cu) (tedit 53D3C0F9)
  (tags SO8)
  (attr smd)
  (fp_text reference Q1 (at -3 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value H-Bridge_Diodes_DMHC3025LSD-13 (at 0 -1.05) (layer F.SilkS) hide
    (effects (font (size 0.3 0.3) (thickness 0.05)))
  )
  (fp_text user 1 (at -2.5 3.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center -2.05 1.55) (end -2.05 1.95) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.45 1.95) (end 2.45 -1.95) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.45 -1.95) (end -2.45 -1.95) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.45 -1.95) (end -2.45 1.95) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.45 1.95) (end 2.45 1.95) (layer F.SilkS) (width 0.127))
  (pad 1 smd rect (at -1.905 2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.635 2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.635 2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.905 2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.905 -2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.635 -2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -0.635 -2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.905 -2.7) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask))
  (model 3D/kicad/Housings_SOIC/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
