(footprint "Arc_14x_Ri_1.2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 53.5 -53 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f8fee7a8-e1bd-4305-85e4-e98c49f5d4a9)
  )
  (fp_text value "Arc_14x_Ri_1.2" (at 53.5 -51.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e6f343ba-df89-4e4d-87a6-b56cecbafb57)
  )
  (fp_text user "${REFERENCE}" (at 53.5 -50 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 951aa451-c0f0-4cd0-afda-bc6aaa99ec23)
  )
  (fp_arc (start -4.825 0) (mid 0 -4.825) (end 4.825 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp a904c887-49f2-4be1-92be-81b82b2b25bb))
  (fp_arc (start -4.525 0) (mid 0 -4.525) (end 4.525 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 4603af9d-52e7-4277-a6f7-5d8f16e708e4))
  (fp_arc (start -4.225 0) (mid 0 -4.225) (end 4.225 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 96991286-3c45-4ded-a533-1227f3ac0677))
  (fp_arc (start -3.925 0) (mid 0 -3.925) (end 3.925 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 264e2e67-b1f9-449f-bfbe-2b6720cefad3))
  (fp_arc (start -3.625 0) (mid 0 -3.625) (end 3.625 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 5db0a2cc-77d3-4a61-b8e0-5723cffd8d0d))
  (fp_arc (start -3.325 0) (mid 0 -3.325) (end 3.325 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 8d7e87d5-a909-4f8f-ac6c-3891f6cc7fd0))
  (fp_arc (start -3.025 0) (mid 0 -3.025) (end 3.025 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 58ed0e85-371a-49dd-8c32-6f387ac47d06))
  (fp_arc (start -2.725 0) (mid 0 -2.725) (end 2.725 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 6236c43a-7a28-4a8a-bec2-32a93bf00c29))
  (fp_arc (start -2.425 0) (mid 0 -2.425) (end 2.425 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 12ae42fb-6433-47f3-ba07-0b9c30a7d20a))
  (fp_arc (start -2.125 0) (mid 0 -2.125) (end 2.125 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp bc9a7e30-3ede-4b69-a96d-f003fb3d0ab6))
  (fp_arc (start -1.825 0) (mid 0 -1.825) (end 1.825 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 2d4028aa-dd6b-413d-8e93-a56e340f83a2))
  (fp_arc (start -1.525 0) (mid 0 -1.525) (end 1.525 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 66941ddb-c6c1-4696-b0e0-e32c5f2488e6))
  (fp_arc (start -1.225 0) (mid 0 -1.225) (end 1.225 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 5bce8717-196a-4fcb-a54a-926fac66a568))
  (fp_arc (start -0.925 0) (mid 0 -0.925) (end 0.925 0)
    (stroke (width 0.15) (type default)) (layer "F.Cu") (tstamp 7188f26b-b6c4-448d-9e37-1ec75f50b7ce))
  (fp_circle (center 0 0) (end 0.6 0)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5e7d7fe8-bb1d-4f0b-b6dd-78ad36c00875))
)
