(footprint "Heatsink_51x36x12mm_M2_47x32mm" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "C6490_Carrier.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "HS2" (at 0 -21 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ef34098c-09fc-4c34-98e0-f1fd058eb8be)
  )
  (fp_text value "HEATSINK" (at 0 23 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 01285966-26fc-4857-ac33-3f11f5b46eb6)
  )
  (fp_text user "${REFERENCE}" (at 0 24.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2210ca1b-9cdf-4763-869c-147730b7b3be)
  )
  (fp_line (start -18 -25.5) (end -16 -25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 4f02ecda-2fb8-4468-8ca6-941159314556))
  (fp_line (start -18 -23.5) (end -18 -25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 18d8f4b2-b241-40aa-beb3-57cd1049582c))
  (fp_line (start -18 23.5) (end -18 25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 1d5cebd4-dd04-4e9a-ac29-b9d9b48099ee))
  (fp_line (start -18 25.5) (end -16 25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp c914e3ce-ace8-4813-8902-1317cbc01523))
  (fp_line (start 16 -25.5) (end 18 -25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp be2f7eb8-4c70-4347-8763-1a07a5dea035))
  (fp_line (start 16 25.5) (end 18 25.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp ac6f64b3-6e52-4a44-803e-a3426ae866da))
  (fp_line (start 18 -25.5) (end 18 -23.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp deb90497-34d9-4670-a6dd-d73d56c9edec))
  (fp_line (start 18 25.5) (end 18 23.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp be8260f8-4cd8-42c2-a82f-6e734f07f44f))
  (fp_rect (start -18 -25.5) (end 18 25.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4dddbbc2-5183-43e3-86c5-a940b7385984))
  (pad "1" thru_hole circle (at -16 -23.5) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp 5406d939-a7c1-4c59-9a58-b7d94fadd5a1))
  (pad "1" connect circle (at -16 -23.5) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp 78876695-2d73-436f-8820-b638ac5f141c))
  (pad "1" thru_hole circle (at -16 23.5) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp e9452382-6db6-4daf-9000-f25fb7dec24b))
  (pad "1" connect circle (at -16 23.5) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp a92ea72a-93fa-4c98-8e6c-6e8f1f45aec5))
  (pad "1" thru_hole circle (at 16 -23.5) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp 56fcacf7-fa0d-431e-9979-23e0dc042f28))
  (pad "1" connect circle (at 16 -23.5) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp c27d9347-d508-4ec5-bc29-9e0bc1c6b811))
  (pad "1" thru_hole circle (at 16 23.5) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp 9baf9d09-eb52-40f7-97df-37cf634e7f7a))
  (pad "1" connect circle (at 16 23.5) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp 15080c09-e5ec-44c5-82b7-676e36ce63da))
  (model "${KICAD7_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink 51x36x12.step"
    (offset (xyz 0 0 2.7))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
