(footprint "1005_C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "0402 1005 Capacitor")
	(property "Reference" "C135"
		(at 0.75 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3530127a-e8e7-49c4-b293-c7acfb6f4e43")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(property "Value" "Csmall"
		(at 0.75 0.375 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d0b368ae-0e6e-47d5-bb76-765b4b9ffa2f")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.05)
			)
			(justify left)
		)
	)
	(property "Footprint" "1005_C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3a9f7087-3a5e-4d6e-9132-8db701931c90")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cacdb8e2-0fdd-4659-a8c4-3ba72cdd1b4d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8ea82dd4-121d-413d-b0da-55f0ee597a4a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" "SPICE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1f69d45d-883c-4e4b-bef8-b3b10703d6a9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Params" "type=\"C\" model=\"100n\" lib=\"\""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1796ade-3510-4d45-b453-df07115030c8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" "1=1 2=2"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7ec543f6-0aab-4a0b-9dba-e6dad00f8965")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.03)
	(solder_paste_margin -0.02)
	(attr smd)
	(fp_poly
		(pts
			(xy 0.225 -0.325) (xy -0.225 -0.325) (xy -0.225 -0.475) (xy 0.225 -0.475)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "8ddf032a-5d07-4607-b776-b84e257c3eab")
	)
	(fp_poly
		(pts
			(xy 0.225 0.475) (xy -0.225 0.475) (xy -0.225 0.325) (xy 0.225 0.325)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "dbd2de7b-cd5e-4eb6-8b69-9c204d5f4554")
	)
	(fp_line
		(start -0.8 -0.2)
		(end -0.8 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b2b2f92f-9be9-4f93-8bf7-3f873ed98c62")
	)
	(fp_line
		(start -0.6 -0.4)
		(end 0.6 -0.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b771f4e8-82ba-4166-a790-ec7f3ad956be")
	)
	(fp_line
		(start -0.6 0.4)
		(end 0.6 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7266a051-085c-41e1-9c9b-2d92980bdfa7")
	)
	(fp_line
		(start 0.8 -0.2)
		(end 0.8 0.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "20a19dcd-c9c7-48ed-8cf8-196b8356e612")
	)
	(fp_arc
		(start -0.8 -0.2)
		(mid -0.741421 -0.341421)
		(end -0.6 -0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3182ea8f-18aa-4485-89b0-769dd9067d2b")
	)
	(fp_arc
		(start -0.6 0.4)
		(mid -0.741421 0.341421)
		(end -0.8 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9e452897-feb1-4a8e-b424-46e150b54f08")
	)
	(fp_arc
		(start 0.6 -0.4)
		(mid 0.741421 -0.341421)
		(end 0.8 -0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7793f067-e754-42b4-a049-1ce76ac01612")
	)
	(fp_arc
		(start 0.8 0.2)
		(mid 0.741421 0.341421)
		(end 0.6 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bd31dc39-1698-49b7-89d6-eeea69afba51")
	)
	(fp_rect
		(start -0.5 -0.25)
		(end 0.5 0.25)
		(stroke
			(width 0.025)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "3f9d82fb-8e80-4792-a66c-54e3b887aa0f")
	)
	(pad "" smd oval
		(at -0.45 0)
		(size 0.3 0.4)
		(layers "F.Paste")
		(uuid "1e600341-d7e5-4051-b561-63812ad96d26")
	)
	(pad "" smd oval
		(at 0.45 0)
		(size 0.3 0.4)
		(layers "F.Paste")
		(uuid "1191bb6f-2da7-4851-9009-22f636230e2c")
	)
	(pad "1" smd roundrect
		(at -0.45 0)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "4843c003-1423-4268-b906-56178c6dd21f")
	)
	(pad "2" smd roundrect
		(at 0.45 0)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left)
		(uuid "c4bb74ca-5a3f-46cf-bc5b-2513edb338ac")
	)
	(model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
