(footprint "Molex_Mini-Fit_Jr_5566-02A_2x01_P4.20mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-02A, example for new mpn: 39-28-x02x, 1 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
  (tags "connector Molex Mini-Fit_Jr side entry")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -3.45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5b31102a-0a75-4a25-88ae-c819dcc3cfee)
  )
  (fp_text value "Molex_Mini-Fit_Jr_5566-02A_2x01_P4.20mm_Vertical" (at 0 9.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b7814bf1-68e3-47ae-b3a8-6b81a0781fcb)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.55) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d10e63b-a45c-4a8c-8f79-ae63a0276e9e)
  )
  (fp_line (start -3.05 -2.6) (end -3.05 0.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 515ff734-d2ec-4826-aa74-de38c8b6ad62))
  (fp_line (start -2.81 -2.36) (end -2.81 7.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 060db758-bd88-4c6b-9728-84a80e115eeb))
  (fp_line (start -2.81 7.46) (end -1.81 7.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d683ce32-d7fb-4427-b9e5-4b37119b8a47))
  (fp_line (start -1.81 7.46) (end -1.81 8.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a9800d77-e980-4ce2-a4ab-43a0e6813fe8))
  (fp_line (start -1.81 8.86) (end 0 8.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0a7101be-8a5c-4c97-9ccc-2365bbcad9ad))
  (fp_line (start -0.2 -2.6) (end -3.05 -2.6)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d9229e4-1ac8-48f4-adfd-3401efba58c5))
  (fp_line (start 0 -2.36) (end -2.81 -2.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1fca929f-de04-468f-9643-74dc0636007f))
  (fp_line (start 0 -2.36) (end 2.81 -2.36)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 610b5716-7883-4760-b149-cc317a7ef540))
  (fp_line (start 1.81 7.46) (end 1.81 8.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a4ad8629-e1bc-4c42-a20f-e29d3588f06b))
  (fp_line (start 1.81 8.86) (end 0 8.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0b706395-b9c6-4440-86ac-45a044d4715e))
  (fp_line (start 2.81 -2.36) (end 2.81 7.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b6d958a-30d6-4a43-aa25-bce80d32f866))
  (fp_line (start 2.81 7.46) (end 1.81 7.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc57dc23-8c17-41aa-8933-8ab972f2d631))
  (fp_line (start -3.2 -2.75) (end -3.2 9.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1c924f8-c36d-4622-8dbe-0ea1c921ed2c))
  (fp_line (start -3.2 9.25) (end 3.2 9.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c4b8a5d2-df3f-48ef-801a-b52d0b9794cd))
  (fp_line (start 3.2 -2.75) (end -3.2 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b125706c-273c-4c9f-8083-427df61c2732))
  (fp_line (start 3.2 9.25) (end 3.2 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a711e09-ba01-469c-9a41-5057b07353a4))
  (fp_line (start -3.05 -2.6) (end -3.05 0.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 98a1089a-1783-48fd-8aa2-deebe4f5e2aa))
  (fp_line (start -2.7 -2.25) (end -2.7 7.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb87fbd9-0ca4-4292-a384-324cf3c9cf18))
  (fp_line (start -2.7 7.35) (end 2.7 7.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b2a0a6b-1b6f-4a7b-aa4e-c88fbf9f78c5))
  (fp_line (start -1.7 7.35) (end -1.7 8.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6880600e-5b10-4af8-a74f-aff8b75bfcdb))
  (fp_line (start -1.7 8.75) (end 1.7 8.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c526d0b-c241-4e46-a559-196df394678a))
  (fp_line (start -1.65 -1) (end -1.65 2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c7e22f9-d5b1-4765-bd2c-352130f70c01))
  (fp_line (start -1.65 2.3) (end 1.65 2.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d009c263-650a-4e41-9069-2220fb7c3589))
  (fp_line (start -1.65 4.025) (end -0.825 3.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bac20216-da4e-42dd-b8b9-7be00712b8c3))
  (fp_line (start -1.65 6.5) (end -1.65 4.025)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d915393-5807-42d4-affb-5b9cb41f2b0e))
  (fp_line (start -0.825 3.2) (end 0.825 3.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a863d617-3958-4198-a8b0-1e94e231f000))
  (fp_line (start -0.2 -2.6) (end -3.05 -2.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 220afb73-d3ad-4958-9366-b141ec78a9ad))
  (fp_line (start 0.825 3.2) (end 1.65 4.025)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 140f6c52-5002-4baa-9199-e0f682e2f9c2))
  (fp_line (start 1.65 -1) (end -1.65 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9fdae440-5e3c-4500-a9b6-78175d21f2b4))
  (fp_line (start 1.65 2.3) (end 1.65 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91448c15-bc30-4411-83a5-481f3efec29b))
  (fp_line (start 1.65 4.025) (end 1.65 6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea056464-3190-4da5-9f8d-21d2a465d997))
  (fp_line (start 1.65 6.5) (end -1.65 6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 45e6a24f-0913-4373-a820-b23eca819572))
  (fp_line (start 1.7 8.75) (end 1.7 7.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06902ec6-2464-4772-bf98-6b45823be832))
  (fp_line (start 2.7 -2.25) (end -2.7 -2.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bad0d4fc-25fa-4491-917f-15c81b9d65af))
  (fp_line (start 2.7 7.35) (end 2.7 -2.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1346a691-0f10-4e0a-a005-19cf01791dd6))
  (pad "1" thru_hole roundrect (at 0 0) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.092593) (tstamp aae32369-4473-4591-b384-af1dae19adbc))
  (pad "2" thru_hole oval (at 0 5.5) (size 2.7 3.3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 1f8ac972-ec82-4ea0-a14c-c603c8a0edde))
  (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-02A_2x01_P4.20mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_Molex.3dshapes/039281023.stp"
    (offset (xyz 0 -2.54 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -180))
  )
)
