(module 4P_4.5x4_5_pitch (layer F.Cu) (tedit 5C40DF23)
  (attr virtual)
  (fp_text reference M1 (at 0 -10.5 -180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value STEPPER (at 2.5 0 -90) (layer F.Fab)
    (effects (font (size 0.25 0.25) (thickness 0.05)))
  )
  (pad 1 connect roundrect (at 0 -7.5) (size 4.5 4) (layers F.Cu F.Mask) (roundrect_rratio 0.167))
  (pad 2 connect roundrect (at 0 -2.5) (size 4.5 4) (layers F.Cu F.Mask) (roundrect_rratio 0.167))
  (pad 3 connect roundrect (at 0 2.5) (size 4.5 4) (layers F.Cu F.Mask) (roundrect_rratio 0.167))
  (pad 4 connect roundrect (at 0 7.5) (size 4.5 4) (layers F.Cu F.Mask) (roundrect_rratio 0.167))
)
