(module Address_pads_3P_zigzag (layer F.Cu) (tedit 586D5CC3)
  (solder_mask_margin 0.001)
  (solder_paste_margin -0.001)
  (attr virtual)
  (fp_text reference JP1 (at -1.475 0 270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value I2C_ADDR (at -0.225 -1.525 180) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user 0 (at 0.75 -0.7 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user 1 (at 0.75 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user 2 (at 0.75 0.7 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_circle (center -0.95 -1.075) (end -0.925 -1.075) (layer F.SilkS) (width 0.125))
  (fp_circle (center -0.95 0.35) (end -0.925 0.35) (layer F.SilkS) (width 0.125))
  (pad 1 connect roundrect (at 0 0 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad H connect roundrect (at -0.49 0.36 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad 2 connect roundrect (at 0 0.72 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad 0 connect roundrect (at 0 -0.72 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad L connect roundrect (at -0.49 -0.36 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad H connect roundrect (at -0.49 -1.08 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad L connect roundrect (at -0.49 1.08 45) (size 0.4 0.4) (layers F.Cu F.Mask)(roundrect_rratio 0.15))
  (pad 7 connect rect (at -0.235 -0.89 45) (size 0.305 0.5) (layers F.Mask))
  (pad "" connect rect (at -0.24 -0.175 45) (size 0.305 0.5) (layers F.Mask))
  (pad "" connect rect (at -0.24 0.545 45) (size 0.305 0.5) (layers F.Mask))
  (pad "" connect rect (at -0.245 -0.54 315) (size 0.305 0.5) (layers F.Mask))
  (pad "" connect rect (at -0.245 0.185 315) (size 0.305 0.5) (layers F.Mask))
  (pad "" connect rect (at -0.25 0.905 315) (size 0.305 0.5) (layers F.Mask))
  (pad "" smd roundrect (at -0.245 -0.54 315) (size 0.4 1) (layers F.Paste)(roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.245 0.9 315) (size 0.4 1) (layers F.Paste)(roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.245 -0.18 45) (size 0.4 1) (layers F.Paste)(roundrect_rratio 0.25))
)
