(module Push_SMD_Mom_6x6mm (layer F.Cu) (tedit 56ABA3CD)
  (tags "SWITCH PUSHBUTTON")
  (solder_mask_margin -0.01)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference SW2 (at 0 -2.5) (layer F.SilkS) hide
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (fp_text value SW2 (at -3.75 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 1 -1.75) (layer F.SilkS) (width 0.127))
  (fp_line (start -3 -3) (end 3 -3) (layer F.SilkS) (width 0.127))
  (fp_line (start 3 -3) (end 3 3) (layer F.SilkS) (width 0.127))
  (fp_line (start 3 3) (end -3 3) (layer F.SilkS) (width 0.127))
  (fp_line (start -3 3) (end -3 -3) (layer F.SilkS) (width 0.127))
  (pad 1 smd rect (at -2.25 4.05) (size 1 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 2.25 4.05) (size 1 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.25 -4.05) (size 1 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.25 -4.05) (size 1 1.9) (layers F.Cu F.Paste F.Mask))
  (model ${KICAD7_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Button_6x6mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 90 180 90))
  )
)
