(module JST_GH_BM07B-GHS-TBT_07x1.25mm_Straight (layer F.Cu) (tedit 57EE9821)
  (descr "JST GH series connector, BM07B-GHS-TBT, top entry type")
  (tags "connector jst GH SMT top vertical entry 1.25mm pitch")
  (attr smd)
  (fp_text reference J1 (at -5.5 -2.25) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MCU (at 0 1.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.4 2.975) (end 4.4 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.4 2.975) (end 4.4 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.4 2.475) (end -4.4 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.4 2.475) (end -4.4 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.1 -0.225) (end -6.1 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.1 -1.325) (end -4.45 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.45 -1.325) (end -4.45 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.45 -0.825) (end -5.6 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.6 -0.825) (end -5.6 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.6 -0.225) (end -6.1 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.1 -0.225) (end 6.1 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.1 -1.325) (end 4.45 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.45 -1.325) (end 4.45 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.45 -0.825) (end 5.6 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.6 -0.825) (end 5.6 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.6 -0.225) (end 6.1 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 -3.175) (end -4 -3.675) (layer F.SilkS) (width 0.15))
  (fp_line (start -4 -3.675) (end -3.5 -3.675) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 -3.675) (end -3.75 -3.175) (layer F.SilkS) (width 0.15))
  (fp_line (start -4 0.325) (end -4 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -4 0.825) (end -3.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 0.825) (end -3.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 0.325) (end -4 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 0.325) (end -2.75 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 0.825) (end -2.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 0.825) (end -2.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 0.325) (end -2.75 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 0.325) (end -1.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 0.825) (end -1 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.825) (end -1 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.325) (end -1.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0.325) (end -0.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0.825) (end 0.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 0.825) (end 0.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 0.325) (end -0.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.325) (end 1 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.825) (end 1.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 0.825) (end 1.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 0.325) (end 1 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.25 0.325) (end 2.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.25 0.825) (end 2.75 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.75 0.825) (end 2.75 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.75 0.325) (end 2.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.5 0.325) (end 3.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.5 0.825) (end 4 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 4 0.825) (end 4 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 4 0.325) (end 3.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.5 -3.05) (end -6.5 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.5 3.6) (end 6.5 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.5 3.6) (end 6.5 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.5 -3.05) (end -6.5 -3.05) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -3.75 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.5 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.25 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 1.25 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 2.5 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 3.75 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 5.5 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.1))
  (pad 8 smd roundrect (at -5.5 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.1))
  (model Connector_JST.3dshapes/JST_GH_BM07B-GHS-TBT.wrl
    (at (xyz -0.2362204724409449 -0.09448818897637795 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz -90 0 180))
  )
)
