(footprint "LiteOn_LTST-S220KSKT" (version 20211232) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F947A8)
  (attr smd)
  (fp_text reference "REF**" (at 0 -15.47 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 41ef6d8e-078c-46e5-a743-15f86f94b1c5)
  )
  (fp_text value "LiteOn_LTST-S220KSKT" (at 0 -13.97 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 217a6ab0-8c75-4e09-8113-c7b7b906da43)
  )
  (fp_text user "${REFERENCE}" (at 0 -12.47 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 57881c8f-ea31-4450-bce6-89885e0a9bfd)
  )
  (fp_line (start -1.075 -0.25) (end -1.075 0.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7e56433f-8047-4182-a23d-dde6a3760eda))
  (fp_line (start -1.075 0.25) (end 1.075 0.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 9caa825e-43a9-45d3-8dad-ce1e46623c13))
  (fp_line (start -0.35 -0.75) (end 0.35 -0.75)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a1ebb81a-5a70-4ccb-880e-6fe3a3cd95db))
  (fp_line (start 1.075 -0.25) (end -1.075 -0.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c3d355e2-5a2e-4900-90d5-2140e7b8830b))
  (fp_line (start 1.075 0.25) (end 1.075 -0.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 4da6302c-cd1f-4909-89d2-621a3bbeb204))
  (fp_arc (start -0.85 -0.25) (mid -0.703553 -0.603553) (end -0.35 -0.75)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 66cf9899-100d-45fb-9b9f-8f866de8a3fe))
  (fp_arc (start 0.35 -0.75) (mid 0.703553 -0.603553) (end 0.85 -0.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 04748a16-5476-4809-b159-9184ff58426c))
  (pad "1" smd roundrect (at -1.25 0) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp b656459b-45a8-4466-bf55-064e0e9bbeb4))
  (pad "2" smd roundrect (at 1.25 0) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp a5acfc13-660b-4475-8069-b28733a7b5eb))
)
