(footprint "SMD Nut M2 x 5.0 SMTSO2050" (version 20221018) (generator pcbnew)
  locked (layer "F.Cu")
  (property "LCSC" "C2916350")
  (property "MFG" "Sinhoo")
  (property "MPN" "SMTSO2050CTJ")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "exclude_from_bom" "")
  (attr smd exclude_from_bom)
  (fp_text reference "H9" (at 0 -7.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 19d00d09-5bf6-46ac-b6af-e3cca5efda03)
  )
  (fp_text value "MOUNT_HOLE" (at 0 -6 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4847dc54-f4b3-415b-979c-47b40a92cf86)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b97589b6-5690-4e76-a14e-e2914791ade7)
  )
  (fp_arc (start -2.533845 0.788749) (mid -2.65374 -0.012456) (end -2.526329 -0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 4292df80-f403-4045-8c3d-00545bde300c))
  (fp_arc (start -1.95 -1.8) (mid -1.316084 -2.304435) (end -0.559519 -2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 71b8de4e-e2c3-4922-92e6-3eb5ae5236c8))
  (fp_arc (start -0.583845 2.588749) (mid -1.337657 2.291979) (end -1.96681 1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp c3d75b4f-ff38-4e54-ba81-a37e57acfda2))
  (fp_arc (start 0.583845 -2.588749) (mid 1.337657 -2.291979) (end 1.96681 -1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp e42c4a65-e46c-448b-8023-b8608a885f7c))
  (fp_arc (start 1.95 1.8) (mid 1.316084 2.304435) (end 0.559519 2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp f4978d4c-0e7c-4a70-9aa4-7f6072e29b0e))
  (fp_arc (start 2.533845 -0.788749) (mid 2.65374 0.012456) (end 2.526329 0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 1263ae42-af2a-41eb-8c42-e814b1434615))
  (fp_circle (center 0 0) (end 2.15 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp ac393253-829d-45c7-90ee-0148cf36f48b))
  (fp_circle (center 0 0) (end 3.25 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 3400a559-7115-4605-a66a-55d58e9fc7e4))
  (pad "1" thru_hole circle locked (at 0 0) (size 4.03 4.03) (drill 3.73) (layers "*.Cu" "B.Mask")
    (zone_connect 2) (tstamp ca411963-9b33-42ca-a7e7-1a07824f7661))
  (pad "1" smd circle locked (at 0 0) (size 6.2 6.2) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp f2f92956-c513-415a-b1ea-16392e81c97e))
  (model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/Nut [SMTSO] [M2 x 5].step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
