(footprint "JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST GH series connector, SM04B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST GH top entry")
  (property "LCSC" "C189895")
  (property "MFG" "JST")
  (property "MPN" "SM04B-GHS-TB(LF)(SN)")
  (property "Sheetfile" "CAN_Node.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J2" (at 0 -3.3) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 1fb31312-5838-4092-af80-c03db35e58c7)
  )
  (fp_text value "CAN_OUT" (at 0 3.3) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 523a934e-7db9-46e2-8474-a5443de86168)
  )
  (fp_text user "${REFERENCE}" (at 0 2.1) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp c08f4ef2-451b-4c4a-9bd6-1bf264999890)
  )
  (fp_line (start -4.235 -1.71) (end -2.435 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94787fd9-3fe3-4102-9c05-61764c0abb9b))
  (fp_line (start -4.235 -0.26) (end -4.235 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d71f1bc7-5242-4184-9468-731d4bc81d55))
  (fp_line (start -2.965 2.56) (end 2.965 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2fe0e5f9-ab1a-41f4-8cc9-458a7a4838ec))
  (fp_line (start -2.435 -1.71) (end -2.435 -2.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b46f0bd9-f059-4156-b68b-e9e0cf75aa14))
  (fp_line (start 4.235 -1.71) (end 2.435 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8218b23e-c848-44e3-a65f-54b3a06fdf3e))
  (fp_line (start 4.235 -0.26) (end 4.235 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af9962d3-8c45-4f7b-8cc8-23190f660f41))
  (fp_line (start -4.4 2.45) (end -4.4 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 979c28ae-007f-428b-af15-ba471a21a175))
  (fp_line (start -4 2.85) (end 4 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9657d795-7487-41fc-b131-bdd98f7f305f))
  (fp_line (start -2.35 -2.55) (end -2.35 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3054d509-1d42-4342-bb30-1c3a5a0e845f))
  (fp_line (start -2.35 -1.85) (end -4.15 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ebe9cd7d-3c1c-4539-b2b9-84d5157752b1))
  (fp_line (start 2.05 -2.85) (end -2.05 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5c43f3f8-c290-41f2-b1af-be416603fd33))
  (fp_line (start 2.35 -2.55) (end 2.35 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc3de31e-0b54-44b1-a245-e709343d32e1))
  (fp_line (start 2.35 -1.85) (end 4.15 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0dd6ca54-df43-45dc-916a-62f93cc4c893))
  (fp_line (start 4.4 2.45) (end 4.4 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cdd47190-b60b-4737-8238-4df169dd3bbe))
  (fp_arc (start -4.4 -1.6) (mid -4.326777 -1.776777) (end -4.15 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fbdf508a-f2f7-48c5-b51a-d51bfe906286))
  (fp_arc (start -4 2.85) (mid -4.282843 2.732843) (end -4.4 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc4475ec-7497-446d-b052-9d577074164d))
  (fp_arc (start -2.35 -2.55) (mid -2.262132 -2.762132) (end -2.05 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 583786d7-9cd7-4d87-8b6d-9135bf30be0b))
  (fp_arc (start 2.05 -2.85) (mid 2.262132 -2.762132) (end 2.35 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bbf2d701-7f15-4428-af6e-b01b14db8d16))
  (fp_arc (start 4.15 -1.85) (mid 4.326777 -1.776777) (end 4.4 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0c629162-ba92-41a2-88aa-eb99c2ae8c10))
  (fp_arc (start 4.4 2.45) (mid 4.282843 2.732843) (end 4 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 30d69596-e6fa-45ab-8507-9728de0946e1))
  (fp_line (start -4.125 -1.6) (end -4.125 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cceea49d-bbe3-4ee3-8304-2b2668d030d5))
  (fp_line (start -4.125 -1.6) (end 4.125 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2354d18f-d6f1-4661-bbea-bf3501d1d01d))
  (fp_line (start -4.125 2.45) (end 4.125 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa3db086-657d-45d0-979f-c02c64485dd1))
  (fp_line (start -2.375 -1.6) (end -1.875 -0.892893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8d1a37b-e01e-4304-90f8-95140e3d6a30))
  (fp_line (start -1.875 -0.892893) (end -1.375 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ddba84d-8334-4381-8efc-9feedc098449))
  (fp_line (start 4.125 -1.6) (end 4.125 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7dccf4d0-20e9-4237-a1ec-ba02fe6486c2))
  (pad "1" smd roundrect (at -1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31ee9534-622a-4e50-8979-1e4e815dff1d))
  (pad "2" smd roundrect (at -0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bf973e43-8799-4473-ae51-48961371abba))
  (pad "3" smd roundrect (at 0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3d686282-dbf7-4c77-a3f9-526083106192))
  (pad "4" smd roundrect (at 1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 198c2d61-bb5e-48be-86f7-ab031047cbdf))
  (pad "MP" smd roundrect (at -3.725 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f9bafd05-5b2c-4b96-91e2-d770611f2872))
  (pad "MP" smd roundrect (at 3.725 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 48f0861a-eec6-473b-a422-7679356adf31))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
