(footprint "X9357WR-2x01-N2SN" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 16.2 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d337872-662f-436e-aefd-e52ec318dd7b)
  )
  (fp_text value "X9357WR-2x01-N2SN" (at 0 -2.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3b19bccd-450b-4cf1-a6b6-eed0c35448ab)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.2 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7f0cfc72-036d-4a68-ac08-212cc05a968a)
  )
  (fp_rect (start -2.95 0.3) (end -2.8 1.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d3b27236-9b07-427a-bcd8-1e544f140803))
  (fp_rect (start 2.8 0.3) (end 2.95 1.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 32069d04-9116-46f9-bdb9-f893a59e6fb3))
  (fp_arc (start -2.8 12.875) (mid -2.853033 12.853033) (end -2.875 12.8)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 2cc3582a-5612-4933-a6e4-9ab946af39ab))
  (fp_arc (start 2.875 12.8) (mid 2.853033 12.853033) (end 2.8 12.875)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 2341dcd1-6778-4ae0-8a89-eb14807fe830))
  (fp_poly
    (pts
      (xy -2.8 11.8)
      (xy -2.8 12.8)
      (xy -1.8 12.8)
      (xy -1.8 12.95)
      (xy -2.8 12.95)
      (xy -2.95 12.8)
      (xy -2.95 11.8)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5b53ca18-bb03-476d-ab35-75aef3a88d3f))
  (fp_poly
    (pts
      (xy 1.8 12.8)
      (xy 2.8 12.8)
      (xy 2.8 11.8)
      (xy 2.95 11.8)
      (xy 2.95 12.8)
      (xy 2.8 12.95)
      (xy 1.8 12.95)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 24fe938d-1bf9-4d62-b197-dedd5df01eed))
  (fp_rect (start -2.8 0) (end 2.8 12.8)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp b48dcc7e-e54a-4295-9550-13d15c2a630f))
  (pad "1" thru_hole circle (at 0 13.9) (size 2.1 2.1) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp 54174217-f418-44b2-b6fb-f0532749ee32))
  (pad "1" smd roundrect (at 0 13.9) (size 2.6 2.6) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.09615384615) (tstamp 1911c5e0-3d8f-4bd1-97e4-07828a2f64b1))
  (pad "2" thru_hole circle (at 0 19.4) (size 2.1 2.1) (drill 1.8) (layers "*.Cu" "*.Mask") (tstamp a5bfc043-e1f4-4080-ad9a-71440c2f6a4e))
  (pad "2" smd roundrect (at 0 19.4) (size 2.6 2.6) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.1470588235) (tstamp 4c56fb59-7043-4409-89e0-7819f0af7f23))
  (model ":KICAD7_3DMODEL_DIR:Connector_XKB.3dshapes/X9357WR-2X01S-XXSN.stp"
    (offset (xyz 0 0 9.93))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
