(module ST_AIS3624DQ_QFN-24 (layer F.Cu) (tedit 57514B39)
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.03)
  (fp_text reference U9 (at 0 -3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value ST_AIS3624DQTR (at 0 3) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.1)))
  )
  (fp_line (start 2 -2) (end 2 2) (layer F.Fab) (width 0.05))
  (fp_line (start 2 2) (end -2 2) (layer F.Fab) (width 0.05))
  (fp_line (start -2 2) (end -2 -2) (layer F.Fab) (width 0.05))
  (fp_line (start -2 -2) (end 2 -2) (layer F.Fab) (width 0.05))
  (fp_text user "IC AREA" (at 0 1) (layer Cmts.User)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_text user "POUR UNDER" (at 0 0) (layer Cmts.User)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_text user "NO COPPER" (at 0 -1) (layer Cmts.User)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_circle (center -2.15 2.45) (end -2.2 2.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 1.7) (end -2.2 2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.2 2.2) (end -1.7 2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.2 1.7) (end 2.2 2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.2 2.2) (end 1.7 2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.7 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.2 -2.2) (end 2.2 -1.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.2 -1.7) (end -2.2 -2.2) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.2 -2.2) (end -1.7 -2.2) (layer F.SilkS) (width 0.127))
  (pad 1 smd oval (at -1.25 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -0.75 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -0.25 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at 0.25 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 2 1.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 2 0.75 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 2 0.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 2 -0.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 0.25 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at -0.25 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at -0.75 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at -1.25 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at -2 -1.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at -2 -0.75 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at -2 -0.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at -2 0.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0 0) (size 2.7 2.7) (layers F.Mask))
  (pad 14 smd oval (at 0.75 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 1.25 -2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 2 -0.75 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 2 -1.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at -2 0.75 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at -2 1.25 90) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at 0.75 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 1.25 2) (size 0.28 0.99) (layers F.Cu F.Paste F.Mask))
  (model Sensor_Motion.3dshapes/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
