(module TI_TPS63025x_VQFN-14 (layer F.Cu) (tedit 574AF6A6)
  (solder_mask_margin 0.04)
  (solder_paste_margin -0.01)
  (attr smd)
  (fp_text reference REF** (at 0 -2.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value TI_TPS63025x_VQFN-14 (at 0 2.3) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.1)))
  )
  (fp_circle (center -1.7 -1.7) (end -1.7 -1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 1.75) (end -1.5 1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.5 1.75) (end -1.5 1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.5 1.25) (end 1.5 1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.5 1.75) (end 1 1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 -1.75) (end 1.5 -1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.5 -1.75) (end 1.5 -1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.5 -1.75) (end -1 -1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.5 -1.75) (end -1.5 -1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.75 -2) (end 1.75 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -2) (end 1.75 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 2) (end -1.75 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 2) (end -1.75 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 -1.5) (end 1.25 1.5) (layer F.Fab) (width 0.05))
  (fp_line (start 1.25 1.5) (end -1.25 1.5) (layer F.Fab) (width 0.05))
  (fp_line (start -1.25 1.5) (end -1.25 -1.5) (layer F.Fab) (width 0.05))
  (fp_line (start -1.25 -1.5) (end 1.25 -1.5) (layer F.Fab) (width 0.05))
  (pad 4 smd oval (at -0.75 1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -0.25 1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 0.25 1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 0.75 1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 0.75 -1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 0.25 -1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at -0.25 -1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at -0.75 -1.4) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 1.15 0.5 90) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 1.15 0 90) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 1.15 -0.5 90) (size 0.24 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.555 -0.49) (size 1.89 0.32) (layers F.Cu F.Mask)
    (solder_mask_margin -0.05))
  (pad 2 smd rect (at -0.555 0) (size 1.89 0.34) (layers F.Cu F.Mask)
    (solder_mask_margin -0.05))
  (pad 3 smd rect (at -0.555 0.49) (size 1.89 0.32) (layers F.Cu F.Mask)
    (solder_mask_margin -0.05))
  (pad 2 smd rect (at -1.05 0) (size 0.8 0.24) (layers F.Cu F.Paste))
  (pad 2 smd rect (at -0.05 0) (size 0.8 0.24) (layers F.Cu F.Paste))
  (pad 1 smd rect (at -1.05 -0.49) (size 0.8 0.24) (layers F.Cu F.Paste))
  (pad 3 smd rect (at -1.05 0.49) (size 0.8 0.24) (layers F.Cu F.Paste))
  (pad 1 smd rect (at -0.05 -0.49) (size 0.8 0.24) (layers F.Cu F.Paste))
  (pad 3 smd rect (at -0.05 0.49) (size 0.8 0.24) (layers F.Cu F.Paste))
)
