(module Omron_G5LE-1 (layer F.Cu) (tedit 594B603D)
  (fp_text reference K2 (at -11.9 0 -270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "TE ORWH-SH-105D1F,000" (at 10.5 0 -270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.5 8.5) (end 9.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 10.5 8.5) (end 9.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 8.5) (end 10.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 6.5) (end 11.5 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 7.5) (end 11.5 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 8.5) (end 11.5 7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 9.5 -8.5) (end 9.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 10.5 -8.5) (end 9.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 -8.5) (end 10.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 -6.5) (end 11.5 -6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 -7.5) (end 11.5 -6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.5 -8.5) (end 11.5 -7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -9.5 8.5) (end -9.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -10.5 8.5) (end -9.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 8.5) (end -10.5 8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 6.5) (end -11.5 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 7.5) (end -11.5 6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 8.5) (end -11.5 7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 -6.5) (end -11.5 -6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 -7.5) (end -11.5 -6.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 -8.5) (end -11.5 -7.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -9.5 -8.5) (end -9.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -10.5 -8.5) (end -9.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.5 -8.5) (end -10.5 -8.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.25 8.25) (end -11.25 -8.25) (layer F.Fab) (width 0.05))
  (fp_line (start 11.25 8.25) (end -11.25 8.25) (layer F.Fab) (width 0.05))
  (fp_line (start 11.25 -8.25) (end 11.25 8.25) (layer F.Fab) (width 0.05))
  (fp_line (start -11.25 -8.25) (end 11.25 -8.25) (layer F.Fab) (width 0.05))
  (pad 4 thru_hole circle (at 5.5 -6) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5.5 6) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -6.7 -6) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -6.7 6) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -8.7 0) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 connect roundrect (at -8.7 0) (size 2.5 2.5) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 connect roundrect (at 5.5 6) (size 2.5 2.5) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 4 connect roundrect (at 5.5 -6) (size 2.5 2.5) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 5 connect circle (at -6.7 -6) (size 2.3 2.3) (layers B.Cu B.Mask))
  (pad 2 connect circle (at -6.7 6) (size 2.3 2.3) (layers B.Cu B.Mask))
  (model Relay_THT.3dshapes/Omron_G5LE-1.step
    (at (xyz -0.344488188976378 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
