(footprint "HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm_ThermalVias" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "HSOP SO")
  (property "LCSC" "C477928")
  (property "MFG" "TI")
  (property "MPN" "LM5164DDAR")
  (property "Sheetfile" "ShuntModule.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "1A synchronous buck converter with ultra-low IQ, 6V - 100V input, adjustable output voltage, HSOP-8")
  (property "ki_keywords" "step-down dc-dc buck regulator adjustable")
  (attr smd)
  (fp_text reference "U4" (at 0 -3.4) (layer "F.SilkS") hide
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 0ceeb32c-8677-42e8-bf54-92c29a77ec8c)
  )
  (fp_text value "LM5164DDA" (at 0 2.15) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.15)))
    (tstamp 04fad1ef-b664-47ab-9852-7c2f8f24c58a)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.95) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 17d53087-51db-419b-a122-e3de9d495b7c)
  )
  (fp_line (start 0 -2.56) (end -3.45 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aee48b79-773f-4947-873e-fd4280715037))
  (fp_line (start 0 -2.56) (end 1.95 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 36e85dad-d006-4f98-b85e-3aef4c9fe596))
  (fp_line (start 0 2.56) (end -1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6a72f763-6a52-44ea-8165-b1361a9dbeb8))
  (fp_line (start 0 2.56) (end 1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5985ea6-ffeb-4e8d-b43f-ba5ec3c746ac))
  (fp_line (start -3.6 -2.05) (end -3.6 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3afab0bf-f692-4b70-aa82-361fdb63bd70))
  (fp_line (start -3.3 -2.35) (end -2.2 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1933ae40-bff4-4713-bec0-02c7f53be756))
  (fp_line (start -3.3 2.35) (end -2.2 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fa89c5b1-48db-4078-8ca9-dc015d1ba669))
  (fp_line (start -2.2 -2.35) (end -2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 64e982f5-309d-411f-bac1-61f09911a0a9))
  (fp_line (start -2.2 2.35) (end -2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 89894d1a-3a46-44fa-96ef-a9f97c5fb097))
  (fp_line (start -1.95 -2.7) (end 1.95 -2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 679431bb-1e81-4e8e-98ef-fd743fae5e7b))
  (fp_line (start -1.95 2.7) (end 1.95 2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9f1735d2-4d9d-4e81-9a49-c0035edda3be))
  (fp_line (start 2.2 -2.35) (end 2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b5251ff-a65f-4ed9-94ff-8368351f8251))
  (fp_line (start 2.2 2.35) (end 2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b442f09e-e87b-41f8-abc9-4efdb0da49fc))
  (fp_line (start 3.3 -2.35) (end 2.2 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dcca0535-a498-454f-9159-8d1eb3ffd788))
  (fp_line (start 3.3 2.35) (end 2.2 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c91d42b7-056b-42bb-b925-398d495c2bea))
  (fp_line (start 3.6 -2.05) (end 3.6 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8b3623f6-2de0-4f78-a5e7-d8b213512b9b))
  (fp_arc (start -3.6 -2.05) (mid -3.512132 -2.262132) (end -3.3 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 57e0c25d-eb5e-4dda-a0ac-adeac9f7f2e6))
  (fp_arc (start -3.3 2.35) (mid -3.512132 2.262132) (end -3.6 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 014d467e-ae62-49a9-af64-a82e4a41dc7c))
  (fp_arc (start -2.2 -2.45) (mid -2.126777 -2.626777) (end -1.95 -2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dee1313a-78b5-4792-b086-808101688ff8))
  (fp_arc (start -1.95 2.7) (mid -2.126777 2.626777) (end -2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 20757801-f78d-4188-a9ed-ce835ac336a8))
  (fp_arc (start 1.95 -2.7) (mid 2.126777 -2.626777) (end 2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ad18c7de-95bc-4a74-b3fd-660b69ac71c2))
  (fp_arc (start 2.2 2.45) (mid 2.126777 2.626777) (end 1.95 2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 54ef82bd-2ab8-4548-a36d-5e563d46c41d))
  (fp_arc (start 3.3 -2.35) (mid 3.512132 -2.262132) (end 3.6 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e7485112-daac-4d34-8374-3e6651c2a9e4))
  (fp_arc (start 3.6 2.05) (mid 3.512132 2.262132) (end 3.3 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8ceab745-5271-442f-80c5-840d969aaa34))
  (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1070937a-fe59-491d-90ae-e3a295f2211a))
  (fp_line (start -1.95 2.45) (end -1.95 -1.475)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca2ce64b-f3d7-465b-8490-3391f1545645))
  (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7e293da5-9265-48f0-a4c7-6c498cb2d069))
  (fp_line (start 1.95 -2.45) (end 1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 635a02bd-3554-49e9-81c7-29909f9a6d0d))
  (fp_line (start 1.95 2.45) (end -1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 08ec0d65-d525-40d8-8474-aca1bf75bfe6))
  (pad "" smd oval (at -2.65 -1.905) (size 1.2 0.5) (layers "F.Paste") (tstamp 3516ba88-1175-4a61-b234-d1cafab2fb10))
  (pad "" smd oval (at -2.65 -0.635) (size 1.2 0.5) (layers "F.Paste") (tstamp ba0d7cc9-3344-40d3-92e2-6920ae8e55ff))
  (pad "" smd oval (at -2.65 0.635) (size 1.2 0.5) (layers "F.Paste") (tstamp 8c0d803b-bfb4-4e08-9789-d632bf700087))
  (pad "" smd oval (at -2.65 1.905) (size 1.2 0.5) (layers "F.Paste") (tstamp 3dfc3c74-1e46-4a20-9eb0-693d8ab6fca9))
  (pad "" smd roundrect (at -0.65 -0.675) (size 1.1 1.05) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp c65dae15-07ae-4ebf-bb03-7ef08e578e78))
  (pad "" smd roundrect (at -0.65 0.675) (size 1.1 1.05) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp c81f90e8-7371-469a-8688-2867dda8a356))
  (pad "" smd roundrect (at 0.65 -0.675) (size 1.1 1.05) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 7b95fe85-cb47-43eb-bbfa-bb5a42708206))
  (pad "" smd roundrect (at 0.65 0.675) (size 1.1 1.05) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 81a07de6-21a8-49d4-a24e-a311808fd077))
  (pad "" smd oval (at 2.65 -1.9) (size 1.2 0.5) (layers "F.Paste") (tstamp dcbfa033-db2d-4bda-a995-bc2b315ac34d))
  (pad "" smd oval (at 2.65 -0.63) (size 1.2 0.5) (layers "F.Paste") (tstamp e680897e-f98c-4489-8d70-496f7b333022))
  (pad "" smd oval (at 2.65 0.64) (size 1.2 0.5) (layers "F.Paste") (tstamp d78a0088-7d19-406c-99a1-47ba91e1da70))
  (pad "" smd oval (at 2.65 1.91) (size 1.2 0.5) (layers "F.Paste") (tstamp e90a2895-ebee-4d94-844b-7da74b123021))
  (pad "1" smd roundrect (at -2.65 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 621f0641-5c7c-4121-8e7b-37d60d449e7a))
  (pad "2" smd roundrect (at -2.65 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp b8c6173a-0b42-4413-8829-e2420f149aa1))
  (pad "3" smd roundrect (at -2.65 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 3185590b-ed0c-42c7-afdf-308979720f87))
  (pad "4" smd roundrect (at -2.65 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e1608a1-6e33-4d1a-9965-de0f62be40dd))
  (pad "5" smd roundrect (at 2.65 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp d461d927-e1d6-4684-a1b0-3fa00792b830))
  (pad "6" smd roundrect (at 2.65 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp c2a574f9-42dc-4901-95f4-5a5dcc0d3813))
  (pad "7" smd roundrect (at 2.65 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 159b3c52-981b-4e69-8c51-1b2831cd8b24))
  (pad "8" smd roundrect (at 2.65 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 260c5921-5ccb-40a7-9c9a-79b63a298491))
  (pad "9" thru_hole circle (at -0.975 -1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp a2cecea2-002f-4db6-a5f9-7303139c59dd))
  (pad "9" thru_hole circle (at -0.975 0) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp cdae00ed-aaee-4420-b06f-2a404b9efbb1))
  (pad "9" thru_hole circle (at -0.975 1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp f8e3eab7-537b-474e-b92f-c6645c391cc5))
  (pad "9" thru_hole circle (at 0 -1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp bfdda6a6-5c8c-48c6-83c4-705b3b9078e3))
  (pad "9" thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp 672330a7-2c3c-462e-922a-0a5b3a4c4eb4))
  (pad "9" smd roundrect (at 0 0) (size 2.41 3.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.04149377593) (tstamp 768d23f4-e2fb-4001-858b-8c77d355d203))
  (pad "9" smd roundrect (at 0 0) (size 2.41 3.1) (layers "B.Cu") (roundrect_rratio 0.08298755187) (tstamp 4e790aae-17df-49fa-bfab-6ca3834bdf33))
  (pad "9" thru_hole circle (at 0 1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp 39346a74-fed3-46b8-a170-24db1443c997))
  (pad "9" thru_hole circle (at 0.975 -1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp e16c9e26-3e00-4ed8-96d8-051a94a26692))
  (pad "9" thru_hole circle (at 0.975 0) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp d2137d86-5815-4c79-b7a0-cbe41c5f8d74))
  (pad "9" thru_hole circle (at 0.975 1.325) (size 0.45 0.45) (drill 0.3) (layers "*.Cu") (tstamp 4405d98f-d52a-456a-84ef-7ee864444948))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
