(footprint "RJ45_Amphenol_RJHSE5380" (version 20220621) (generator pcbnew)
  (layer "F.Cu")
  (descr "Shielded, https://www.amphenolcanada.com/ProductSearch/drawings/AC/RJHSE538X.pdf")
  (tags "RJ45 8p8c ethernet cat5")
  (property "Sheetfile" "File: Teensy41Carrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61")
  (property "ki_keywords" "8P8C RJ female connector")
  (attr through_hole)
  (fp_text reference "J4" (at 3.56 -9.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4d1778cd-a45b-4399-b09a-ced46df34257)
  )
  (fp_text value "8P8C" (at 3.56 9.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aacf7d67-88b2-418c-9b87-9af6ad32060a)
  )
  (fp_text user "${REFERENCE}" (at 3.56 -6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp beca5595-642e-48fe-b8ba-c8f3fca8996c)
  )
  (fp_line (start -5.5 -1.2) (end -5 -0.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 36be4124-4cb2-4ea6-8141-ea4e9618271d))
  (fp_line (start -5.5 -0.2) (end -5.5 -1.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f2e5071-be17-43be-9ab4-0f2a189e0ea5))
  (fp_line (start -5 -0.7) (end -5.5 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b96e5fe3-af0e-40b1-8d81-d29da6abe15b))
  (fp_line (start -4.805 -8.11) (end -4.805 -0.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8126e4db-8ef9-4674-8e66-2105082277d0))
  (fp_line (start -4.805 7.86) (end -4.805 2.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ef32b19-ef77-4ce2-93d0-d11f4bf55d8e))
  (fp_line (start -4.76 -8.11) (end 11.88 -8.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c54c51c-00b0-438f-b790-8def6cd3d217))
  (fp_line (start -4.76 7.86) (end 11.925 7.86)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6d83252-f578-40a2-8e3e-9110b87b8633))
  (fp_line (start 11.925 -8.11) (end 11.925 -0.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a719042a-e097-4821-bdcb-a5fe0f09f017))
  (fp_line (start 11.925 7.86) (end 11.925 2.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e08e5eb5-ac5c-4539-9d68-0e9a99f811d3))
  (fp_line (start -6.22 -8.5) (end -6.22 8.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8d250c51-1312-4960-8e48-ba93e552939d))
  (fp_line (start -6.22 -8.5) (end 13.34 -8.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 59fcfa34-b302-4d1b-8339-3b7e01b86e9c))
  (fp_line (start -6.22 8.25) (end 13.34 8.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa3b7560-6dfb-4167-ab31-8e5a78d730fd))
  (fp_line (start 13.34 -8.5) (end 13.34 8.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ef69ba88-f819-49bf-a7b8-5a51b3f52ed1))
  (fp_line (start -4.695 -7) (end -4.695 7.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c80adc90-af68-4057-9907-1d72003ce539))
  (fp_line (start -4.695 -7) (end -3.695 -8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffec8686-c7a4-476e-b456-c62985b7f771))
  (fp_line (start -4.695 7.75) (end 11.815 7.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 11fc0963-60f0-4470-b0ed-2dcfba8b37ba))
  (fp_line (start -3.695 -8) (end 11.815 -8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c6e0bbea-71c2-4d9c-b3e9-dca1e5c26a9e))
  (fp_line (start 11.815 -8) (end 11.815 7.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 750be042-6aa0-43e6-83af-73c475cac999))
  (pad "" np_thru_hole circle (at -2.79 -2.54) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask) (tstamp af53bfea-8136-4f1e-bd9e-f81318ff2514))
  (pad "" np_thru_hole circle (at 9.91 -2.54) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask) (tstamp 9073139d-7f02-456e-9519-cb675d128e66))
  (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp fe5bdfe0-1061-43db-91d5-8277a65194b0))
  (pad "2" thru_hole circle (at 1.016 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 672c8125-fb08-4f7e-b8cf-0ee40e16c073))
  (pad "3" thru_hole circle (at 2.032 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 44e1a5d0-551b-4518-9bbd-de903326ddf0))
  (pad "4" thru_hole circle (at 3.048 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 988c9e00-1108-4908-800a-d7cafb8215d5))
  (pad "5" thru_hole circle (at 4.064 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 12ac5de3-4bdc-4d4e-a65a-243a52350a07))
  (pad "6" thru_hole circle (at 5.08 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp c17c942c-e7df-4ac2-b213-8574c6e16a63))
  (pad "7" thru_hole circle (at 6.096 0) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 0e4cb07f-1719-4ca8-9db6-2989f90efb60))
  (pad "8" thru_hole circle (at 7.112 1.78) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask) (tstamp 4a23022d-7661-4942-8c07-1e6dfe694539))
  (pad "SH" thru_hole circle (at -4.57 0.89) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask) (tstamp 7bd6a068-61b5-4b4f-bec9-69541e18e1e3))
  (pad "SH" thru_hole circle (at 11.69 0.89) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask) (tstamp 9dcac5fb-5f02-44ab-ac72-c1c565c69dfb))
  (model "${KICAD7_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Amphenol_RJHSE5380.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_RJ.3dshapes/M-RJHSE-X380-REVT1.STEP"
    (offset (xyz 3.5 1.55 3.05))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
