(module 2x9_1.5mm (layer F.Cu) (tedit 57546431)
  (solder_mask_margin -0.02)
  (attr virtual)
  (fp_text reference P4 (at 0 -7.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value PROGRAM (at 2 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -1.75 -7) (end 1.75 -7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -7) (end 1.75 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 7) (end -1.75 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 7) (end -1.75 -7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -6.75) (end 1.5 -6.75) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 -6.75) (end 1.5 6.75) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 6.75) (end -1.5 6.75) (layer F.Fab) (width 0.05))
  (fp_line (start -1.5 6.75) (end -1.5 -6.75) (layer F.Fab) (width 0.05))
  (fp_text user 1 (at -2 -6) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 connect roundrect (at -0.75 -6) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 2 connect roundrect (at 0.75 -6) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 3 connect roundrect (at -0.75 -4.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 4 connect roundrect (at 0.75 -4.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 5 connect roundrect (at -0.75 -3) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 6 connect roundrect (at 0.75 -3) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 7 connect roundrect (at -0.75 -1.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 8 connect roundrect (at 0.75 -1.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 9 connect roundrect (at -0.75 0) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 10 connect roundrect (at 0.75 0) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 11 connect roundrect (at -0.75 1.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 12 connect roundrect (at 0.75 1.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 13 connect roundrect (at -0.75 3) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 14 connect roundrect (at 0.75 3) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 15 connect roundrect (at -0.75 4.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 16 connect roundrect (at 0.75 4.5) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 17 connect roundrect (at -0.75 6) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 18 connect roundrect (at 0.75 6) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
)
